(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 48)
    (no_connects 0)
    (area 52.019999 50.749999 77.520001 76.250001)
    (thickness 1.6)
    (drawings 57)
    (tracks 256)
    (zones 0)
    (modules 15)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /Vin)
  (net 2 GND)
  (net 3 3v3)
  (net 4 /RST)
  (net 5 /GPIO16)
  (net 6 /GPIO13)
  (net 7 /GPIO12)
  (net 8 /GPIO14)
  (net 9 /CH_PD)
  (net 10 /ADC)
  (net 11 /SCL)
  (net 12 /SDA)
  (net 13 /TX)
  (net 14 /RX)
  (net 15 /GPIO0)
  (net 16 /GPIO2)
  (net 17 /GPIO15)
  (net 18 "Net-(U1-Pad17)")
  (net 19 "Net-(U1-Pad18)")
  (net 20 "Net-(U1-Pad19)")
  (net 21 "Net-(U1-Pad20)")
  (net 22 "Net-(U1-Pad21)")
  (net 23 "Net-(U1-Pad22)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
  )
  (net_class gnd ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.762)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Vin)
    (add_net 3v3)
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ADC)
    (add_net /CH_PD)
    (add_net /GPIO0)
    (add_net /GPIO12)
    (add_net /GPIO13)
    (add_net /GPIO14)
    (add_net /GPIO15)
    (add_net /GPIO16)
    (add_net /GPIO2)
    (add_net /RST)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58F20968)
    (at 71.12 67.31 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 1u1 (at 3.175 0 360) (layer B.SilkS))
    (fp_text value C (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 3.175 0 540) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /Vin))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58F20954)
    (at 63.5 67.31 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 1u2 (at 3.175 -0.127 540) (layer B.SilkS))
    (fp_text value C (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 3.175 -0.127 360) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58F203E3)
    (at 57.785 70.485 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 1u3 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value C (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.651 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58F1ECFC)
    (at 53.34 73.66 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Vin))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ESP_brd:Pin_Header_Angled_1x02_Pitch2.54mm (layer B.Cu) (tedit 58F2098F)
    (at 58.42 57.15 270)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference P2 (at 4.315 2.27 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X02 (at 4.315 -4.81 270) (layer B.Fab) hide)
    (fp_text user %R (at 4.315 2.27 270) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 2.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /RST))
    (pad 2 smd rect (at 0 -2.54 270) (size 2.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /GPIO16))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58F1ED05)
    (at 53.34 71.12 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 20.11 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Vin))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIO13))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIO12))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO14))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIO16))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /CH_PD))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ADC))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58F1ED36)
    (at 60.96 73.66 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 3v3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58F1ED0D)
    (at 76.2 53.34)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P5 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 20.11) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /TX))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /RX))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCL))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SDA))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GPIO0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /GPIO15))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ESP_brd:Pin_Header_Straight_1x06_Pitch2.54mm_SMD (layer B.Cu) (tedit 58F20590)
    (at 58.42 53.34 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P6 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -15.03 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 2.33 270) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 1.7 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 0 -2.54 270) (size 1.7 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -5.08 270) (size 1.7 1.7) (layers B.Cu B.Paste B.Mask)
      (net 14 /RX))
    (pad 4 smd rect (at 0 -7.62 270) (size 1.7 1.7) (layers B.Cu B.Paste B.Mask)
      (net 13 /TX))
    (pad 5 smd rect (at 0 -10.16 270) (size 1.7 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /RST))
    (pad 6 smd rect (at 0 -12.7 270) (size 1.7 1.7) (layers B.Cu B.Paste B.Mask)
      (net 15 /GPIO0))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58F204BB)
    (at 67.31 56.515 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.048 0 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 /CH_PD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58F204C2)
    (at 67.31 58.42)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.048 0.127) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /RST))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58F20400)
    (at 71.755 70.485 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /GPIO15))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58F204C9)
    (at 67.31 60.325)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.048 0.127) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 /GPIO0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP_brd:ESP-12E (layer F.Cu) (tedit 58F208D0)
    (at 57.785 52.07)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 10.795 11.43) (layer F.SilkS))
    (fp_text value ESP-12E (at 6.35 6.35) (layer F.Fab) hide)
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.CrtYd))
    (pad 1 smd rect (at 0 0) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 /RST))
    (pad 2 smd rect (at 0 2) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 /ADC))
    (pad 3 smd rect (at 0 4) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 /CH_PD))
    (pad 4 smd rect (at 0 6) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 /GPIO16))
    (pad 5 smd rect (at 0 8) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 /GPIO14))
    (pad 6 smd rect (at 0 10) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 /GPIO12))
    (pad 7 connect rect (at 0 12) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 6 /GPIO13))
    (pad 8 smd rect (at 0 14) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 3v3))
    (pad 9 smd rect (at 14 14) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 14 12) (size 2.5 1.1) (drill (offset 0.6 0)) (layers F.Cu F.Paste F.Mask)
      (net 17 /GPIO15))
    (pad 11 smd rect (at 14 10) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 16 /GPIO2))
    (pad 12 smd rect (at 14 8) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 15 /GPIO0))
    (pad 13 smd rect (at 14 6) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 /SDA))
    (pad 14 smd rect (at 14 4) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCL))
    (pad 15 smd rect (at 14 2) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 14 /RX))
    (pad 16 smd rect (at 14 0) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 13 /TX))
    (pad 17 smd rect (at 1.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 3.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 5.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 7.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 9.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 11.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad22)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing_Handsoldering (layer B.Cu) (tedit 58F2097D)
    (at 67.31 66.04 90)
    (descr "SOT89-3, Housing, Handsoldering,")
    (tags "SOT89-3 Housing Handsoldering ")
    (attr smd)
    (fp_text reference U2 (at -4.445 0.127 180) (layer B.SilkS))
    (fp_text value HT7333 (at 0.5 -3.15 90) (layer B.Fab) hide)
    (fp_text user %R (at 0.38 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.98 1.5 180) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.98 0 180) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 /Vin))
    (pad 3 smd rect (at -1.98 -1.5 180) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 3v3))
    (pad 2 smd rect (at 1.98 0 180) (size 2 4) (layers B.Cu B.Paste B.Mask)
      (net 1 /Vin))
    (pad 2 smd trapezoid (at -0.37 0) (size 1.5 0.75) (rect_delta 0 -0.5 ) (layers B.Cu B.Paste B.Mask)
      (net 1 /Vin))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing_Handsoldering.wrl
      (at (xyz 0.02 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text RST (at 55.245 53.213 90) (layer B.SilkS))
  (gr_text ADC (at 55.245 55.88 90) (layer B.SilkS))
  (gr_text CH (at 55.245 58.293 90) (layer F.SilkS))
  (gr_text G16 (at 55.245 60.833 90) (layer B.SilkS))
  (gr_text G14 (at 55.245 63.5 90) (layer B.SilkS))
  (gr_text G12 (at 55.245 66.04 90) (layer F.SilkS))
  (gr_text G13 (at 55.245 68.453 90) (layer F.SilkS))
  (gr_text TX (at 74.422 53.213 90) (layer B.SilkS))
  (gr_text RX (at 74.422 55.88 90) (layer B.SilkS))
  (gr_text SCL (at 74.422 58.166 90) (layer B.SilkS))
  (gr_text SDA (at 74.422 60.706 90) (layer B.SilkS))
  (gr_text G0 (at 74.422 63.373 90) (layer B.SilkS))
  (gr_text G2 (at 74.422 65.913 90) (layer B.SilkS))
  (gr_text G15 (at 74.422 68.453 90) (layer B.SilkS))
  (gr_text GND (at 74.549 70.993 90) (layer B.SilkS))
  (gr_text MST (at 73.66 74.676) (layer F.Mask))
  (gr_text "Vin 12V max" (at 58.42 71.628 90) (layer B.SilkS))
  (gr_text "R+C: 0805" (at 58.801 65.659) (layer F.SilkS))
  (gr_text "C: 1uF" (at 58.801 64.389) (layer F.SilkS))
  (gr_text "R2,3: 10K" (at 58.801 63.246) (layer F.SilkS))
  (gr_text "R1,3: 1K" (at 58.801 61.214) (layer F.SilkS))
  (gr_text "HT7333 LDO" (at 58.801 59.944) (layer F.SilkS))
  (gr_text "ESP8266 brd\n04/2017" (at 58.674 52.959) (layer F.SilkS))
  (gr_text WAKEUP (at 59.69 64.135 90) (layer B.SilkS))
  (gr_text 3.3V (at 58.42 55.245) (layer B.SilkS))
  (gr_text GND (at 60.96 55.245) (layer B.SilkS))
  (gr_text RX (at 63.5 55.245) (layer B.SilkS))
  (gr_text TX (at 66.167 55.245) (layer B.SilkS))
  (gr_text RST (at 68.58 55.245) (layer B.SilkS))
  (gr_text G0 (at 71.12 55.245) (layer B.SilkS))
  (gr_text RST (at 55.245 53.213 90) (layer F.SilkS))
  (gr_text ADC (at 55.245 55.88 90) (layer F.SilkS))
  (gr_text CH (at 55.245 58.293 90) (layer B.SilkS))
  (gr_text G16 (at 55.245 60.833 90) (layer F.SilkS))
  (gr_text G14 (at 55.245 63.5 90) (layer F.SilkS))
  (gr_text G12 (at 55.245 66.04 90) (layer B.SilkS))
  (gr_text Vin (at 55.245 71.12 90) (layer B.SilkS))
  (gr_text G13 (at 55.245 68.453 90) (layer B.SilkS))
  (gr_text GND (at 56.007 75.565) (layer F.SilkS))
  (gr_text Vin (at 53.467 75.565) (layer F.SilkS))
  (gr_text Vin (at 55.245 71.12 90) (layer F.SilkS))
  (gr_text 3.3V (at 60.96 71.882) (layer F.SilkS))
  (gr_text GND (at 63.5 71.882) (layer F.SilkS))
  (gr_text SCL (at 65.913 71.882) (layer F.SilkS))
  (gr_text SDA (at 68.58 71.882) (layer F.SilkS))
  (gr_text GND (at 74.549 70.993 90) (layer F.SilkS))
  (gr_text G15 (at 74.422 68.453 90) (layer F.SilkS))
  (gr_text G2 (at 74.422 65.913 90) (layer F.SilkS))
  (gr_text G0 (at 74.422 63.373 90) (layer F.SilkS))
  (gr_text SDA (at 74.422 60.706 90) (layer F.SilkS))
  (gr_text SCL (at 74.422 58.166 90) (layer F.SilkS))
  (gr_text RX (at 74.422 55.88 90) (layer F.SilkS))
  (gr_text TX (at 74.422 53.213 90) (layer F.SilkS))
  (gr_line (start 52.07 76.2) (end 52.07 50.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 77.47 76.2) (end 52.07 76.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 77.47 50.8) (end 77.47 76.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.07 50.8) (end 77.47 50.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.216 75.946) (xy 52.324 75.946) (xy 52.324 51.054) (xy 77.216 51.054)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.216 75.946) (xy 52.324 75.946) (xy 52.324 51.054) (xy 77.216 51.054)
      )
    )
  )
)
