(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 52)
    (zones 0)
    (modules 5)
    (nets 10)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.1524)
    (user_trace_width 0.1778)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (user_trace_width 1.143)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (user_trace_width 1.778)
    (user_trace_width 2.032)
    (user_trace_width 2.286)
    (user_trace_width 2.54)
    (user_trace_width 3.048)
    (trace_clearance 0.1524)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.254)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.635 0.3175)
    (user_via 0.762 0.635)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.3 0.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /RST)
  (net 3 /SWCLK)
  (net 4 /TX)
  (net 5 /RX)
  (net 6 /SWDIO)
  (net 7 /VCC)
  (net 8 /OPT)
  (net 9 /VSENSE)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net /OPT)
    (add_net /RST)
    (add_net /RX)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TX)
    (add_net /VCC)
    (add_net /VSENSE)
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad9)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer Top) (tedit 59FED5CC)
    (at 131.0132 69.1896 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /VSENSE))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /OPT))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /VSENSE))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer Top) (tedit 5A19A420)
    (at 139.192 81.8388 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 5.31) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_1.27mm:PinSocket_2x05_P1.27mm_Vertical (layer Bottom) (tedit 5A19A420)
    (at 142.8496 74.7776 180)
    (descr "Through hole straight socket strip, 2x05, 1.27mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x05 1.27mm double row")
    (fp_text reference J2 (at -0.635 2.135) (layer B.SilkS) hide)
    (fp_text value Conn_02x05_Odd_Even (at -0.635 -7.215) (layer B.Fab))
    (fp_text user %R (at -0.635 -2.54 -90) (layer B.Fab))
    (pad 10 thru_hole oval (at -1.27 -5.08 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 /RST))
    (pad 9 thru_hole oval (at 0 -5.08 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -1.27 -3.81 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -3.81 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -1.27 -2.54 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -2.54 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 4 thru_hole oval (at -1.27 -1.27 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 /SWCLK))
    (pad 3 thru_hole oval (at 0 -1.27 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at -1.27 0 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 /SWDIO))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 /VSENSE))
    (model ${KISYS3DMOD}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_2x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer Top) (tedit 59FED5CC)
    (at 139.2428 75.7174 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 225) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /TX))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Horizontal (layer Top) (tedit 59FED5CB)
    (at 133.4262 81.407 180)
    (descr "Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x04 2.54mm double row")
    (fp_text reference J1 (at 5.655 -2.27) (layer F.SilkS) hide)
    (fp_text value Conn_02x04_Odd_Even (at 5.655 9.89) (layer F.Fab))
    (fp_text user %R (at 5.31 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /RST))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SWCLK))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /TX))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /OPT))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RX))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SWDIO))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VCC))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x04_P2.54mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text VCC (at 139.0396 71.2216) (layer F.SilkS))
  (gr_text V (at 130.9624 71.3486) (layer F.SilkS))
  (gr_text VSENSE (at 143.2052 71.4248) (layer F.SilkS))
  (gr_text G (at 136.2202 71.2216) (layer F.SilkS))
  (gr_text OPT (at 133.4516 71.374) (layer F.SilkS))
  (gr_text GND (at 141.3256 79.0448 90) (layer F.SilkS))
  (gr_text VCC (at 141.3256 82.296 90) (layer F.SilkS))
  (gr_text RX (at 136.8806 76.581 90) (layer F.SilkS))
  (gr_text TX (at 136.8552 73.1012 90) (layer F.SilkS))
  (gr_line (start 123.2662 84.6328) (end 131.9276 84.6328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.2662 67.6656) (end 123.2662 84.6328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.6558 67.6656) (end 123.2662 67.6656) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.542 71.5772) (end 141.6558 67.6656) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.542 80.6704) (end 145.542 71.5772) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.5796 84.6328) (end 145.542 80.6704) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.9276 84.6328) (end 141.5796 84.6328) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name /GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.7305 67.7672) (xy 141.224 67.9704) (xy 145.2118 71.7042) (xy 145.0594 80.2894) (xy 141.5034 83.8708)
        (xy 129.8194 83.7692)
      )
    )
  )
)
