<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.42" y2="0" width="0" layer="20"/>
<wire x1="31.42" y1="0" x2="31.42" y2="41.9" width="0" layer="20"/>
<wire x1="31.42" y1="41.9" x2="0" y2="41.9" width="0" layer="20"/>
<wire x1="0" y1="41.9" x2="0.0254" y2="28.321" width="0" layer="20"/>
<wire x1="0.0254" y1="28.321" x2="15.2654" y2="28.321" width="0" layer="20"/>
<wire x1="15.2654" y1="28.321" x2="15.24" y2="9.525" width="0" layer="20"/>
<wire x1="15.24" y1="9.525" x2="0" y2="9.525" width="0" layer="20"/>
<wire x1="0" y1="9.525" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>Wiper</text>
<text>12V</text>
<text>RV-Project.Com
Dimmer Control
Board V3.3
8/10/2019</text>
<text>Auto</text>
<text>12VIN</text>
<text>12VOUT</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>E</text>
<text>F</text>
<text>A</text>
<text>B</text>
<text>E</text>
<text>D</text>
<text>C</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>B</text>
<text>A</text>
<text>Resistor 
Programming</text>
<text>C</text>
<text>A</text>
</plain>
<libraries>
<library name="a-lib_Passives">
<description>Thru-Hole Passives (Resistors, Capacitors)</description>
<packages>
<package name="2OMMSLIDER_LED">
</package>
</packages>
</library>
<library name="a-lib_SMD">
<description>All SMD Devices; Actives, Passives, Connectors</description>
<packages>
<package name="1206-RES">
</package>
<package name="SMD-JUMPER_3">
<description>Pad Size: 0.18"x0.06"&lt;br&gt;Resist remoted between pads for ease of solder bridge.</description>
</package>
<package name="DO214AC_JBEND">
<description>Pad Size: 0.3"x0.1"</description>
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="1X03_HEADER">
<description>Pitch: 0.1" (2.54mm)
&lt;br&gt;Drill: 0.040" dia</description>
</package>
</packages>
</library>
<library name="a-lib">
<description>Archive Library (for old designs) - do not use for new components.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="1X01_HEADER">
<description>Drill: 0.039" dia</description>
</package>
<package name="1X04">
<description>Pitch: 0.1" (2.54mm)
&lt;br&gt;Drill: 0.040" dia</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="a-lib_Passives" package="2OMMSLIDER_LED" value="10K"/>
<element name="R2" library="a-lib_SMD" package="1206-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value=""/>
<element name="J1" library="a-lib_Connectors" package="1X03_HEADER" value="M3HEADER"/>
<element name="J2" library="a-lib_SMD" package="SMD-JUMPER_3" value="SMD-JUMPER"/>
<element name="J3" library="a-lib_SMD" package="SMD-JUMPER_3" value="SMD-JUMPER"/>
<element name="D1" library="a-lib_SMD" package="DO214AC_JBEND" value="1N400x">
<attribute name="MARKING" value="M1-M7"/>
<attribute name="NAME"/>
</element>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib_SMD" package="1206-RES" value="1K"/>
<element name="JP1" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="a-lib" package="1X04" value="M4HEADER"/>
</elements>
<signals>
<signal name="N$4">
<contactref element="J2" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="3"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="B"/>
</signal>
<signal name="N$3">
<contactref element="J4" pad="4"/>
<contactref element="JP3" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="JP2" pad="1"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="J4" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J4" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="E"/>
<contactref element="LED1" pad="K"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="A"/>
<contactref element="JP1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
