(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~65~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 94)
    (zones 0)
    (modules 5)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.7 3.3)
    (pad_drill 1.6)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 /GND)
  (net 4 /+5V)
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad9)")
  (net 7 /+12V)
  (net 8 "Net-(J1-Pad11)")
  (net 9 /-12V)
  (net 10 /PS-ON)
  (net 11 "Net-(J1-Pad18)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PS-ON)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (net_class Power ""
    (clearance 0.762)
    (trace_width 1.27)
    (via_dia 1.016)
    (via_drill 0.635)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+12V)
    (add_net /+5V)
    (add_net /-12V)
    (add_net /GND)
  )
  (module ATX2PCjr:Molex_Mini-Fit_Jr_5566-20A2_2x10_P4.20mm_Vertical-LARGE (layer F.Cu) (tedit 5B90B595)
    (at 75.26167 83.990307 45)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-20A2, example for new mpn: 39-28-920x, 10 Pins per row, Mounting: Snap-in Plastic Peg PCB Lock (http://www.molex.com/pdm_docs/sd/039289068_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr side entryplastic_peg")
    (fp_text reference J1 (at 18.9 -3.45 45) (layer F.SilkS))
    (fp_text value "ATX Connector" (at 18.9 9.95 45) (layer F.Fab))
    (fp_text user %R (at 18.9 -1.55 45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 4.199999 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 8.4 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 4 thru_hole oval (at 12.599999 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 /+5V))
    (pad 5 thru_hole oval (at 16.8 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 6 thru_hole oval (at 20.999999 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 /+5V))
    (pad 7 thru_hole oval (at 25.2 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 8 thru_hole oval (at 29.399999 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 33.6 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 37.8 0 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 7 /+12V))
    (pad 11 thru_hole oval (at 0 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 4.2 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 9 /-12V))
    (pad 13 thru_hole oval (at 8.4 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 14 thru_hole oval (at 12.6 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 /PS-ON))
    (pad 15 thru_hole oval (at 16.8 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 16 thru_hole oval (at 21 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 17 thru_hole oval (at 25.2 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 18 thru_hole oval (at 29.4 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad18)"))
    (pad 19 thru_hole oval (at 33.6 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 /+5V))
    (pad 20 thru_hole oval (at 37.8 5.5 45) (size 2.7 3.3) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 /+5V))
    (pad "" np_thru_hole circle (at -4.7 5.04 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 42.5 5.04 45) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5566-20A2_2x10_P4.20mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "ATX2PCjr:Mate-N-Lok Vertical" (layer F.Cu) (tedit 5B9096BA)
    (at 130 60.16 90)
    (fp_text reference J5 (at -1 3 90) (layer F.SilkS))
    (fp_text value "Floppy Power" (at 0 -3 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.24 0 90) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 7 /+12V))
    (pad 3 thru_hole circle (at 2.16 0 90) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 2 thru_hole circle (at -2.92 0 90) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 1 thru_hole circle (at -8 0 90) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 4 /+5V))
  )
  (module "ATX2PCjr:PCjr Power Board Card Edge" (layer F.Cu) (tedit 5B5B8AE1)
    (at 106.38 84)
    (fp_text reference J2 (at -2.24 1.852) (layer F.SilkS))
    (fp_text value "PCjr Card Edge" (at 20.32 13.97) (layer F.Fab))
    (pad 10 smd rect (at 37.75 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 7 /+12V))
    (pad 9 smd rect (at 33.8 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 8 smd rect (at 29.86 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 7 smd rect (at 25.91 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 4 /+5V))
    (pad 6 smd rect (at 21.97 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 4 /+5V))
    (pad 5 smd rect (at 18 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 4 /+5V))
    (pad 4 smd rect (at 14 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 4 /+5V))
    (pad 3 smd rect (at 10.13 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 2 smd rect (at 6.19 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 1 smd rect (at 2.25 5.66) (size 2.5 11.32) (layers F.Cu F.Paste F.Mask)
      (net 9 /-12V))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 143.81 68.95 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value "Power Switch Header" (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /PS-ON))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 143.81 58.27 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value "Fan Header" (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /+12V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "- + -\nFan" (at 139.7 55.88 270) (layer F.SilkS))
  (gr_text +12V (at 144.054 79.756 270) (layer F.SilkS))
  (gr_text -12V (at 108.204 79.756 270) (layer F.SilkS))
  (gr_text GND (at 137.958 80.978 270) (layer F.SilkS))
  (gr_text GND (at 114.3 80.772 270) (layer F.SilkS))
  (gr_text +5V (at 127.29 80.47 270) (layer F.SilkS))
  (gr_text "Y   K   K   R" (at 123.952 60.452 270) (layer F.SilkS))
  (gr_line (start 146.59 50.24) (end 101.01 50.24) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.58 84.01) (end 146.58 50.23) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.58 84.01) (end 146.58 96.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.75 86.48) (end 101.01 50.22) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.36 94.11) (end 64.75 86.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.41 94.11) (end 72.36 94.11) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.82 83.7) (end 81.41 94.11) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 83.7) (end 91.82 83.7) (layer Edge.Cuts) (width 0.15))
  (gr_text "Connector Clearance\n" (at 106 101) (layer Dwgs.User))
  (gr_text " - +\nPower" (at 139.7 67.31 270) (layer F.SilkS))
  (gr_text "By AkBKukU" (at 118.11 92.71) (layer B.Cu))
  (gr_text "ATX to PCjr   v1.12" (at 127 86.36) (layer B.Cu))
  (gr_line (start 106.426 96.266) (end 146.558 96.266) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106.426 83.693) (end 106.426 96.266) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 101.59833 83.693) (end 106.426 83.693) (layer Edge.Cuts) (width 0.2))
  (zone (net 4) (net_name /+5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.162 38.1) (xy 89.662 34.29) (xy 54.102 94.742) (xy 130.556 125.73) (xy 190.754 76.708)
        (xy 185.928 43.434)
      )
    )
  )
  (zone (net 3) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.648 84.074) (xy 155.702 84.074) (xy 153.67 34.036) (xy 90.424 44.704) (xy 50.546 76.962)
        (xy 60.198 105.41) (xy 94.488 94.234) (xy 104.902 83.82) (xy 104.394 84.074)
      )
    )
  )
)
