(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 93)
    (zones 0)
    (modules 7)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 DIN)
  (net 4 CLK)
  (net 5 LOAD)
  (net 6 "Net-(J2-Pad1)")
  (net 7 S.)
  (net 8 SG)
  (net 9 SF)
  (net 10 SE)
  (net 11 SD)
  (net 12 SC)
  (net 13 SB)
  (net 14 SA)
  (net 15 D0)
  (net 16 D1)
  (net 17 D2)
  (net 18 D3)
  (net 19 D4)
  (net 20 D5)
  (net 21 D6)
  (net 22 D7)
  (net 23 "Net-(R1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CLK)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net DIN)
    (add_net GND)
    (add_net LOAD)
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net S.)
    (add_net SA)
    (add_net SB)
    (add_net SC)
    (add_net SD)
    (add_net SE)
    (add_net SF)
    (add_net SG)
    (add_net VCC)
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 19.812 26.3001 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 3.0845 0.0508 180) (layer F.SilkS))
    (fp_text value C (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 5CA633E9)
    (at 41.5036 19.7104)
    (descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x05 2.54mm single row")
    (fp_text reference SPI (at 0 -2.77) (layer F.SilkS))
    (fp_text value SPI (at 0 12.93) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 CLK))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 DIN))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 LOAD))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5CA633F3)
    (at 19.812 19.812)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference DCHN (at 0.0508 -2.1336) (layer F.SilkS))
    (fp_text value DOUT (at 0 2.77) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5CA63422)
    (at 38.9636 13.6144 270)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference SEG (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value SEGMENTS (at 0 20.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SD))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 S.))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 SE))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SC))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SG))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 SB))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SF))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 SA))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5CA6341D)
    (at 38.862 34.544 270)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference DIG (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value DIGITS (at 0 20.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 D1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 D5))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 D7))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 D3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 D2))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 D6))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 D4))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 D0))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5CA63416)
    (at 30.5165 16.51)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.82) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 VCC))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 23 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm (layer F.Cu) (tedit 5CA63737)
    (at 30.226 24.638 90)
    (descr "24-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -8.8 90) (layer F.SilkS) hide)
    (fp_text value MAX7219 (at -8.2296 -11.5316 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -6.985 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 DIN))
    (pad 2 smd rect (at -4.7 -5.715 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 D0))
    (pad 3 smd rect (at -4.7 -4.445 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 D4))
    (pad 4 smd rect (at -4.7 -3.175 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -4.7 -1.905 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 D6))
    (pad 6 smd rect (at -4.7 -0.635 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 D2))
    (pad 7 smd rect (at -4.7 0.635 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 D3))
    (pad 8 smd rect (at -4.7 1.905 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 D7))
    (pad 9 smd rect (at -4.7 3.175 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -4.7 4.445 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 D5))
    (pad 11 smd rect (at -4.7 5.715 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 D1))
    (pad 12 smd rect (at -4.7 6.985 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 LOAD))
    (pad 13 smd rect (at 4.7 6.985 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 CLK))
    (pad 14 smd rect (at 4.7 5.715 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 SA))
    (pad 15 smd rect (at 4.7 4.445 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 SF))
    (pad 16 smd rect (at 4.7 3.175 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 SB))
    (pad 17 smd rect (at 4.7 1.905 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 SG))
    (pad 18 smd rect (at 4.7 0.635 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R1-Pad2)"))
    (pad 19 smd rect (at 4.7 -0.635 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 20 smd rect (at 4.7 -1.905 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 SC))
    (pad 21 smd rect (at 4.7 -3.175 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 SE))
    (pad 22 smd rect (at 4.7 -4.445 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 S.))
    (pad 23 smd rect (at 4.7 -5.715 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 SD))
    (pad 24 smd rect (at 4.7 -6.985 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text * (at 21.844 28.6004) (layer F.SilkS))
  (gr_text I (at 27.432 16.6116) (layer F.SilkS))
  (gr_line (start 43.18 11.43) (end 17.78 11.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 43.18 36.83) (end 43.18 11.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 17.78 36.83) (end 43.18 36.83) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 17.78 11.43) (end 17.78 36.83) (layer Edge.Cuts) (width 0.15))
  (gr_text "D: 1 5 7 3 2 6 4 0" (at 31.3944 32.3088) (layer B.SilkS))
  (gr_text "S: A F B G C E . D" (at 31.75 16.3576) (layer B.SilkS))
  (gr_text "CLK\nVCC\nDIN\nCS/LD\nGND" (at 39.878 24.892) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.78 11.43) (xy 17.78 36.83) (xy 43.18 36.83) (xy 43.18 11.43)
      )
    )
  )
)
