(kicad_pcb (version 20171130) (host pcbnew 5.1.8-db9833491~88~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 3)
    (zones 0)
    (modules 6)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad3)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C1-Pad3)")
  )
  (module dpg_vcap:161-60-polyvaricon (layer F.Cu) (tedit 5FC1B3FC)
    (at 157.48 -1066.8 270)
    (descr "161/60 polyvaricon")
    (tags polyvaricon)
    (attr smd)
    (fp_text reference C1 (at 11.684 8.128 180) (layer F.SilkS))
    (fp_text value C_Variable_2_section (at 0 8.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 11.684 8.382 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.5) (layers *.Cu *.Mask))
    (pad 3 smd rect (at 7.8 14.55 180) (size 7.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad3)"))
    (pad 2 smd rect (at 0 14.55 180) (size 7.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -7.8 14.55 180) (size 7.5 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad "" np_thru_hole circle (at 7 0 180) (size 1.25 1.25) (drill 1.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7 0 180) (size 1.25 1.25) (drill 1.25) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-50-3_LongPad-WithHole_Housing.wrl
      (offset (xyz -0.7619999885559082 3.301999950408935 -0.7619999885559082))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 157.48 -1052.449)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 5.588 -0.127) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 157.48 -1044.575)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 7.62 -0.889) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 0)
    (at 140.208 -1058.926 270)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J3 (at 0 -3.50012 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0.24892 3.74904 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.064 4.064) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad3)"))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 0)
    (at 140.208 -1066.8 270)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J2 (at 0 -3.50012 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0.24892 3.74904 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.064 4.064) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 0)
    (at 140.208 -1074.674 270)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at 0 -3.50012 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0.24892 3.74904 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 4.064 4.064) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
  )
  (dimension 13.97 (width 0.15) (layer Dwgs.User)
    (gr_text "13.970 mm" (at 153.005 -1066.8 270) (layer Dwgs.User))
    (feature1 (pts (xy 157.48 -1059.815) (xy 153.718579 -1059.815)))
    (feature2 (pts (xy 157.48 -1073.785) (xy 153.718579 -1073.785)))
    (crossbar (pts (xy 154.305 -1073.785) (xy 154.305 -1059.815)))
    (arrow1a (pts (xy 154.305 -1059.815) (xy 153.718579 -1060.941504)))
    (arrow1b (pts (xy 154.305 -1059.815) (xy 154.891421 -1060.941504)))
    (arrow2a (pts (xy 154.305 -1073.785) (xy 153.718579 -1072.658496)))
    (arrow2b (pts (xy 154.305 -1073.785) (xy 154.891421 -1072.658496)))
  )
  (dimension 13.97 (width 0.15) (layer Dwgs.User)
    (gr_text "0.5500 in" (at 162.336 -1066.8 270) (layer Dwgs.User))
    (feature1 (pts (xy 157.48 -1059.815) (xy 161.622421 -1059.815)))
    (feature2 (pts (xy 157.48 -1073.785) (xy 161.622421 -1073.785)))
    (crossbar (pts (xy 161.036 -1073.785) (xy 161.036 -1059.815)))
    (arrow1a (pts (xy 161.036 -1059.815) (xy 160.449579 -1060.941504)))
    (arrow1b (pts (xy 161.036 -1059.815) (xy 161.622421 -1060.941504)))
    (arrow2a (pts (xy 161.036 -1073.785) (xy 160.449579 -1072.658496)))
    (arrow2b (pts (xy 161.036 -1073.785) (xy 161.622421 -1072.658496)))
  )
  (gr_line (start 168.656 -1040.384) (end 168.656 -1077.976) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 -1040.384) (end 137.16 -1077.976) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.656 -1040.384) (end 137.16 -1040.384) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 -1077.976) (end 168.656 -1077.976) (layer Edge.Cuts) (width 0.1))
)
