(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 70)
    (no_connects 0)
    (area 49.924999 125.924999 115.075001 182.575001)
    (thickness 1.6)
    (drawings 21)
    (tracks 284)
    (zones 0)
    (modules 43)
    (nets 56)
  )
  (page A4)
  (layers
    (0 top signal)
    (31 bottom signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 50 126)
    (grid_origin 50 126)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D12-Pad1)")
  (net 7 "Net-(D4-Pad1)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 "Net-(D5-Pad1)")
  (net 10 "Net-(D7-Pad1)")
  (net 11 "Net-(D7-Pad2)")
  (net 12 "Net-(D8-Pad1)")
  (net 13 "Net-(D10-Pad1)")
  (net 14 "Net-(D10-Pad2)")
  (net 15 "Net-(D11-Pad1)")
  (net 16 "Net-(D13-Pad1)")
  (net 17 "Net-(D13-Pad2)")
  (net 18 "Net-(D14-Pad1)")
  (net 19 "Net-(D16-Pad1)")
  (net 20 "Net-(D16-Pad2)")
  (net 21 "Net-(D17-Pad1)")
  (net 22 /PP3)
  (net 23 "Net-(Q1-Pad3)")
  (net 24 +5V)
  (net 25 "Net-(Q2-Pad2)")
  (net 26 /SIGLED)
  (net 27 /ID_SD)
  (net 28 /ID_SC)
  (net 29 "Net-(U1-Pad3)")
  (net 30 "Net-(U1-Pad4)")
  (net 31 "Net-(U1-Pad5)")
  (net 32 "Net-(U1-Pad7)")
  (net 33 "Net-(U1-Pad8)")
  (net 34 "Net-(U1-Pad10)")
  (net 35 "Net-(U1-Pad11)")
  (net 36 "Net-(U1-Pad12)")
  (net 37 "Net-(U1-Pad13)")
  (net 38 "Net-(U1-Pad15)")
  (net 39 "Net-(U1-Pad16)")
  (net 40 "Net-(U1-Pad17)")
  (net 41 "Net-(U1-Pad18)")
  (net 42 /SPI_MOSI)
  (net 43 /SPI_MISO)
  (net 44 "Net-(U1-Pad22)")
  (net 45 /SPI_SCLK)
  (net 46 /SPI_CE0)
  (net 47 "Net-(U1-Pad26)")
  (net 48 "Net-(U1-Pad29)")
  (net 49 "Net-(U1-Pad31)")
  (net 50 "Net-(U1-Pad32)")
  (net 51 "Net-(U1-Pad33)")
  (net 52 "Net-(U1-Pad35)")
  (net 53 "Net-(U1-Pad36)")
  (net 54 "Net-(U1-Pad37)")
  (net 55 "Net-(U1-Pad38)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net /PP3)
    (add_net /SIGLED)
    (add_net /SPI_CE0)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net /SPI_SCLK)
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(Q1-Pad3)")
  )
  (module SMD_Packages:SOIC-8-N (layer top) (tedit 58993444)
    (at 57 138 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 3.25 -1.5 180) (layer F.SilkS))
    (fp_text value CAT24C32 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 22 /PP3))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 28 /ID_SC))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 27 /ID_SD))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 1 GND))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm locked (layer top) (tedit 589884A4)
    (at 53.5 129.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at -5.75 -2.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm locked (layer top) (tedit 589884AB)
    (at 111.5 129.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 -4.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm locked (layer top) (tedit 589884C1)
    (at 111.5 179)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 6.75 2.75) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm locked (layer top) (tedit 58988493)
    (at 53.5 179)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 -2.75) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 locked (layer top) (tedit 58988498)
    (at 61 180)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 8.25 3.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 locked (layer top) (tedit 589884DC)
    (at 61 160)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 7.75 3.25) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DE6C)
    (at 64.5 141.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DE72)
    (at 64.5 147.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DE7A)
    (at 64.5 153.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DE80)
    (at 71.5 141.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D4 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DE87)
    (at 71.5 147.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D5 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DE8D)
    (at 71.5 153.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D6 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DE97)
    (at 78.5 141.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D7 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DE9C)
    (at 78.5 147.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D8 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D7-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DEA1)
    (at 78.5 153.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D9 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DEB4)
    (at 85.5 141.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D10 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D10-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DEBB)
    (at 85.5 147.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D11 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D11-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DEC1)
    (at 85.5 153.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D12 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D11-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DEC7)
    (at 92.5 141.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D13 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D13-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(D13-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DECC)
    (at 92.5 147.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D14 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(D14-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DED4)
    (at 92.5 153.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D15 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(D14-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DEDA)
    (at 99.5 141.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D16 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(D16-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(D16-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DEDF)
    (at 99.5 147.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D17 (at 1.25 -2) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(D17-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(D16-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 5898DEF2)
    (at 99.5 153.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D18 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(D17-Pad1)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer top) (tedit 58993480)
    (at 104 177.5 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at -2.25 1.25 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PP3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:SOT126_SOT32_Housing_Horizontal (layer top) (tedit 0)
    (at 110 144 180)
    (descr "SOT126, SOT32, Housing, Horizontal,")
    (tags "SOT126, SOT32, Housing, Horizontal,")
    (fp_text reference Q1 (at 0.14986 -17.89938 180) (layer F.SilkS))
    (fp_text value BD139 (at 0.70104 4.30022 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.69926 1.69926) (drill 1.19888) (layers *.Cu *.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 1 thru_hole circle (at -2.29108 0 180) (size 1.69926 1.69926) (drill 1.19888) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.29108 0 180) (size 1.69926 1.69926) (drill 1.19888) (layers *.Cu *.Mask)
      (net 23 "Net-(Q1-Pad3)"))
    (pad "" np_thru_hole circle (at 0 -12.79906 180) (size 3.2004 3.2004) (drill 3.2004) (layers *.Cu *.Mask))
    (model TO_SOT_Packages_THT.3dshapes/SOT126_SOT32_Housing_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer top) (tedit 587A3A7B)
    (at 53 172)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference Q2 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value Q_Photo_NPN (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 +5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(Q2-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58307C0D)
    (at 66.5 137.5)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 5 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 24 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58307C0D)
    (at 73.5 137.5)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 5 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 24 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58307C0D)
    (at 80.5 137.5)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 5 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 24 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 11 "Net-(D7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 5898DF05)
    (at 110 136 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 2 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 26 /SIGLED))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 23 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58993495)
    (at 110 139)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -0.25 2) (layer F.SilkS))
    (fp_text value 100k (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 23 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58307C0D)
    (at 87.5 137.5)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 5 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 24 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 14 "Net-(D10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58307C0D)
    (at 94.5 137.5)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 5 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 24 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 17 "Net-(D13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58307C0D)
    (at 101.5 137.5)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 5 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 24 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 20 "Net-(D16-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 5898DF3D)
    (at 55 165 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -5 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 25 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 5899346C)
    (at 57 142.5 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 4.75 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 22 /PP3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58993460)
    (at 57 148 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 4.75 0 180) (layer F.SilkS))
    (fp_text value 3.9k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 27 /ID_SD))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer top) (tedit 58993469)
    (at 57 145.25 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at 4.75 0 180) (layer F.SilkS))
    (fp_text value 3.9k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers top F.Paste F.Mask)
      (net 28 /ID_SC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer top) (tedit 58993448)
    (at 58.5 131 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference U1 (at -2.5 -0.75 180) (layer F.SilkS))
    (fp_text value Raspberry_Pi_2_3 (at 1.27 50.65 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /SPI_MOSI))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /SPI_MISO))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /SPI_SCLK))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /SPI_CE0))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /ID_SD))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /ID_SC))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(U1-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(U1-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(U1-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(U1-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(U1-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(U1-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /SIGLED))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer top) (tedit 58993477)
    (at 55 162 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 2 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers top F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer top) (tedit 589934AB)
    (at 57 154.75 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 3.5 -1.5 180) (layer F.SilkS))
    (fp_text value MCP3002 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 24 +5V))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 45 /SPI_SCLK))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 43 /SPI_MISO))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 42 /SPI_MOSI))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 25 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers top F.Paste F.Mask)
      (net 46 /SPI_CE0))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 115 129) (end 115 179.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Raspberry Pi IR Led Camera Hat" (at 89 180.75) (layer F.SilkS))
  (gr_text "Pi Cam" (at 65 169.5 90) (layer F.SilkS))
  (gr_line (start 50 145) (end 50 164) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95 163.5) (end 95 162.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95 163.5) (end 94 163.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96 171) (end 96 163.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 171) (end 94 163.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 178.5) (end 94 171) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95 178.5) (end 95 179.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95 178.5) (end 96 178.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96 171) (end 96 178.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 45 (width 0.3) (layer Dwgs.User)
    (gr_text "45.000 mm" (at 72.5 188.35) (layer Dwgs.User))
    (feature1 (pts (xy 95 182.5) (xy 95 189.7)))
    (feature2 (pts (xy 50 182.5) (xy 50 189.7)))
    (crossbar (pts (xy 50 187) (xy 95 187)))
    (arrow1a (pts (xy 95 187) (xy 93.873496 187.586421)))
    (arrow1b (pts (xy 95 187) (xy 93.873496 186.413579)))
    (arrow2a (pts (xy 50 187) (xy 51.126504 187.586421)))
    (arrow2b (pts (xy 50 187) (xy 51.126504 186.413579)))
  )
  (gr_line (start 50 164) (end 50 179.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 145) (end 50 129) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53 182.5) (end 112 182.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53 126) (end 112 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112 129) (end 112 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 53 179.5) (end 53 182.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112 179.5) (end 115 179.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 53 129) (end 50 129) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.5 172) (xy 105 172) (xy 105 132.5) (xy 114.5 132.5)
      )
    )
  )
)
