<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.0">
<drawing>
<board>
<plain>
<wire x1="161.210625" y1="49.768125" x2="161.210625" y2="-1.11125" width="0" layer="20"/>
<wire x1="161.210625" y1="-1.11125" x2="21.11375" y2="-1.11125" width="0" layer="20"/>
<text>ATF16V8B/QL</text>
<text>Routage
"Vente"</text>
<text>Routage
"FFVIMan"</text>
<text>Banc de
test :
PIC/SPLD</text>
<text>FFVIMan.fr
R&amp;D</text>
<text>FFVIMan.fr
R&amp;D</text>
<text>FFVIMan.fr - R&amp;D</text>
<text>CIC</text>
<text>uIGR</text>
<text>Patch D4</text>
<wire x1="161.210625" y1="49.768125" x2="137.715625" y2="49.768125" width="0" layer="20"/>
<wire x1="137.715625" y1="49.768125" x2="135.334375" y2="47.386875" width="0" layer="20"/>
<wire x1="135.334375" y1="47.386875" x2="68.976875" y2="47.386875" width="0" layer="20"/>
<wire x1="68.976875" y1="47.386875" x2="66.595625" y2="49.768125" width="0" layer="20"/>
<wire x1="66.595625" y1="49.768125" x2="21.11375" y2="49.768125" width="0" layer="20"/>
<wire x1="21.11375" y1="49.768125" x2="21.11375" y2="-1.11125" width="0" layer="20"/>
<hole x="43.18" y="33.3375" drill="12.7"/>
<text>F1</text>
<text>VCC</text>
<text>GND</text>
<text>LED60</text>
<text>LED50</text>
<text>CP10</text>
<text>CPUN</text>
<text>CP8</text>
<text>CP6</text>
<text>CIC11</text>
<text>CIC10</text>
<text>CIC8</text>
<text>CIC7</text>
<text>CIC2</text>
<text>CIC1</text>
<text>D4OUT</text>
<text>PARDN</text>
<text>PA7</text>
<text>PA6</text>
<text>PA5</text>
<text>PA4</text>
<text>PA3</text>
<text>PA2</text>
<text>PA1</text>
<text>PA0</text>
<text>VCCEXT</text>
<text>X1EXT</text>
<text>GND</text>
<text>VPP</text>
<text>VDD</text>
<text>DAT</text>
<text>CLK</text>
<text>DIP SW</text>
<text>ICSP OFF</text>
<text>R</text>
<text>Rev.2</text>
<text>02/2019</text>
<text>02/2019</text>
<text>ICSP</text>
<text>Fusible</text>
<text>Adapt.</text>
<text>VCC</text>
<text>GND</text>
<text>LED</text>
<text>SW</text>
<text>EXT1</text>
<text>PA7</text>
<text>PA1</text>
<text>PA3</text>
<text>PA5</text>
<text>PA6</text>
<text>PA4</text>
<text>PA2</text>
<text>CP6</text>
<text>CP10</text>
<text>CP8</text>
<text>CIC10</text>
<text>CIC1</text>
<text>CIC2</text>
<text>X1EXT</text>
<text>VCCEXT</text>
<text>PA0</text>
<text>PARDN</text>
<text>VCC</text>
<text>D4OUT</text>
<text>GND</text>
<text>CIC7</text>
<text>CIC8</text>
<text>CPUN</text>
<text>LED50</text>
<text>LED60</text>
<text>CIC11</text>
</plain>
<libraries>
<library name="con-3m">
<description>&lt;b&gt;3M Connectors&lt;/b&gt;&lt;p&gt;
PCMCIA-CompactFlash Connectors&lt;p&gt;
Zero Insertion Force Socked&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="214-3339-00-0602J">
<description>&lt;b&gt;3M TEXTOOL 14 pol. DIP&lt;/b&gt; Lever actuated zero insertion force mechanism &lt;p&gt;
Hersteller: 3M TEXTOOL&lt;br&gt;
Herstellerbez.:  214-3339-00-0602J&lt;br&gt;
Farnell Best.-Nr.: 4666290&lt;br&gt;
Source: http://www.3M.com/ehpd</description>
</package>
<package name="240-1280-00-0602J">
<description>&lt;b&gt;3M TEXTOOL 40 pol. DIP&lt;/b&gt; Lever actuated zero insertion force mechanism &lt;p&gt;
Hersteller: 3M TEXTOOL&lt;br&gt;
Herstellerbez.:  240-1280-00-0602J&lt;br&gt;
Farnell Best.-Nr.: 4665466&lt;br&gt;
Source: http://www.3M.com/ehpd</description>
</package>
</packages>
</library>
<library name="rcl-nouv">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl-patch">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="portmanette">
<packages>
<package name="MLXDRSMT28">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X25">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="pcb-vente">
<packages>
<package name="PADBANC">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-02">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
<package name="EDG-05">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="7395-05">
<description>&lt;b&gt;KK® 254 Wire-to-Board Header, Right Angle, with Friction Lock, 5 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022057058_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="16F630/16F676" library="con-3m" package="214-3339-00-0602J" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="16F684/ICSP" library="con-3m" package="214-3339-00-0602J" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl-nouv" package="R0603" value="180">
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl-nouv" package="R0603" value="180">
<attribute name="NAME"/>
</element>
<element name="C4" library="rcl-patch" package="C0603" value="">
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl-patch" package="C0603" value="">
<attribute name="NAME"/>
</element>
<element name="C1" library="rcl-patch" package="C0603" value="">
<attribute name="NAME"/>
</element>
<element name="ATF16V8B" library="con-3m" package="240-1280-00-0602J" value="">
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl-patch" package="C0603" value="">
<attribute name="NAME"/>
</element>
<element name="CONT1" library="portmanette" package="MLXDRSMT28" value="">
<attribute name="NAME"/>
</element>
<element name="EXT1" library="SparkFun-Passives" package="1X25" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl-nouv" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ICSP" library="con-molex" package="7395-05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="special" package="EDG-05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl-nouv" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW3" library="special" package="EDG-02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCCIN" library="pcb-vente" package="PADBANC" value=""/>
<element name="GNDIN" library="pcb-vente" package="PADBANC" value=""/>
</elements>
<signals>
<signal name="VDD/VCC">
<contactref element="ICSP" pad="3"/>
<contactref element="16F684/ICSP" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="SW2" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="16F630/16F676" pad="8"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="SW2" pad="5"/>
<contactref element="EXT1" pad="25"/>
<contactref element="CONT1" pad="17"/>
<contactref element="ATF16V8B" pad="20"/>
<contactref element="ATF16V8B" pad="40"/>
<contactref element="VCCIN" pad="FIL"/>
</signal>
<signal name="CIC8">
<contactref element="16F684/ICSP" pad="9"/>
<contactref element="16F630/16F676" pad="6"/>
<contactref element="R3" pad="2"/>
<contactref element="EXT1" pad="16"/>
<contactref element="CONT1" pad="9"/>
</signal>
<signal name="GND">
<contactref element="16F684/ICSP" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="16F630/16F676" pad="14"/>
<contactref element="16F630/16F676" pad="11"/>
<contactref element="16F684/ICSP" pad="1"/>
<contactref element="16F630/16F676" pad="7"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="POWER" pad="K"/>
<contactref element="ICSP" pad="4"/>
<contactref element="SW2" pad="1"/>
<contactref element="EXT1" pad="26"/>
<contactref element="CONT1" pad="13"/>
<contactref element="ATF16V8B" pad="10"/>
<contactref element="ATF16V8B" pad="30"/>
<contactref element="GNDIN" pad="FIL"/>
</signal>
<signal name="VPP/D4MODE">
<contactref element="ICSP" pad="5"/>
<contactref element="16F684/ICSP" pad="11"/>
<contactref element="SW2" pad="9"/>
</signal>
<signal name="D4MODE">
<contactref element="16F630/16F676" pad="10"/>
<contactref element="SW2" pad="2"/>
<contactref element="ATF16V8B" pad="13"/>
<contactref element="ATF16V8B" pad="33"/>
</signal>
<signal name="D4ONOFF">
<contactref element="16F684/ICSP" pad="14"/>
<contactref element="ATF16V8B" pad="15"/>
<contactref element="ATF16V8B" pad="35"/>
</signal>
<signal name="CI2">
<contactref element="16F684/ICSP" pad="2"/>
<contactref element="16F630/16F676" pad="13"/>
</signal>
<signal name="CI1">
<contactref element="16F684/ICSP" pad="3"/>
<contactref element="16F630/16F676" pad="12"/>
</signal>
<signal name="TR3">
<contactref element="16F684/ICSP" pad="13"/>
<contactref element="R1" pad="2"/>
<contactref element="SW3" pad="1"/>
</signal>
<signal name="TR2">
<contactref element="R2" pad="2"/>
<contactref element="16F684/ICSP" pad="12"/>
<contactref element="SW3" pad="2"/>
</signal>
<signal name="L50">
<contactref element="R2" pad="1"/>
<contactref element="SW3" pad="3"/>
<contactref element="EXT1" pad="23"/>
<contactref element="CONT1" pad="3"/>
</signal>
<signal name="L60">
<contactref element="R1" pad="1"/>
<contactref element="SW3" pad="4"/>
<contactref element="EXT1" pad="24"/>
<contactref element="CONT1" pad="5"/>
</signal>
<signal name="CP8">
<contactref element="16F684/ICSP" pad="4"/>
<contactref element="EXT1" pad="20"/>
<contactref element="CONT1" pad="8"/>
</signal>
<signal name="CPUN">
<contactref element="16F684/ICSP" pad="10"/>
<contactref element="EXT1" pad="22"/>
<contactref element="CONT1" pad="7"/>
</signal>
<signal name="CLK/CP10">
<contactref element="ICSP" pad="1"/>
<contactref element="16F684/ICSP" pad="5"/>
<contactref element="SW2" pad="8"/>
</signal>
<signal name="CP10">
<contactref element="SW2" pad="3"/>
<contactref element="EXT1" pad="21"/>
<contactref element="CONT1" pad="10"/>
</signal>
<signal name="DAT/CP6">
<contactref element="ICSP" pad="2"/>
<contactref element="16F684/ICSP" pad="6"/>
<contactref element="SW2" pad="7"/>
</signal>
<signal name="CP6">
<contactref element="SW2" pad="4"/>
<contactref element="EXT1" pad="19"/>
<contactref element="CONT1" pad="12"/>
</signal>
<signal name="CIC11">
<contactref element="16F630/16F676" pad="1"/>
<contactref element="EXT1" pad="18"/>
<contactref element="CONT1" pad="1"/>
</signal>
<signal name="CIC2">
<contactref element="16F630/16F676" pad="2"/>
<contactref element="EXT1" pad="14"/>
<contactref element="CONT1" pad="2"/>
</signal>
<signal name="CIC1">
<contactref element="16F630/16F676" pad="3"/>
<contactref element="EXT1" pad="13"/>
<contactref element="CONT1" pad="4"/>
</signal>
<signal name="CIC10">
<contactref element="16F630/16F676" pad="4"/>
<contactref element="EXT1" pad="17"/>
<contactref element="CONT1" pad="6"/>
</signal>
<signal name="CIC7">
<contactref element="16F630/16F676" pad="9"/>
<contactref element="EXT1" pad="15"/>
<contactref element="CONT1" pad="11"/>
</signal>
<signal name="PARDN">
<contactref element="EXT1" pad="11"/>
<contactref element="CONT1" pad="19"/>
<contactref element="ATF16V8B" pad="9"/>
<contactref element="ATF16V8B" pad="29"/>
</signal>
<signal name="D4OUT">
<contactref element="EXT1" pad="12"/>
<contactref element="CONT1" pad="15"/>
<contactref element="ATF16V8B" pad="16"/>
<contactref element="ATF16V8B" pad="17"/>
<contactref element="ATF16V8B" pad="18"/>
<contactref element="ATF16V8B" pad="19"/>
<contactref element="ATF16V8B" pad="36"/>
<contactref element="ATF16V8B" pad="37"/>
<contactref element="ATF16V8B" pad="38"/>
<contactref element="ATF16V8B" pad="39"/>
</signal>
<signal name="PA0">
<contactref element="EXT1" pad="3"/>
<contactref element="CONT1" pad="21"/>
<contactref element="ATF16V8B" pad="1"/>
<contactref element="ATF16V8B" pad="28"/>
</signal>
<signal name="PA2">
<contactref element="EXT1" pad="5"/>
<contactref element="CONT1" pad="26"/>
<contactref element="ATF16V8B" pad="2"/>
<contactref element="ATF16V8B" pad="27"/>
</signal>
<signal name="PA4">
<contactref element="EXT1" pad="7"/>
<contactref element="CONT1" pad="24"/>
<contactref element="ATF16V8B" pad="3"/>
<contactref element="ATF16V8B" pad="26"/>
</signal>
<signal name="PA6">
<contactref element="EXT1" pad="9"/>
<contactref element="CONT1" pad="22"/>
<contactref element="ATF16V8B" pad="4"/>
<contactref element="ATF16V8B" pad="25"/>
</signal>
<signal name="PA1">
<contactref element="EXT1" pad="4"/>
<contactref element="CONT1" pad="16"/>
<contactref element="ATF16V8B" pad="5"/>
<contactref element="ATF16V8B" pad="22"/>
</signal>
<signal name="PA3">
<contactref element="EXT1" pad="6"/>
<contactref element="CONT1" pad="18"/>
<contactref element="ATF16V8B" pad="6"/>
<contactref element="ATF16V8B" pad="23"/>
</signal>
<signal name="PA5">
<contactref element="EXT1" pad="8"/>
<contactref element="CONT1" pad="20"/>
<contactref element="ATF16V8B" pad="7"/>
<contactref element="ATF16V8B" pad="24"/>
</signal>
<signal name="PA7">
<contactref element="EXT1" pad="10"/>
<contactref element="CONT1" pad="14"/>
<contactref element="ATF16V8B" pad="8"/>
<contactref element="ATF16V8B" pad="21"/>
</signal>
<signal name="X1EXT">
<contactref element="EXT1" pad="1"/>
<contactref element="CONT1" pad="25"/>
</signal>
<signal name="VCCEXT">
<contactref element="EXT1" pad="2"/>
<contactref element="CONT1" pad="23"/>
</signal>
<signal name="LEDPOWER">
<contactref element="POWER" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="SW2" pad="10"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="S$2">
</signal>
<signal name="S$3">
</signal>
<signal name="S$1">
</signal>
<signal name="S$4">
</signal>
<signal name="S$9">
</signal>
<signal name="S$10">
</signal>
<signal name="S$11">
</signal>
<signal name="S$12">
</signal>
<signal name="S$13">
</signal>
<signal name="CONTOUR">
</signal>
<signal name="S$6">
</signal>
<signal name="S$5">
</signal>
<signal name="S$7">
</signal>
</signals>
</board>
</drawing>
</eagle>
