(kicad_pcb (version 4) (host pcbnew 4.0.7-e1-6374~58~ubuntu16.04.1)
  (general
    (links 11)
    (no_connects 0)
    (area 123.383333 59.065 162.116667 113.655)
    (thickness 1.6)
    (drawings 6)
    (tracks 44)
    (zones 0)
    (modules 11)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x000f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D3-Pad2)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 59974ED2)
    (at 138.25 67.5)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 599751FA)
    (at 147.8 71.2 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 2.31 180) (layer B.SilkS))
    (fp_text value 2K (at 5.05 0.1 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 599DF729)
    (at 147.8 91.6 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 2.1818 -2.1006 180) (layer B.SilkS))
    (fp_text value 750 (at 5.05 0.1 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 599751E4)
    (at 147.8 84.9 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 2.31 180) (layer B.SilkS))
    (fp_text value 2K (at 5.05 -0.1 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:Push_E-Switch_KS01Q01 locked (layer F.Cu) (tedit 54BFC791)
    (at 140.25 74)
    (descr "E-Switch KS01Q01")
    (tags "Push Button")
    (fp_text reference SW1 (at 2.5 2.5) (layer F.SilkS))
    (fp_text value SW_Push (at 2.5 -2.04914) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 5 5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model Buttons_Switches_THT.3dshapes/Push_E-Switch_KS01Q01.wrl
      (at (xyz 0.1 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_5pin_straight (layer B.Cu) (tedit 599DF77D)
    (at 142.75 107.5 180)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 5pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 5pin, straight,")
    (fp_text reference J1 (at -0.0234 3.9188 180) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 0 -5.08 180) (layer B.Fab))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 3 thru_hole oval (at 0 0 180) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 0 180) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 59974EDE)
    (at 142.75 95.25)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 59974ED2)
    (at 147.25 67.5)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_D5.0mm locked (layer F.Cu) (tedit 587A3A7B)
    (at 141.5 64)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value PWR (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm locked (layer F.Cu) (tedit 587A3A7B)
    (at 141.5 101.5)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value CAM (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm locked (layer F.Cu) (tedit 587A3A7B)
    (at 141.5 89)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value MIC (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Arthur Fabre\nIBM Research Almaden\n2017/08/18" (at 147.7264 98.8822 90) (layer F.SilkS))
  (gr_text "Cube LLB v1" (at 142.7988 110.5408) (layer F.SilkS))
  (gr_line (start 135.5 61) (end 135.5 111.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150 111.5) (end 150 61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.5 111.5) (end 150 111.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.5 61) (end 150 61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.127) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150 111.5) (xy 135.5 111.5) (xy 135.5 61) (xy 150 61)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.127) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150 111.5) (xy 135.5 111.5) (xy 135.5 61) (xy 150 61)
      )
    )
  )
)
