<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="18.415" y2="0" width="0.254" layer="20"/>
<wire x1="18.415" y1="0" x2="20.32" y2="1.905" width="0.254" layer="20" curve="90"/>
<wire x1="20.32" y1="1.905" x2="20.32" y2="10.795" width="0.254" layer="20"/>
<wire x1="20.32" y1="10.795" x2="18.415" y2="12.7" width="0.254" layer="20" curve="90"/>
<wire x1="18.415" y1="12.7" x2="1.905" y2="12.7" width="0.254" layer="20"/>
<wire x1="1.905" y1="12.7" x2="0" y2="10.795" width="0.254" layer="20" curve="90"/>
<wire x1="0" y1="10.795" x2="0" y2="0" width="0.254" layer="20"/>
<text>GND</text>
<text>VCC</text>
<text>DIV</text>
<text>OUT</text>
<text>KD0GLS 2019</text>
<text>COARSE</text>
<text>FINE</text>
<text>LTC1799 VFDO</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="CONN_BREAKAWAY_1X1_100_SQUARE">
</package>
<package name="CONN_BREAKAWAY_1X1_100_ROUND">
</package>
<package name="0603">
</package>
<package name="SOT23-5">
</package>
<package name="TRIMPOT_BOURNS_3296">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="1" library="kd0gls" package="CONN_BREAKAWAY_1X1_100_SQUARE" value="CONN_BREAKAWAY_1X1_100_SQUARE"/>
<element name="2" library="kd0gls" package="CONN_BREAKAWAY_1X1_100_ROUND" value="CONN_BREAKAWAY_1X1_100_ROUND"/>
<element name="3" library="kd0gls" package="CONN_BREAKAWAY_1X1_100_ROUND" value="CONN_BREAKAWAY_1X1_100_ROUND"/>
<element name="4" library="kd0gls" package="CONN_BREAKAWAY_1X1_100_ROUND" value="CONN_BREAKAWAY_1X1_100_ROUND"/>
<element name="C1" library="kd0gls" package="0603" value="0.1uF"/>
<element name="U1" library="kd0gls" package="SOT23-5" value="LTC1799"/>
<element name="R1" library="kd0gls" package="0603" value="3K"/>
<element name="VR2" library="kd0gls" package="TRIMPOT_BOURNS_3296" value="10K"/>
<element name="VR1" library="kd0gls" package="TRIMPOT_BOURNS_3296" value="1M"/>
</elements>
<signals>
<signal name="GND">
<contactref element="2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="DIV">
<contactref element="U1" pad="4"/>
<contactref element="1" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="U1" pad="5"/>
<contactref element="3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="3"/>
<contactref element="VR1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="4" pad="1"/>
<contactref element="VR2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="VR2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="VR1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
