(kicad_pcb (version 20171130) (host pcbnew 5.1.5-5.1.5)
  (general
    (thickness 1.6)
    (drawings 27)
    (tracks 95)
    (zones 0)
    (modules 18)
    (nets 15)
  )
  (page USLetter)
  (title_block
    (title "5v to 12v booster")
    (date 2020-01-02)
    (rev 1.2.4)
    (company "Copyright © 2018 by Aaron Williams")
    (comment 1 "5V to 12V boost converter")
    (comment 2 "Limited to 400ma")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.56)
    (via_drill 0.3)
    (via_min_size 0.3)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 0.8 0.8)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 "Net-(C7-Pad1)")
  (net 4 +5V)
  (net 5 "Net-(U1-Pad5)")
  (net 6 "Net-(U1-Pad10)")
  (net 7 "Net-(U1-Pad14)")
  (net 8 /SW)
  (net 9 /FET_CTL)
  (net 10 /FET_DRV)
  (net 11 /FB)
  (net 12 /COMP)
  (net 13 /FREQ)
  (net 14 /SS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.56)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /COMP)
    (add_net /FB)
    (add_net /FET_CTL)
    (add_net /FET_DRV)
    (add_net /FREQ)
    (add_net /SS)
    (add_net /SW)
    (add_net GND)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad5)")
  )
  (net_class 12V ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.56)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
  )
  (net_class 5V ""
    (clearance 0.2)
    (trace_width 0.8)
    (via_dia 0.56)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 113.6 79.44 180)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 4.385 -2.27 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 4.385 7.35 180) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /FET_CTL))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 132.8 72.9)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 4.385 -2.27) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 4.385 9.89) (layer F.Fab))
    (fp_text user %R (at 2.77 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /FET_DRV))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aaron:QFN-16-1EP_3x3mm_P0.5mm_EP2.7x2.7mm_ThermalVias (layer F.Cu) (tedit 5BCD8F8B)
    (at 120.9 76.15 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at -2.45 -1.4) (layer F.SilkS))
    (fp_text value TPS55340-Q1 (at 0 2.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at 0.5 0.5 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at -0.5 0.5 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at -0.5 -0.5 270) (size 0.73 0.73) (layers F.Paste))
    (pad 17 thru_hole circle (at -0.5 0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 17 thru_hole circle (at 0.5 0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 17 thru_hole circle (at 0.5 -0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 17 thru_hole circle (at -0.5 -0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad "" smd rect (at 0.5 -0.5 270) (size 0.73 0.73) (layers F.Paste))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers B.Cu)
      (net 2 GND))
    (pad 16 smd oval (at -0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /SW))
    (pad 15 smd oval (at -0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /SW))
    (pad 14 smd oval (at 0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad14)"))
    (pad 13 smd oval (at 0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad10)"))
    (pad 9 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /FREQ))
    (pad 8 smd oval (at 0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /FB))
    (pad 7 smd oval (at 0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /COMP))
    (pad 6 smd oval (at -0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd oval (at -0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad5)"))
    (pad 4 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /SS))
    (pad 3 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /SW))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP2.7x2.7mm_ThermalVias.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/aaronw/kicad/library/git-old/kicad-library/modules/packages3d/Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 5BCD8F81)
    (at 128.8 73.1 180)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at 2.8 1 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905 180) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 /SW))
    (pad 1 smd rect (at -1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aaron:L_Vishay_IHLP-1212 (layer F.Cu) (tedit 5BC76786)
    (at 124.8 74.7 270)
    (descr "Inductor, Vishay, IHLP series, 3.0mmx3.0mm")
    (tags "inductor vishay ihlp smd")
    (attr smd)
    (fp_text reference L1 (at -2.3 1.6) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 3.024 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /SW))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Vishay_IHLP-1212.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/aaronw/kicad/library/aaron/packages3d/IND_IHLP-1212BZ.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer F.Cu) (tedit 5A02FF57)
    (at 128.3 80.2)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q1 (at 1.5 1) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /FET_DRV))
    (pad 2 smd rect (at -1 0.65 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.65 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /FET_CTL))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.6 79.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -1.7 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /FET_CTL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117.2125 79.7)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.0125 -0.6) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117.9 77.4125 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.5875 2.8) (layer F.SilkS))
    (fp_text value 820pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /COMP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117.3125 75.2 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.0625 0.05 180) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /SS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.8 78.7 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 1.9 0.17) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120 73.1 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.1 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117 73.1)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -0.0375 -1.1) (layer F.SilkS))
    (fp_text value 6.8uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.2 76.6 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0.18 -2.12 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 2.28 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.45 79.8 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.7 0.05) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /FB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.4 77.4875 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0.2875 -1.3 180) (layer F.SilkS))
    (fp_text value 1.69k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /COMP))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121 79.8125 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 1.6875 0) (layer F.SilkS))
    (fp_text value 18.2k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /FREQ))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.2 78.7125 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.2875 -0.27 180) (layer F.SilkS))
    (fp_text value 86.6k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /FB))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Input: 4.5-5.5V" (at 124.62 73.15) (layer B.SilkS))
  (gr_text "Output: 12V, 0.5A" (at 124.1 74.72) (layer B.SilkS))
  (gr_text "Version 1.2.4" (at 126.76 76.31) (layer B.SilkS))
  (gr_text FET- (at 131.28 80.23 90) (layer F.SilkS))
  (gr_text G (at 131.2 78.01) (layer F.SilkS))
  (gr_text +12 (at 130.42 74.7) (layer F.SilkS))
  (gr_text "FET Ctl" (at 117.05 81.1) (layer F.SilkS))
  (gr_text G (at 115.2 76.3) (layer F.SilkS))
  (gr_text +5 (at 113.6 72.85) (layer F.SilkS))
  (gr_text "Copyright © 2018\nby Aaron Williams" (at 123.95 78.76) (layer B.SilkS))
  (gr_line (start 112.2 81.8) (end 112.2 71.5) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 134.1 81.8) (end 112.2 81.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 134.1 71.5) (end 134.1 81.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 112.2 71.5) (end 134.1 71.5) (layer Edge.Cuts) (width 0.2))
  (zone (net 4) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 121.2 74.3) (xy 125.500581 74.300581) (xy 125.5 71) (xy 111 71) (xy 111 75.4)
        (xy 114.1 75.4) (xy 115.2 74.3)
      )
    )
  )
  (zone (net 1) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.4 71.7) (xy 125.4 74) (xy 123.6 74) (xy 123.6 76.9) (xy 128.6 76.9)
        (xy 134 76.9) (xy 134 74.5) (xy 133.8 74.5) (xy 133.8 71.7)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111 71) (xy 110.9 82.6) (xy 134 82.7) (xy 134.1 71.1)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111 75.6) (xy 114.3 75.6) (xy 115.6 74.3) (xy 115.6 73.6) (xy 115.6 72.9)
        (xy 118.7 72.9) (xy 118.9 72.7) (xy 118.9 75.3) (xy 121.6 75.3) (xy 121.8 75.5)
        (xy 121.8 76.8) (xy 134 76.8) (xy 133.9 81.8) (xy 110.9 81.8)
      )
    )
  )
  (zone (net 4) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.6 75.4) (xy 113.7 75.4) (xy 116.1 73) (xy 116.6 73) (xy 119.4 73)
        (xy 120.1 73.7) (xy 121.1 73.7) (xy 123.3 73.7) (xy 123.3 71) (xy 111 71)
        (xy 111 75.4)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.1 72.7) (xy 119 72.7) (xy 119 75.9) (xy 116.1 75.9)
      )
    )
  )
  (zone (net 8) (net_name /SW) (layer F.Cu) (hatch full 0.508)
    (priority 8)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.4 74.3) (xy 125.4 74.3) (xy 125.4 76.9) (xy 123.8 76.9) (xy 123 76.1)
        (xy 122.3 76.1) (xy 122.3 75.2) (xy 121.4 75.2)
      )
    )
  )
)
