(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 8)
    (no_connects 0)
    (area 141.674999 94.424999 160.075001 110.575001)
    (thickness 1.6)
    (drawings 7)
    (tracks 0)
    (zones 0)
    (modules 7)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.11)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U2-Pad5)")
  (net 3 "Net-(U1-Pad7)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad5)")
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58DE9E67)
    (at 165.3 92.3)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad "" np_thru_hole circle (at -14.25 3) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm_h7.3mm (layer F.Cu) (tedit 58DE9B01)
    (at 153.5 107 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=7.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference UP (at -2.5 2.5 180) (layer F.SilkS))
    (fp_text value UP (at -2.5 2.5 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)") (solder_mask_margin -0.1))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad7)") (solder_mask_margin -0.1))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)") (solder_mask_margin -0.1))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad7)") (solder_mask_margin -0.1))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h7.3mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm_h7.3mm (layer F.Cu) (tedit 58DE9B10)
    (at 144 107 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=7.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference DOWN (at -2.5 2 180) (layer F.SilkS))
    (fp_text value DOWN (at -2.5 2 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad7)") (solder_mask_margin -0.1))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(U2-Pad5)") (solder_mask_margin -0.1))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad7)") (solder_mask_margin -0.1))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(U2-Pad5)") (solder_mask_margin -0.1))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h7.3mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58DE9AC4)
    (at 145 97)
    (fp_text reference PD (at 0 2) (layer F.SilkS))
    (fp_text value PD (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 "Net-(U2-Pad5)") (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58DE9AD2)
    (at 157 97)
    (fp_text reference PU (at 0 2) (layer F.SilkS))
    (fp_text value PU (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)") (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58DE9ACC)
    (at 151 97.5)
    (fp_text reference GND (at 0 2) (layer F.SilkS))
    (fp_text value GND (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad7)") (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58DE9E58)
    (at 151 109.7)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (gr_text "Potard \n" (at 150.5 109.25) (layer B.SilkS))
  (gr_text "SmartPWM V3" (at 151 103.25) (layer B.SilkS))
  (gr_text "SUYATOX\n" (at 151 98.25) (layer B.SilkS))
  (gr_line (start 160 110.5) (end 160 94.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.75 110.5) (end 160 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.75 94.5) (end 141.75 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160 94.5) (end 141.75 94.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(U2-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.11))
    (min_thickness 0.11)
    (fill yes (arc_segments 16) (thermal_gap 0.11) (thermal_bridge_width 0.123))
    (polygon
      (pts
        (xy 148.75 97) (xy 145.5 98.25) (xy 145.5 110.5) (xy 141.75 110.5) (xy 141.75 94.5)
        (xy 148.75 94.5)
      )
    )
  )
  (zone (net 3) (net_name "Net-(U1-Pad7)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.11))
    (min_thickness 0.11)
    (fill yes (arc_segments 16) (thermal_gap 0.11) (thermal_bridge_width 0.123))
    (polygon
      (pts
        (xy 152.5 98.5) (xy 155 99.5) (xy 155 110.5) (xy 147 110.5) (xy 147 99.25)
        (xy 149.5 98.5) (xy 149.5 94.5) (xy 152.5 94.5)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.11))
    (min_thickness 0.11)
    (fill yes (arc_segments 16) (thermal_gap 0.11) (thermal_bridge_width 0.123))
    (polygon
      (pts
        (xy 160 110.5) (xy 156.5 110.5) (xy 156.5 98.5) (xy 153.25 97) (xy 153.25 94.5)
        (xy 160 94.5)
      )
    )
  )
  (zone (net 2) (net_name "Net-(U2-Pad5)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.11))
    (min_thickness 0.11)
    (fill yes (arc_segments 16) (thermal_gap 0.11) (thermal_bridge_width 0.123))
    (polygon
      (pts
        (xy 148.75 97) (xy 145.5 98.25) (xy 145.5 110.5) (xy 141.75 110.5) (xy 141.75 94.5)
        (xy 148.75 94.5)
      )
    )
  )
  (zone (net 3) (net_name "Net-(U1-Pad7)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.11))
    (min_thickness 0.11)
    (fill yes (arc_segments 16) (thermal_gap 0.11) (thermal_bridge_width 0.123))
    (polygon
      (pts
        (xy 152.5 98.5) (xy 155 99.5) (xy 155 110.5) (xy 147 110.5) (xy 147 99.25)
        (xy 149.5 98.5) (xy 149.5 94.5) (xy 152.5 94.5)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.11))
    (min_thickness 0.11)
    (fill yes (arc_segments 16) (thermal_gap 0.11) (thermal_bridge_width 0.123))
    (polygon
      (pts
        (xy 160 110.5) (xy 156.5 110.5) (xy 156.5 98.5) (xy 153.25 97) (xy 153.25 94.5)
        (xy 160 94.5)
      )
    )
  )
)
