(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 221)
    (zones 0)
    (modules 30)
    (nets 59)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1)
    (edge_width 0.2)
    (via_size 0.889)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.889)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 104.521 139.319)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x000f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "D:/Users/Jacob/Documents/Repo/Adapters/soic multi adapter/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "Net-(J1-Pad13)")
  (net 14 "Net-(J1-Pad14)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 "Net-(J1-Pad16)")
  (net 17 "Net-(J1-Pad17)")
  (net 18 "Net-(J1-Pad18)")
  (net 19 "Net-(J1-Pad19)")
  (net 20 "Net-(J1-Pad20)")
  (net 21 "Net-(J1-Pad21)")
  (net 22 "Net-(J1-Pad22)")
  (net 23 "Net-(J2-Pad23)")
  (net 24 "Net-(J2-Pad24)")
  (net 25 "Net-(J2-Pad25)")
  (net 26 "Net-(J2-Pad26)")
  (net 27 "Net-(J2-Pad27)")
  (net 28 "Net-(J2-Pad28)")
  (net 29 "Net-(J2-Pad29)")
  (net 30 "Net-(J2-Pad30)")
  (net 31 "Net-(J2-Pad31)")
  (net 32 "Net-(J2-Pad32)")
  (net 33 "Net-(J2-Pad33)")
  (net 34 "Net-(J2-Pad34)")
  (net 35 "Net-(J2-Pad35)")
  (net 36 "Net-(J2-Pad36)")
  (net 37 "Net-(J2-Pad37)")
  (net 38 "Net-(J2-Pad38)")
  (net 39 "Net-(J2-Pad39)")
  (net 40 "Net-(J2-Pad40)")
  (net 41 "Net-(J2-Pad41)")
  (net 42 "Net-(J2-Pad42)")
  (net 43 "Net-(J2-Pad43)")
  (net 44 "Net-(J2-Pad44)")
  (net 45 "Net-(J4-Pad1)")
  (net 46 "Net-(J4-Pad2)")
  (net 47 "Net-(J4-Pad3)")
  (net 48 "Net-(J4-Pad4)")
  (net 49 "Net-(J5-Pad5)")
  (net 50 "Net-(J5-Pad6)")
  (net 51 "Net-(J5-Pad7)")
  (net 52 "Net-(J5-Pad8)")
  (net 53 "Net-(J7-Pad1)")
  (net 54 "Net-(J7-Pad2)")
  (net 55 "Net-(J7-Pad3)")
  (net 56 "Net-(J8-Pad4)")
  (net 57 "Net-(J8-Pad5)")
  (net 58 "Net-(J8-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.254)
    (uvia_dia 0.889)
    (uvia_drill 0.254)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad35)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad37)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad39)")
    (add_net "Net-(J2-Pad40)")
    (add_net "Net-(J2-Pad41)")
    (add_net "Net-(J2-Pad42)")
    (add_net "Net-(J2-Pad43)")
    (add_net "Net-(J2-Pad44)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J8-Pad5)")
    (add_net "Net-(J8-Pad6)")
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 171.704 125.603)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module IPC_HDR:HDRV4W64P254_4X1_1016X254H1062 (layer F.Cu) (tedit 5C899AA8)
    (at 170.688 137.16)
    (descr "Header, Vertical, 2.54 mm pitch; 0.64 mm lead width, 4 pins, 1 row, 4 pins per row, 10.16 mm L X 2.54 mm W X 10.62 mm H body")
    (fp_text reference J4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 3.81 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 48 "Net-(J4-Pad4)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at -1.27 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 46 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 45 "Net-(J4-Pad1)"))
  )
  (module IPC_HDR:HDRV4W64P254_4X1_1016X254H1062 (layer F.Cu) (tedit 5C899B12)
    (at 170.688 128.016 180)
    (descr "Header, Vertical, 2.54 mm pitch; 0.64 mm lead width, 4 pins, 1 row, 4 pins per row, 10.16 mm L X 2.54 mm W X 10.62 mm H body")
    (fp_text reference J6 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 3.81 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 52 "Net-(J5-Pad8)"))
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 51 "Net-(J5-Pad7)"))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad6)"))
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 49 "Net-(J5-Pad5)"))
  )
  (module IPC_HDR:HDRV3W64P254_3X1_762X254H1062 (layer F.Cu) (tedit 5C899963)
    (at 170.688 118.364)
    (descr "Header, Vertical, 2.54 mm pitch; 0.64 mm lead width, 3 pins, 1 row, 3 pins per row, 7.62 mm L X 2.54 mm W X 10.62 mm H body")
    (fp_text reference J7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 2.54 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 55 "Net-(J7-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 54 "Net-(J7-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 53 "Net-(J7-Pad1)"))
  )
  (module IPC_HDR:HDRV3W64P254_3X1_762X254H1062 (layer F.Cu) (tedit 5C8998F1)
    (at 170.688 109.22 180)
    (descr "Header, Vertical, 2.54 mm pitch; 0.64 mm lead width, 3 pins, 1 row, 3 pins per row, 7.62 mm L X 2.54 mm W X 10.62 mm H body")
    (fp_text reference J9 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 58 "Net-(J8-Pad6)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 57 "Net-(J8-Pad5)"))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 56 "Net-(J8-Pad4)"))
  )
  (module IPC_HDR:HDRV22W64P254_22X1_5588X254H1062 (layer F.Cu) (tedit 5C8997FB)
    (at 133.35 137.16)
    (descr "Header, Vertical, 2.54 mm pitch; 0.64 mm lead width, 22 pins, 1 row, 22 pins per row, 55.88 mm L X 2.54 mm W X 10.62 mm H body")
    (fp_text reference J1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Conn_01x22_Male (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 22 thru_hole circle (at 26.67 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad22)"))
    (pad 21 thru_hole circle (at 24.13 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 21.59 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 19.05 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad19)"))
    (pad 18 thru_hole circle (at 16.51 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 13.97 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad17)"))
    (pad 16 thru_hole circle (at 11.43 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 15 thru_hole circle (at 8.89 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 14 thru_hole circle (at 6.35 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 13 thru_hole circle (at 3.81 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 12 thru_hole circle (at 1.27 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 11 thru_hole circle (at -1.27 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 10 thru_hole circle (at -3.81 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 thru_hole circle (at -6.35 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 8 thru_hole circle (at -8.89 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at -11.43 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 6 thru_hole circle (at -13.97 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at -16.51 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at -19.05 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at -21.59 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -24.13 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at -26.67 0) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module IPC_HDR:HDRV22W64P254_22X1_5588X254H1062 (layer F.Cu) (tedit 5C899797)
    (at 133.35 109.22 180)
    (descr "Header, Vertical, 2.54 mm pitch; 0.64 mm lead width, 22 pins, 1 row, 22 pins per row, 55.88 mm L X 2.54 mm W X 10.62 mm H body")
    (fp_text reference J3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x22_Male (at 0 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 22 thru_hole circle (at 26.67 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad44)"))
    (pad 21 thru_hole circle (at 24.13 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 43 "Net-(J2-Pad43)"))
    (pad 20 thru_hole circle (at 21.59 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 42 "Net-(J2-Pad42)"))
    (pad 19 thru_hole circle (at 19.05 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad41)"))
    (pad 18 thru_hole circle (at 16.51 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad40)"))
    (pad 17 thru_hole circle (at 13.97 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad39)"))
    (pad 16 thru_hole circle (at 11.43 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad38)"))
    (pad 15 thru_hole circle (at 8.89 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad37)"))
    (pad 14 thru_hole circle (at 6.35 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad36)"))
    (pad 13 thru_hole circle (at 3.81 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad35)"))
    (pad 12 thru_hole circle (at 1.27 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad34)"))
    (pad 11 thru_hole circle (at -1.27 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad33)"))
    (pad 10 thru_hole circle (at -3.81 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad32)"))
    (pad 9 thru_hole circle (at -6.35 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad31)"))
    (pad 8 thru_hole circle (at -8.89 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad30)"))
    (pad 7 thru_hole circle (at -11.43 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad29)"))
    (pad 6 thru_hole circle (at -13.97 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad28)"))
    (pad 5 thru_hole circle (at -16.51 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad27)"))
    (pad 4 thru_hole circle (at -19.05 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad26)"))
    (pad 3 thru_hole circle (at -21.59 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad25)"))
    (pad 2 thru_hole circle (at -24.13 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad24)"))
    (pad 1 thru_hole rect (at -26.67 0 180) (size 1.59 1.59) (drill 1.06) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad23)"))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 164.465 132.588)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 164.465 133.604)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 162.433 133.604)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 162.433 132.588)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 162.433 131.572)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 164.465 131.572)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 170.688 125.603)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 169.672 125.603)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 171.704 120.777)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 170.688 120.777)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 169.672 120.777)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 164.465 114.808)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 164.465 113.792)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 164.465 112.776)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 162.433 114.808)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 162.433 113.792)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module IPC_SOIC127P:SOIC44P127_2850X1603X300L76X43N_Special (layer F.Cu) (tedit 5C81B6B0)
    (at 133.35 123.19)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_02x22_Top_Bottom (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -13.335 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -12.065 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -10.795 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -9.525 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -8.255 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -6.985 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -5.715 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at -4.445 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at -3.175 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 smd rect (at -1.905 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at -0.635 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 12 smd rect (at 0.635 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 13 smd rect (at 1.905 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 14 smd rect (at 3.175 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 15 smd rect (at 4.445 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 16 smd rect (at 5.715 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 17 smd rect (at 6.985 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad17)"))
    (pad 18 smd rect (at 8.225 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad18)"))
    (pad 19 smd rect (at 9.525 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad19)"))
    (pad 20 smd rect (at 10.795 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad20)"))
    (pad 21 smd rect (at 12.065 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-Pad21)"))
    (pad 22 smd rect (at 13.335 5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-Pad22)"))
    (pad 23 smd rect (at 13.335 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad23)"))
    (pad 24 smd rect (at 12.065 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J2-Pad24)"))
    (pad 25 smd rect (at 10.795 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J2-Pad25)"))
    (pad 26 smd rect (at 9.525 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-Pad26)"))
    (pad 27 smd rect (at 8.255 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J2-Pad27)"))
    (pad 28 smd rect (at 6.985 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J2-Pad28)"))
    (pad 29 smd rect (at 5.715 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-Pad29)"))
    (pad 30 smd rect (at 4.445 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J2-Pad30)"))
    (pad 31 smd rect (at 3.175 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J2-Pad31)"))
    (pad 32 smd rect (at 1.905 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J2-Pad32)"))
    (pad 33 smd rect (at 0.635 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J2-Pad33)"))
    (pad 34 smd rect (at -0.635 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J2-Pad34)"))
    (pad 35 smd rect (at -1.905 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad35)"))
    (pad 36 smd rect (at -3.175 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J2-Pad36)"))
    (pad 37 smd rect (at -4.445 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J2-Pad37)"))
    (pad 38 smd rect (at -5.715 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J2-Pad38)"))
    (pad 39 smd rect (at -6.985 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J2-Pad39)"))
    (pad 40 smd rect (at -8.255 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J2-Pad40)"))
    (pad 41 smd rect (at -9.525 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J2-Pad41)"))
    (pad 42 smd rect (at -10.795 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J2-Pad42)"))
    (pad 43 smd rect (at -12.065 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J2-Pad43)"))
    (pad 44 smd rect (at -13.335 -5.1075) (size 0.6 7.215) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J2-Pad44)"))
  )
  (module IPC_SOT:SOT23-8P65_280X145L45X30N (layer F.Cu) (tedit 5C81EDB5)
    (at 170.688 132.588)
    (descr "Small Outline Transistor (SOT23), 0.65 mm pitch; 8 pin, 2.90 mm L X 1.60 mm W X 1.45 mm H body")
    (attr smd)
    (fp_text reference J5 (at 0 0) (layer F.Fab) hide)
    (fp_text value Conn_02x04_Top_Bottom (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.975 1.205 90) (size 1.11 0.46) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at -0.325 1.205 90) (size 1.11 0.46) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J4-Pad2)"))
    (pad 3 smd rect (at 0.325 1.205 90) (size 1.11 0.46) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J4-Pad3)"))
    (pad 4 smd rect (at 0.975 1.205 90) (size 1.11 0.46) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J4-Pad4)"))
    (pad 5 smd rect (at 0.975 -1.205 90) (size 1.11 0.46) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J5-Pad5)"))
    (pad 6 smd rect (at 0.325 -1.205 90) (size 1.11 0.46) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J5-Pad6)"))
    (pad 7 smd rect (at -0.325 -1.205 90) (size 1.11 0.46) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J5-Pad7)"))
    (pad 8 smd rect (at -0.975 -1.205 90) (size 1.11 0.46) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J5-Pad8)"))
  )
  (module IPC_SOT:SOT23-6P95_280X145L45X37N (layer F.Cu) (tedit 5C81F105)
    (at 170.688 113.792)
    (descr "Small Outline Transistor (SOT23), 0.95 mm pitch; 6 pin, 2.90 mm L X 1.60 mm W X 1.45 mm H body")
    (attr smd)
    (fp_text reference J8 (at 0 0) (layer F.Fab) hide)
    (fp_text value Conn_02x03_Top_Bottom (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 1.23 90) (size 1.16 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J7-Pad1)"))
    (pad 2 smd rect (at 0 1.23 90) (size 1.16 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J7-Pad2)"))
    (pad 3 smd rect (at 0.95 1.23 90) (size 1.16 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J7-Pad3)"))
    (pad 4 smd rect (at 0.95 -1.23 90) (size 1.16 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J8-Pad4)"))
    (pad 5 smd rect (at 0 -1.23 90) (size 1.16 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J8-Pad5)"))
    (pad 6 smd rect (at -0.95 -1.23 90) (size 1.16 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J8-Pad6)"))
  )
  (module MTG:MTGNP79H79 (layer F.Cu) (tedit 5C82DE20)
    (at 162.433 112.776)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MTGNPxxxxH25 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.7874 0.7874) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 154.94 123.19 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 170.688 113.792 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 170.688 132.588 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_line (start 171.958 125.857) (end 169.418 125.857) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 171.958 120.523) (end 171.958 125.857) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 169.418 120.523) (end 171.958 120.523) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 169.418 125.857) (end 169.418 120.523) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 162.179 131.318) (end 162.179 133.858) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.719 131.318) (end 162.179 131.318) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.719 133.858) (end 164.719 131.318) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 162.179 133.858) (end 164.719 133.858) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 162.179 115.062) (end 162.179 112.522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.719 115.062) (end 162.179 115.062) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.719 112.522) (end 164.719 115.062) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.179 112.522) (end 164.719 112.522) (layer Edge.Cuts) (width 0.1))
  (gr_text SOT23-6 (at 165.862 113.792 90) (layer F.SilkS))
  (gr_text SOT23-8 (at 165.862 132.588 90) (layer F.SilkS))
  (gr_line (start 176.657 107.061) (end 176.657 120.523) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.719 120.523) (end 164.719 107.061) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.719 120.523) (end 176.657 120.523) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 176.657 107.061) (end 164.719 107.061) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.719 125.857) (end 164.719 139.319) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 176.657 125.857) (end 164.719 125.857) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 176.657 139.319) (end 176.657 125.857) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.719 139.319) (end 176.657 139.319) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_text "150 MIL TO 525 MIL" (at 111.125 123.19 90) (layer F.SilkS))
  (gr_text SOIC44P127 (at 108.712 123.19 90) (layer F.SilkS))
  (gr_text "ADAPTER\n" (at 106.299 123.19 90) (layer F.SilkS))
  (gr_line (start 162.179 107.061) (end 162.179 139.319) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.521 107.061) (end 162.179 107.061) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.521 139.319) (end 104.521 107.061) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.179 139.319) (end 104.521 139.319) (angle 90) (layer Edge.Cuts) (width 0.15))
)
