(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 40)
    (tracks 157)
    (zones 0)
    (modules 28)
    (nets 26)
  )
  (page A4)
  (title_block
    (title "PCB274-Quad Opto Isolators to level shift signals")
    (date "10Jan20. Keep vers ID consistent 1+3 places")
    (rev 1.1)
    (comment 3 "Quad optocoupler. I wanted for CCTV control-by-PIR work\\nStarted 12 Dec 19- Day Johnson took over UK")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.200001 3.200001)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(Din1-Pad1)")
  (net 2 "Net-(Din1-Pad2)")
  (net 3 "Net-(Din2-Pad1)")
  (net 4 "Net-(Din2-Pad2)")
  (net 5 "Net-(Din3-Pad2)")
  (net 6 "Net-(Din3-Pad1)")
  (net 7 "Net-(Din4-Pad2)")
  (net 8 "Net-(Din4-Pad1)")
  (net 9 "Net-(Dout1-Pad1)")
  (net 10 "Net-(Dout2-Pad1)")
  (net 11 "Net-(Dout3-Pad1)")
  (net 12 "Net-(Dout4-Pad1)")
  (net 13 GND)
  (net 14 GNDD)
  (net 15 "Net-(Jout1-Pad3)")
  (net 16 "Net-(Jout1-Pad4)")
  (net 17 "Net-(Jout2-Pad1)")
  (net 18 "Net-(Jout2-Pad2)")
  (net 19 "Net-(Jout2-Pad3)")
  (net 20 "Net-(Jout2-Pad4)")
  (net 21 "Net-(Rin1-Pad1)")
  (net 22 "Net-(Rin2-Pad1)")
  (net 23 "Net-(Rin3-Pad1)")
  (net 24 "Net-(Rin4-Pad1)")
  (net 25 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net GNDD)
    (add_net "Net-(Din1-Pad1)")
    (add_net "Net-(Din1-Pad2)")
    (add_net "Net-(Din2-Pad1)")
    (add_net "Net-(Din2-Pad2)")
    (add_net "Net-(Din3-Pad1)")
    (add_net "Net-(Din3-Pad2)")
    (add_net "Net-(Din4-Pad1)")
    (add_net "Net-(Din4-Pad2)")
    (add_net "Net-(Dout1-Pad1)")
    (add_net "Net-(Dout2-Pad1)")
    (add_net "Net-(Dout3-Pad1)")
    (add_net "Net-(Dout4-Pad1)")
    (add_net "Net-(Jout1-Pad3)")
    (add_net "Net-(Jout1-Pad4)")
    (add_net "Net-(Jout2-Pad1)")
    (add_net "Net-(Jout2-Pad2)")
    (add_net "Net-(Jout2-Pad3)")
    (add_net "Net-(Jout2-Pad4)")
    (add_net "Net-(Rin1-Pad1)")
    (add_net "Net-(Rin2-Pad1)")
    (add_net "Net-(Rin3-Pad1)")
    (add_net "Net-(Rin4-Pad1)")
    (add_net VCC)
  )
  (module "aaTKB frm Jan2020:Camden_CTB3051-Rapid21-4707_1x04_P3.50mm" (layer F.Cu) (tedit 5E18B3AF)
    (at 157.5 137.2 270)
    (descr "Molex 734 Male header (for PCBs); Straight solder pin 1 x 1 mm, 734-134 , 4 Pins (http://www.farnell.com/datasheets/2157639.pdf), generated with kicad-footprint-generator")
    (tags "connector Wago  side entry")
    (fp_text reference Jin2 (at 12.827 2.413 180) (layer F.SilkS))
    (fp_text value ~ (at 5.6 -6.5 90) (layer F.Fab))
    (fp_text user %R (at 12.954 2.413 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 10.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 3 thru_hole oval (at 7 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 2 thru_hole oval (at 3.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 13 GND))
    (model ${KISYS3DMOD}/Connector_Wago.3dshapes/Wago_734-134_1x04_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 173.99 127)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at -0.39 -2.2) (layer F.SilkS))
    (fp_text value LTV-827 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at -0.889 -2.286) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(Jout1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 GNDD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(Rin2-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(Jout1-Pad4)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 GNDD))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(Rin1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 130.048 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference Din1 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value ~ (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(Din1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(Din1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 135.128 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference Din2 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value ~ (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(Din2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(Din2-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 143.51 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference Din3 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value ~ (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(Din3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(Din3-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 164.465 148.59 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference Din4 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value ~ (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(Din4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(Din4-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 185.928 128.905 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference Dout1 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(Dout1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 185.928 134.747 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference Dout2 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(Dout2-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 185.928 141.986 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference Dout3 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(Dout3-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 185.928 149.352 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference Dout4 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(Dout4-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 173.99 140.97)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 4.01 -1.97) (layer F.SilkS))
    (fp_text value LTV-827 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.286) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(Jout2-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 GNDD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(Rin4-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(Jout2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 GNDD))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(Rin3-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 189.484 129.54 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLout1 (at 1.778 1.905 90) (layer F.SilkS))
    (fp_text value R (at 1.27 1.92 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(Jout1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(Dout1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 171.577 127.508 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference Rin1 (at 1.905 1.016) (layer F.SilkS))
    (fp_text value ~ (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 1.778 -0.127) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(Din1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(Rin1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 189.484 135.636 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLout2 (at 1.778 1.905 90) (layer F.SilkS))
    (fp_text value R (at 1.27 1.92 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(Jout1-Pad4)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(Dout2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 190.119 142.748 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLout3 (at 1.905 1.778 90) (layer F.SilkS))
    (fp_text value R (at 1.27 1.92 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(Jout2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(Dout3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 187.706 144.399 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLout4 (at 1.905 -0.762) (layer F.SilkS) hide)
    (fp_text value R (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -1.92) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(Jout2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(Dout4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:Camden_CTB3051-Rapid21-4707_1x04_P3.50mm" (layer F.Cu) (tedit 5E18B3AF)
    (at 200.66 123.19 270)
    (descr "Molex 734 Male header (for PCBs); Straight solder pin 1 x 1 mm, 734-134 , 4 Pins (http://www.farnell.com/datasheets/2157639.pdf), generated with kicad-footprint-generator")
    (tags "connector Wago  side entry")
    (fp_text reference Jout1 (at -2.159 0.381 180) (layer F.SilkS))
    (fp_text value ~ (at 5.6 -6.5 90) (layer F.Fab))
    (fp_text user %R (at -2.032 0.381) (layer F.Fab))
    (pad 4 thru_hole oval (at 10.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 16 "Net-(Jout1-Pad4)"))
    (pad 3 thru_hole oval (at 7 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 15 "Net-(Jout1-Pad3)"))
    (pad 2 thru_hole oval (at 3.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 14 GNDD))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 25 VCC))
    (model ${KISYS3DMOD}/Connector_Wago.3dshapes/Wago_734-134_1x04_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:Camden_CTB3051-Rapid21-4707_1x04_P3.50mm" (layer F.Cu) (tedit 5E18B3AF)
    (at 200.66 137.16 270)
    (descr "Molex 734 Male header (for PCBs); Straight solder pin 1 x 1 mm, 734-134 , 4 Pins (http://www.farnell.com/datasheets/2157639.pdf), generated with kicad-footprint-generator")
    (tags "connector Wago  side entry")
    (fp_text reference Jout2 (at 12.7 0.127 180) (layer F.SilkS))
    (fp_text value ~ (at 5.6 -6.5 90) (layer F.Fab))
    (fp_text user %R (at 12.827 0.127 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 10.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 20 "Net-(Jout2-Pad4)"))
    (pad 3 thru_hole oval (at 7 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 19 "Net-(Jout2-Pad3)"))
    (pad 2 thru_hole oval (at 3.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 18 "Net-(Jout2-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 17 "Net-(Jout2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wago.3dshapes/Wago_734-134_1x04_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 171.577 132.588 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference Rin2 (at 2.032 0.889) (layer F.SilkS))
    (fp_text value ~ (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -0.381) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(Din2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(Rin2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 171.577 140.97 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference Rin3 (at 1.905 0.762) (layer F.SilkS))
    (fp_text value ~ (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -0.635) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(Rin3-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(Din3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 171.577 146.05 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference Rin4 (at 2.032 0.762) (layer F.SilkS))
    (fp_text value ~ (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 "Net-(Rin4-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(Din4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 167.894 130.048)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLin1 (at 1.905 -0.889) (layer F.SilkS))
    (fp_text value ~ (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 2.159 0.381) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(Din1-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 167.894 135.128)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLin2 (at 2.032 -0.889) (layer F.SilkS))
    (fp_text value ~ (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 2.286 0.381) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(Din2-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 167.894 143.51)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLin3 (at 1.905 -0.889) (layer F.SilkS))
    (fp_text value ~ (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 1.651 0.381) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(Din3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:R_1-8thW_Horiz-mod_of__Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm" (layer F.Cu) (tedit 5E18A2F4)
    (at 167.894 148.59)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLin4 (at 1.905 -1.016) (layer F.SilkS))
    (fp_text value ~ (at 1.27 1.92) (layer F.Fab) hide)
    (fp_text user %R (at 2.032 0.635) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(Din4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:TKB_MountingHole_3.2mm_M3" (layer F.Cu) (tedit 5E18BFD0)
    (at 167.132 122.809)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 0) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user ~ (at 0.05 -4.15) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "aaTKB frm Jan2020:TKB_MountingHole_3.2mm_M3" (layer F.Cu) (tedit 5E18BFD0)
    (at 192.532 148.209)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 0.127) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user ~ (at 0.05 -4.15) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "aaTKB frm Jan2020:Camden_CTB3051-Rapid21-4707_1x04_P3.50mm" (layer F.Cu) (tedit 5E18B3AF)
    (at 157.5 123.2 270)
    (descr "Molex 734 Male header (for PCBs); Straight solder pin 1 x 1 mm, 734-134 , 4 Pins (http://www.farnell.com/datasheets/2157639.pdf), generated with kicad-footprint-generator")
    (tags "connector Wago  side entry")
    (fp_text reference Jin1 (at -2.2 2.7 180) (layer F.SilkS))
    (fp_text value ~ (at 5.6 -6.5 90) (layer F.Fab))
    (fp_text user %R (at 9.6 5.35 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 2 "Net-(Din1-Pad2)"))
    (pad 2 thru_hole oval (at 3.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(Din2-Pad2)"))
    (pad 3 thru_hole oval (at 7 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 "Net-(Din3-Pad2)"))
    (pad 4 thru_hole oval (at 10.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 7 "Net-(Din4-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Wago.3dshapes/Wago_734-134_1x04_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "http://sheepdogguides.com/elec/\n     pcb/PCB274-quad-opto-coupler.htm" (at 193.04 134.112 -90) (layer B.SilkS))
  (gr_text "N.B.  Grounds linked **" (at 162.052 150.368) (layer B.SilkS))
  (gr_text http://SheepdogGuides.com (at 172.2 137.6) (layer F.SilkS))
  (gr_text Out1 (at 197.231 130.302) (layer B.SilkS))
  (gr_text Out2 (at 197.231 133.731) (layer B.SilkS))
  (gr_text Out3 (at 197.231 137.414) (layer B.SilkS))
  (gr_text Out4 (at 197.231 140.716) (layer B.SilkS))
  (gr_text n/c (at 197.358 144.145) (layer B.SilkS))
  (gr_text n/c (at 197.358 147.447) (layer B.SilkS))
  (gr_text Ch1 (at 154.432 123.19) (layer B.SilkS))
  (gr_text Ch2 (at 154.432 126.746) (layer B.SilkS))
  (gr_text Ch3 (at 154.432 130.175) (layer B.SilkS))
  (gr_text Ch4 (at 154.432 133.731) (layer B.SilkS))
  (gr_text 0vIn (at 154.178 137.1) (layer B.SilkS))
  (gr_text 0vIn (at 154.178 140.716) (layer B.SilkS))
  (gr_text 0vIn (at 154.178 144.145) (layer B.SilkS))
  (gr_text "ver 1.1 10 Jan 2020" (at 170.307 138.684) (layer B.SilkS))
  (gr_line (start 205.2 119.634) (end 205.2 151.257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.273 119.634) (end 205.2 119.634) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.273 151.257) (end 152.273 119.634) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 205.2 151.257) (end 152.273 151.257) (layer Edge.Cuts) (width 0.1))
  (gr_text SheepdogGuides.com (at 203.454 136.271 -90) (layer B.SilkS))
  (gr_text "TK Boyd started 12Dec19" (at 171.958 137.16) (layer B.SilkS))
  (gr_text 0vIn (at 154.178 147.701) (layer B.SilkS))
  (gr_text 0vOut (at 196.85 127) (layer B.SilkS))
  (gr_text Vcc (at 197.485 123.19) (layer B.SilkS))
  (gr_text "PCB274 v1.1" (at 194.2 134.6 90) (layer F.SilkS))
)
