(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 356)
    (no_connects 0)
    (area 35.919999 58.332143 270.315 144.232857)
    (thickness 1.6)
    (drawings 18)
    (tracks 722)
    (zones 0)
    (modules 146)
    (nets 82)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.4 6.4)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C17-Pad2)")
  (net 4 "Net-(C18-Pad2)")
  (net 5 "Net-(C19-Pad2)")
  (net 6 "Net-(C21-Pad2)")
  (net 7 "Net-(C22-Pad2)")
  (net 8 "Net-(C23-Pad2)")
  (net 9 "Net-(CON1-Pad1)")
  (net 10 "Net-(LED1-Pad4)")
  (net 11 "Net-(LED1-Pad2)")
  (net 12 "Net-(LED2-Pad4)")
  (net 13 "Net-(LED3-Pad4)")
  (net 14 "Net-(LED4-Pad4)")
  (net 15 "Net-(LED5-Pad4)")
  (net 16 "Net-(LED6-Pad4)")
  (net 17 "Net-(LED7-Pad4)")
  (net 18 "Net-(LED8-Pad4)")
  (net 19 "Net-(LED10-Pad2)")
  (net 20 "Net-(LED10-Pad4)")
  (net 21 "Net-(LED11-Pad4)")
  (net 22 "Net-(LED12-Pad4)")
  (net 23 "Net-(LED13-Pad4)")
  (net 24 "Net-(LED15-Pad4)")
  (net 25 "Net-(LED16-Pad4)")
  (net 26 "Net-(LED17-Pad4)")
  (net 27 "Net-(LED18-Pad4)")
  (net 28 "Net-(LED19-Pad4)")
  (net 29 "Net-(LED20-Pad4)")
  (net 30 "Net-(LED21-Pad4)")
  (net 31 "Net-(LED22-Pad4)")
  (net 32 "Net-(LED23-Pad4)")
  (net 33 "Net-(LED24-Pad4)")
  (net 34 "Net-(LED25-Pad4)")
  (net 35 "Net-(LED26-Pad4)")
  (net 36 "Net-(LED27-Pad4)")
  (net 37 "Net-(LED28-Pad4)")
  (net 38 "Net-(LED31-Pad4)")
  (net 39 "Net-(LED32-Pad4)")
  (net 40 "Net-(LED33-Pad4)")
  (net 41 "Net-(LED34-Pad4)")
  (net 42 "Net-(LED35-Pad4)")
  (net 43 "Net-(LED36-Pad4)")
  (net 44 "Net-(LED37-Pad4)")
  (net 45 "Net-(LED38-Pad4)")
  (net 46 "Net-(LED39-Pad4)")
  (net 47 "Net-(LED40-Pad4)")
  (net 48 "Net-(LED41-Pad4)")
  (net 49 "Net-(LED42-Pad4)")
  (net 50 "Net-(LED43-Pad4)")
  (net 51 "Net-(LED45-Pad4)")
  (net 52 "Net-(LED46-Pad4)")
  (net 53 "Net-(LED47-Pad4)")
  (net 54 "Net-(LED48-Pad4)")
  (net 55 "Net-(LED49-Pad4)")
  (net 56 "Net-(LED50-Pad4)")
  (net 57 "Net-(LED51-Pad4)")
  (net 58 "Net-(LED52-Pad4)")
  (net 59 "Net-(LED53-Pad4)")
  (net 60 "Net-(LED54-Pad4)")
  (net 61 "Net-(LED55-Pad4)")
  (net 62 "Net-(LED56-Pad4)")
  (net 63 D2)
  (net 64 "Net-(P2-Pad3)")
  (net 65 "Net-(P2-Pad2)")
  (net 66 "Net-(P3-Pad3)")
  (net 67 "Net-(P3-Pad2)")
  (net 68 "Net-(P4-Pad3)")
  (net 69 "Net-(P4-Pad2)")
  (net 70 "Net-(P5-Pad1)")
  (net 71 "Net-(P5-Pad2)")
  (net 72 Tx)
  (net 73 Rx)
  (net 74 "Net-(P5-Pad6)")
  (net 75 RESET)
  (net 76 D0)
  (net 77 "Net-(LED14-Pad4)")
  (net 78 "Net-(LED29-Pad4)")
  (net 79 "Net-(LED30-Pad4)")
  (net 80 "Net-(LED44-Pad4)")
  (net 81 "Net-(LED57-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net D0)
    (add_net D2)
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED1-Pad4)")
    (add_net "Net-(LED10-Pad2)")
    (add_net "Net-(LED10-Pad4)")
    (add_net "Net-(LED11-Pad4)")
    (add_net "Net-(LED12-Pad4)")
    (add_net "Net-(LED13-Pad4)")
    (add_net "Net-(LED14-Pad4)")
    (add_net "Net-(LED15-Pad4)")
    (add_net "Net-(LED16-Pad4)")
    (add_net "Net-(LED17-Pad4)")
    (add_net "Net-(LED18-Pad4)")
    (add_net "Net-(LED19-Pad4)")
    (add_net "Net-(LED2-Pad4)")
    (add_net "Net-(LED20-Pad4)")
    (add_net "Net-(LED21-Pad4)")
    (add_net "Net-(LED22-Pad4)")
    (add_net "Net-(LED23-Pad4)")
    (add_net "Net-(LED24-Pad4)")
    (add_net "Net-(LED25-Pad4)")
    (add_net "Net-(LED26-Pad4)")
    (add_net "Net-(LED27-Pad4)")
    (add_net "Net-(LED28-Pad4)")
    (add_net "Net-(LED29-Pad4)")
    (add_net "Net-(LED3-Pad4)")
    (add_net "Net-(LED30-Pad4)")
    (add_net "Net-(LED31-Pad4)")
    (add_net "Net-(LED32-Pad4)")
    (add_net "Net-(LED33-Pad4)")
    (add_net "Net-(LED34-Pad4)")
    (add_net "Net-(LED35-Pad4)")
    (add_net "Net-(LED36-Pad4)")
    (add_net "Net-(LED37-Pad4)")
    (add_net "Net-(LED38-Pad4)")
    (add_net "Net-(LED39-Pad4)")
    (add_net "Net-(LED4-Pad4)")
    (add_net "Net-(LED40-Pad4)")
    (add_net "Net-(LED41-Pad4)")
    (add_net "Net-(LED42-Pad4)")
    (add_net "Net-(LED43-Pad4)")
    (add_net "Net-(LED44-Pad4)")
    (add_net "Net-(LED45-Pad4)")
    (add_net "Net-(LED46-Pad4)")
    (add_net "Net-(LED47-Pad4)")
    (add_net "Net-(LED48-Pad4)")
    (add_net "Net-(LED49-Pad4)")
    (add_net "Net-(LED5-Pad4)")
    (add_net "Net-(LED50-Pad4)")
    (add_net "Net-(LED51-Pad4)")
    (add_net "Net-(LED52-Pad4)")
    (add_net "Net-(LED53-Pad4)")
    (add_net "Net-(LED54-Pad4)")
    (add_net "Net-(LED55-Pad4)")
    (add_net "Net-(LED56-Pad4)")
    (add_net "Net-(LED57-Pad4)")
    (add_net "Net-(LED6-Pad4)")
    (add_net "Net-(LED7-Pad4)")
    (add_net "Net-(LED8-Pad4)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad6)")
    (add_net RESET)
    (add_net Rx)
    (add_net Tx)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(CON1-Pad1)")
  )
  (module Libraries:BuckBoostModules (layer B.Cu) (tedit 58DB4CAB)
    (at 83.82 79.375 270)
    (fp_text reference P1 (at 22.86 34.29 270) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 24.765 34.29 270) (layer B.Fab))
    (fp_text user OUT- (at 41.402 4.572 270) (layer B.SilkS))
    (fp_text user OUT+ (at 41.402 16.764 270) (layer B.SilkS))
    (fp_text user IN- (at 2.032 4.572 270) (layer B.SilkS))
    (fp_text user IN+ (at 2.032 16.764 270) (layer B.SilkS))
    (pad 1 thru_hole rect (at 1.778 19.558 270) (size 3.556 3.556) (drill 1.524) (layers *.Cu *.Mask)
      (net 9 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole rect (at 1.778 1.778 270) (size 3.556 3.556) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at 41.656 19.558 270) (size 3.556 3.556) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 41.656 1.778 270) (size 3.556 3.556) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 6.604 18.796 270) (size 4.826 4.826) (drill 3.175) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 36.83 2.54 270) (size 4.826 4.826) (drill 3.175) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58DB47DA)
    (at 114.935 93.345)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -2.54 -17.78) (layer F.SilkS))
    (fp_text value .1uF (at -1.905 -17.78) (layer F.Fab))
    (fp_text user %R (at 0.635 -17.145) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58DB47EC)
    (at 114.935 102.235)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -1.27 -26.67) (layer F.SilkS))
    (fp_text value .1uF (at -1.27 -26.67) (layer F.Fab))
    (fp_text user %R (at -3.81 -26.035) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58DB47E9)
    (at 114.935 99.695)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -3.81 -24.13) (layer F.SilkS))
    (fp_text value .1uF (at 1.27 -24.765) (layer F.Fab))
    (fp_text user %R (at -1.27 -23.495) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58DB47D7)
    (at 114.935 90.805)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -1.27 -15.24) (layer F.SilkS))
    (fp_text value .1uF (at -3.175 -15.24) (layer F.Fab))
    (fp_text user %R (at -0.635 -14.605) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BAE)
    (at 250.19 95.25 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -0.635 -15.24 270) (layer B.SilkS))
    (fp_text value .1uF (at -24.13 1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4B40)
    (at 250.19 106.68 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -0.635 -14.605 270) (layer B.SilkS))
    (fp_text value .1uF (at -0.635 -10.795 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A9A)
    (at 219.71 113.03 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 14.605 1.905 270) (layer B.SilkS))
    (fp_text value .1uF (at 15.24 -3.175 270) (layer B.Fab))
    (fp_text user %R (at 14.605 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB49B7)
    (at 208.915 85.725)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at -0.635 -13.335) (layer B.SilkS))
    (fp_text value .1uF (at -1.905 -12.065) (layer B.Fab))
    (fp_text user %R (at -2.54 -12.7) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A49)
    (at 208.915 121.285)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0.635 10.16) (layer B.SilkS))
    (fp_text value .1uF (at 0 10.795) (layer B.Fab))
    (fp_text user %R (at 0 8.89) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A09)
    (at 179.07 113.03 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 17.145 0 270) (layer B.SilkS))
    (fp_text value .1uF (at 15.24 -7.62 270) (layer B.Fab))
    (fp_text user %R (at 19.685 -0.635 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A14)
    (at 168.275 121.285)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 1.27 7.62) (layer B.SilkS))
    (fp_text value .1uF (at 0.635 7.62) (layer B.Fab))
    (fp_text user %R (at 0 6.35) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB49E0)
    (at 174.625 103.505)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at 0 -30.48) (layer B.SilkS))
    (fp_text value .1uF (at 0.635 -31.115) (layer B.Fab))
    (fp_text user %R (at -0.635 -29.21) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB49DB)
    (at 168.275 103.505)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at 0.635 -29.845) (layer B.SilkS))
    (fp_text value .1uF (at 0 -29.845) (layer B.Fab))
    (fp_text user %R (at 0.635 -29.21) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4AEB)
    (at 250.19 113.03 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at -0.635 -8.89 270) (layer B.SilkS))
    (fp_text value .1uF (at 3.81 -9.525 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -9.525 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BA7)
    (at 229.87 95.25 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at -22.225 2.54 270) (layer B.SilkS))
    (fp_text value .1uF (at -23.495 -1.905 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4B98)
    (at 215.265 85.725)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 1.905 -13.335) (layer B.SilkS))
    (fp_text value .1uF (at 0 -13.97) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A84)
    (at 215.265 103.505)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at 1.27 26.67) (layer B.SilkS))
    (fp_text value .1uF (at 4.445 24.765) (layer B.Fab))
    (fp_text user %R (at 3.175 24.765) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A39)
    (at 199.39 113.03 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 16.51 0 270) (layer B.SilkS))
    (fp_text value .1uF (at 17.145 -2.54 270) (layer B.Fab))
    (fp_text user %R (at 15.875 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB49EA)
    (at 179.07 106.68 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C19 (at -34.29 1.27 270) (layer B.SilkS))
    (fp_text value .1uF (at -33.02 -0.635 270) (layer B.Fab))
    (fp_text user %R (at -33.655 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C19-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A0E)
    (at 174.625 121.285)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C20 (at 1.905 10.16) (layer B.SilkS))
    (fp_text value .1uF (at 1.27 6.35) (layer B.Fab))
    (fp_text user %R (at 1.905 8.89) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BA6)
    (at 229.87 88.9 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C21 (at -15.875 3.175 270) (layer B.SilkS))
    (fp_text value .1uF (at -18.415 -3.175 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C21-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4AC2)
    (at 229.87 106.68 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C22 (at 24.13 -0.635 270) (layer B.SilkS))
    (fp_text value .1uF (at 20.955 -5.715 270) (layer B.Fab))
    (fp_text user %R (at 24.765 -0.635 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C22-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4AA0)
    (at 219.71 106.68 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C23 (at 22.86 0.635 270) (layer B.SilkS))
    (fp_text value .1uF (at 22.86 -2.54 270) (layer B.Fab))
    (fp_text user %R (at 23.495 -2.54 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C23-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A65)
    (at 208.915 103.505)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C24 (at 0 27.94) (layer B.SilkS))
    (fp_text value .1uF (at -1.905 24.765) (layer B.Fab))
    (fp_text user %R (at -1.27 31.115) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB49A1)
    (at 199.39 88.9 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C25 (at -14.605 4.445 270) (layer B.SilkS))
    (fp_text value .1uF (at -14.605 -0.635 270) (layer B.Fab))
    (fp_text user %R (at -15.875 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4994)
    (at 189.23 92.075 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C26 (at -19.05 1.905 270) (layer B.SilkS))
    (fp_text value .1uF (at -18.415 -1.27 270) (layer B.Fab))
    (fp_text user %R (at -19.05 2.54 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB497A)
    (at 179.07 95.25 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C27 (at -20.32 0.635 270) (layer B.SilkS))
    (fp_text value .1uF (at -20.955 -3.81 270) (layer B.Fab))
    (fp_text user %R (at -19.685 -2.54 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4AB8)
    (at 229.87 113.03 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C28 (at 15.24 1.27 270) (layer B.SilkS))
    (fp_text value .1uF (at 16.51 -2.54 270) (layer B.Fab))
    (fp_text user %R (at 16.51 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4B9B)
    (at 219.71 88.9 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C29 (at -19.685 0 270) (layer B.SilkS))
    (fp_text value .1uF (at -19.05 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BA9)
    (at 219.71 95.25 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C30 (at -22.86 -0.635 270) (layer B.SilkS))
    (fp_text value .1uF (at -23.495 -3.81 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A53)
    (at 215.265 121.285)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C31 (at 1.27 8.89) (layer B.SilkS))
    (fp_text value .1uF (at 0.635 8.89) (layer B.Fab))
    (fp_text user %R (at 0.635 10.795) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB49AE)
    (at 199.39 95.25 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C32 (at -22.225 4.445 270) (layer B.SilkS))
    (fp_text value .1uF (at -22.225 -0.635 270) (layer B.Fab))
    (fp_text user %R (at -22.225 3.81 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A3E)
    (at 199.39 106.68 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C33 (at 21.59 2.54 270) (layer B.SilkS))
    (fp_text value .1uF (at 24.765 -1.905 270) (layer B.Fab))
    (fp_text user %R (at 21.59 0.635 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4A27)
    (at 189.23 109.22 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C34 (at 19.05 3.81 270) (layer B.SilkS))
    (fp_text value .1uF (at 19.685 -3.175 270) (layer B.Fab))
    (fp_text user %R (at 18.415 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB495E)
    (at 179.07 88.9 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C35 (at -19.05 1.27 270) (layer B.SilkS))
    (fp_text value .1uF (at -13.97 -2.54 270) (layer B.Fab))
    (fp_text user %R (at -17.78 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BAD)
    (at 250.19 88.9 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C36 (at -0.635 -15.875 270) (layer B.SilkS))
    (fp_text value .1uF (at -16.51 1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BA2)
    (at 245.745 85.725)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C37 (at 1.905 -14.605) (layer B.SilkS))
    (fp_text value 10uF (at -1.27 -14.605) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BA4)
    (at 239.395 85.725)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C38 (at -0.635 -13.97) (layer B.SilkS))
    (fp_text value .1uF (at -1.905 -14.605) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4ADC)
    (at 245.745 121.285)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C39 (at 1.27 8.89) (layer B.SilkS))
    (fp_text value .1uF (at 0.635 5.08) (layer B.Fab))
    (fp_text user %R (at 0 8.255) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4ACA)
    (at 239.395 121.285)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C40 (at 0 7.62) (layer B.SilkS))
    (fp_text value .1uF (at 0.635 8.255) (layer B.Fab))
    (fp_text user %R (at 0.635 12.065) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BB0)
    (at 245.745 103.505)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C41 (at 18.415 1.905) (layer B.SilkS))
    (fp_text value .1uF (at -1.905 -31.115) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4BAB)
    (at 239.395 103.505)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C42 (at 26.035 0) (layer B.SilkS))
    (fp_text value .1uF (at -0.635 -31.115) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4868)
    (at 144.145 121.285)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C43 (at 0.635 6.35) (layer B.SilkS))
    (fp_text value .1uF (at 0 7.62) (layer B.Fab))
    (fp_text user %R (at 0.635 7.62) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB486D)
    (at 137.795 121.285)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C44 (at 0.635 6.35) (layer B.SilkS))
    (fp_text value .1uF (at 0 8.89) (layer B.Fab))
    (fp_text user %R (at 0.635 7.62) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4876)
    (at 128.27 113.03 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C45 (at 15.875 0.635 270) (layer B.SilkS))
    (fp_text value .1uF (at 16.51 -2.54 270) (layer B.Fab))
    (fp_text user %R (at 17.145 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB48AB)
    (at 128.27 106.68 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C46 (at 20.955 1.27 270) (layer B.SilkS))
    (fp_text value .1uF (at 20.32 0 270) (layer B.Fab))
    (fp_text user %R (at 21.59 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB48C5)
    (at 144.145 103.505)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C47 (at 1.905 24.13) (layer B.SilkS))
    (fp_text value .1uF (at 4.445 24.13) (layer B.Fab))
    (fp_text user %R (at -0.635 24.13) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB48C7)
    (at 137.795 103.505)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C48 (at 0 24.13) (layer B.SilkS))
    (fp_text value .1uF (at 6.985 24.13) (layer B.Fab))
    (fp_text user %R (at 1.905 24.13) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB48EA)
    (at 128.27 95.25 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C49 (at -22.225 1.27 270) (layer B.SilkS))
    (fp_text value .1uF (at -24.765 -2.54 270) (layer B.Fab))
    (fp_text user %R (at -22.86 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB48DD)
    (at 128.27 88.9 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C50 (at -17.145 -0.635 270) (layer B.SilkS))
    (fp_text value .1uF (at -16.51 -3.81 270) (layer B.Fab))
    (fp_text user %R (at -17.145 0.635 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB48FC)
    (at 144.145 85.725)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C51 (at 0.635 -11.43) (layer B.SilkS))
    (fp_text value .1uF (at 0.635 -15.875) (layer B.Fab))
    (fp_text user %R (at 0 -11.43) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB48FA)
    (at 137.795 85.725)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C52 (at 0.635 -12.7) (layer B.SilkS))
    (fp_text value .1uF (at -0.635 -11.43) (layer B.Fab))
    (fp_text user %R (at 0 -12.065) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB49CC)
    (at 158.75 113.03 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C53 (at 15.875 1.905 270) (layer B.SilkS))
    (fp_text value .1uF (at -41.275 -3.81 270) (layer B.Fab))
    (fp_text user %R (at 16.51 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB49C6)
    (at 158.75 106.68 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C54 (at -33.655 0.635 270) (layer B.SilkS))
    (fp_text value 10uF (at -33.02 -1.27 270) (layer B.Fab))
    (fp_text user %R (at -33.655 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4926)
    (at 158.75 95.25 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C55 (at -20.955 2.54 270) (layer B.SilkS))
    (fp_text value .1uF (at -21.59 1.27 270) (layer B.Fab))
    (fp_text user %R (at -19.685 3.81 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB491C)
    (at 158.75 88.9 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C56 (at -15.875 3.175 270) (layer B.SilkS))
    (fp_text value .1uF (at -14.605 -0.635 270) (layer B.Fab))
    (fp_text user %R (at -15.24 4.445 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB494B)
    (at 174.625 85.725)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C57 (at 0 -15.24) (layer B.SilkS))
    (fp_text value .1uF (at -0.635 -13.335) (layer B.Fab))
    (fp_text user %R (at -0.635 -14.605) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB493D)
    (at 168.275 85.725)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C58 (at -0.635 -12.065) (layer B.SilkS))
    (fp_text value .1uF (at -0.635 -13.335) (layer B.Fab))
    (fp_text user %R (at -1.27 -12.065) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4905)
    (at 148.59 88.9 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C59 (at -15.24 1.905 270) (layer B.SilkS))
    (fp_text value 10uF (at -14.605 -0.635 270) (layer B.Fab))
    (fp_text user %R (at -15.24 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4916)
    (at 148.59 95.25 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C60 (at -21.59 1.905 270) (layer B.SilkS))
    (fp_text value .1uF (at -21.59 -0.635 270) (layer B.Fab))
    (fp_text user %R (at -22.86 2.54 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB48ED)
    (at 144.145 83.185 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED1 (at 10.795 -4.445 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 14.605 0.635 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(LED1-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(LED1-Pad2)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB48EB)
    (at 137.795 83.185 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED2 (at 10.16 -3.81 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 15.24 3.175 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(LED2-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(LED1-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB48D9)
    (at 130.81 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED3 (at -3.81 -13.335) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.905 -15.875) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(LED3-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(LED2-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB492C)
    (at 130.81 95.25)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED4 (at 1.905 -22.86) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 1.27 -20.32) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(LED4-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(LED3-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB48C2)
    (at 144.145 100.965 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED5 (at -26.67 -2.54 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -33.02 8.89 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(LED5-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(LED4-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB48BF)
    (at 137.795 100.965 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED6 (at -27.305 -13.335 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -33.655 12.7 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(LED6-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(LED5-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB48AD)
    (at 130.81 106.68)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED7 (at 2.54 19.685) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0.635 22.225) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED7-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(LED6-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB489F)
    (at 130.81 113.03)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED8 (at -0.635 14.605) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 1.905 15.24) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED8-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED7-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB484C)
    (at 137.795 118.745 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED9 (at -10.16 -2.54 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -15.875 2.54 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED10-Pad2)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED8-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB486A)
    (at 144.145 118.745 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED10 (at -10.795 -2.54 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -17.145 3.81 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(LED10-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED10-Pad2)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB488D)
    (at 151.13 113.03)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED11 (at 2.54 15.24) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0 19.685) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED11-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(LED10-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB488F)
    (at 151.13 106.68)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED12 (at 0 20.955) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 1.905 24.13) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(LED12-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED11-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4930)
    (at 151.13 95.25)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED13 (at -1.27 -20.955) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -3.175 -19.05) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED13-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(LED12-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4908)
    (at 151.13 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED14 (at -0.635 -16.51) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.905 -15.24) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(LED14-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED13-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4944)
    (at 174.625 83.185 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED15 (at 10.16 -5.08 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 15.24 3.175 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(LED15-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(LED14-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4942)
    (at 168.275 83.185 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED16 (at 10.16 -5.08 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 15.875 2.54 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED16-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(LED15-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4919)
    (at 161.29 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED17 (at -1.27 -14.605) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -3.81 -16.51) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(LED17-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED16-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4932)
    (at 161.29 95.25)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED18 (at -1.27 -21.59) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.905 -19.685) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED18-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(LED17-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB49D7)
    (at 174.625 100.965 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED19 (at 27.305 -3.175 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 34.29 6.985 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(LED19-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED18-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB49ED)
    (at 168.275 100.965 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED20 (at 27.94 -1.905 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -34.925 2.54 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(LED20-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(LED19-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB49BB)
    (at 161.29 106.68)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED21 (at -0.635 -33.02) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -5.715 22.86) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(LED21-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(LED20-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB49C9)
    (at 161.29 113.03)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED22 (at 2.54 -39.37) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.27 19.685) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(LED22-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(LED21-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A17)
    (at 168.275 118.745 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED23 (at -10.16 -1.905 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -14.605 5.08 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(LED23-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(LED22-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A16)
    (at 174.625 118.745 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED24 (at -10.16 -3.81 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -15.875 1.905 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(LED24-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(LED23-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A01)
    (at 181.61 113.03)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED25 (at 1.27 17.145) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 6.35 18.415) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(LED25-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(LED24-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB49FE)
    (at 181.61 106.68)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED26 (at -0.635 -33.655) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 5.08 24.13) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(LED26-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(LED25-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4989)
    (at 181.61 95.25)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED27 (at 1.27 -19.685) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -2.54 -19.685) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(LED27-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(LED26-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4962)
    (at 181.61 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED28 (at -0.635 -13.335) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0 -13.335) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(LED28-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(LED27-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4997)
    (at 191.77 92.075)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED29 (at 1.905 -19.05) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.905 -18.415) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(LED29-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(LED28-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A29)
    (at 191.77 109.22)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED30 (at 0 19.685) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.27 21.59) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(LED30-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(LED29-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B81)
    (at 215.265 83.185 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED31 (at 11.43 -2.54 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0.635 50.165 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(LED31-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(LED30-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B7F)
    (at 208.915 83.185 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED32 (at 10.795 -5.08 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.27 57.15 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(LED32-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(LED31-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB499A)
    (at 201.93 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED33 (at -1.27 -15.24) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -3.175 -15.24) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(LED33-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(LED32-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB49AB)
    (at 201.93 95.25)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED34 (at -3.175 -22.86) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -3.81 -21.59) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(LED34-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(LED33-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4AA6)
    (at 215.265 100.965 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED35 (at -29.845 3.81 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -32.385 8.255 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(LED35-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(LED34-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A67)
    (at 208.915 100.965 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED36 (at -29.21 -3.81 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -34.29 1.27 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(LED36-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(LED35-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A42)
    (at 201.93 106.68)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED37 (at 1.27 20.32) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0 21.59) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(LED37-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(LED36-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A40)
    (at 201.93 113.03)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED38 (at 0 14.605) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -0.635 22.225) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(LED38-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(LED37-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A4B)
    (at 208.915 118.745 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED39 (at -10.795 -3.175 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -15.24 3.81 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(LED39-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(LED38-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A54)
    (at 215.265 118.745 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED40 (at -14.605 -2.54 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -15.875 3.81 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(LED40-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(LED39-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4A9E)
    (at 222.25 113.03)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED41 (at 0 13.97) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -2.54 15.875) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(LED41-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(LED40-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4AA2)
    (at 222.25 106.68)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED42 (at 4.445 20.955) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -6.985 26.035) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(LED42-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(LED41-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B92)
    (at 222.25 95.25)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED43 (at 0.635 -23.495) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 1.27 -24.13) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(LED43-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(LED42-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B8E)
    (at 222.25 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED44 (at 1.27 -16.51) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 2.54 -19.685) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(LED44-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(LED43-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B84)
    (at 245.745 83.185 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED45 (at 12.065 -2.54 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.27 23.495 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(LED45-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(LED44-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B82)
    (at 239.395 83.185 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED46 (at 14.605 -3.81 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0.635 27.94 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(LED46-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(LED45-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B8D)
    (at 232.41 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED47 (at 0 -17.78) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.905 -20.955) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(LED47-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(LED46-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B94)
    (at 232.41 95.25)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED48 (at -1.27 -21.59) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -3.81 -24.13) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(LED48-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(LED47-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B8B)
    (at 245.745 100.965 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED49 (at -1.27 21.59 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.905 18.415 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(LED49-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(LED48-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B45)
    (at 239.395 100.965 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED50 (at 1.905 27.94 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.905 23.495 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(LED50-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(LED49-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4AC0)
    (at 232.41 106.68)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED51 (at 0 24.13) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -1.905 22.86) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(LED51-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(LED50-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4AB5)
    (at 232.41 113.03)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED52 (at 0 13.335) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -3.81 16.51) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(LED52-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(LED51-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4ACC)
    (at 239.395 118.745 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED53 (at -10.795 -3.81 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -15.24 5.08 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(LED53-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(LED52-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4ADD)
    (at 245.745 118.745 90)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED54 (at -8.89 -2.54 90) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -14.605 3.175 90) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(LED54-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(LED53-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6 90) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4AEC)
    (at 252.73 113.03)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED55 (at 0.635 13.97) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 1.27 19.05) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(LED55-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(LED54-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4AEE)
    (at 252.73 106.68)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED56 (at 0 22.225) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at -0.635 21.59) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(LED56-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(LED55-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B4A)
    (at 252.73 95.25)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED57 (at 12.7 -3.175) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0.635 34.925) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(LED57-Pad4)"))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(LED56-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 58DB4B88)
    (at 252.73 88.9)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED58 (at 0 -15.875) (layer F.SilkS))
    (fp_text value WS2812B-5050-SMD (at 0 -16.51) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 63 D2))
    (pad 2 smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(LED57-Pad4)"))
    (pad 1 smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Libraries:MicroUSBtoTTLModule (layer B.Cu) (tedit 58DB4CAA)
    (at 59.69 107.95 90)
    (fp_text reference P5 (at -1.27 -9.525 90) (layer B.SilkS))
    (fp_text value "Serial Module" (at 1.27 -10.795 90) (layer B.Fab))
    (fp_text user +5V (at 6.35 -3.175 360) (layer B.SilkS))
    (fp_text user GND (at 3.81 -3.175 360) (layer B.SilkS))
    (fp_text user TXO (at 1.27 -3.175 360) (layer B.SilkS))
    (fp_text user RXI (at -1.27 -3.175 360) (layer B.SilkS))
    (fp_text user DTR (at -3.81 -3.175 360) (layer B.SilkS))
    (fp_text user 3V3 (at -6.35 -3.175 360) (layer B.SilkS))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 "Net-(P5-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 Tx))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 Rx))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "Net-(P5-Pad6)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer B.Cu) (tedit 58DB4CB9)
    (at 93.345 120.65)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference P6 (at -2.54 7.62) (layer B.SilkS))
    (fp_text value "Reset Button" (at 0.635 7.62) (layer B.Fab))
    (fp_text user %R (at 0 7.62) (layer B.Fab))
    (pad 1 smd rect (at -4.59 0) (size 2.18 1.6) (layers B.Cu B.Paste B.Mask)
      (net 75 RESET))
    (pad 2 smd rect (at 4.59 0) (size 2.18 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_FSMSM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer B.Cu) (tedit 58DB4CB1)
    (at 93.345 111.76)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference P7 (at -3.175 13.97) (layer B.SilkS))
    (fp_text value "Program Button" (at 0.635 15.24) (layer B.Fab))
    (fp_text user %R (at 0.635 14.605) (layer B.Fab))
    (pad 1 smd rect (at -4.59 0) (size 2.18 1.6) (layers B.Cu B.Paste B.Mask)
      (net 76 D0))
    (pad 2 smd rect (at 4.59 0) (size 2.18 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_FSMSM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58DB4828)
    (at 85.725 120.65 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -6.985 1.27 90) (layer B.SilkS))
    (fp_text value 10k (at -6.35 -2.54 90) (layer B.Fab))
    (fp_text user %R (at -6.35 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 75 RESET))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:ESP8266-01 (layer B.Cu) (tedit 58DB4CB3)
    (at 92.71 103.505)
    (fp_text reference U1 (at 4.445 22.225) (layer B.SilkS))
    (fp_text value ESP8266-01 (at 0.635 23.495) (layer B.Fab))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 Rx))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at -1.27 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 RESET))
    (pad 5 thru_hole circle (at 1.27 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 D2))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 7 thru_hole circle (at 3.81 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 3.81 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 Tx))
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4895)
    (at 148.59 106.68 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C61 (at 21.59 0 270) (layer B.SilkS))
    (fp_text value 10uF (at 20.32 -6.985 270) (layer B.Fab))
    (fp_text user %R (at 20.955 0.635 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58DB4888)
    (at 148.59 113.03 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C62 (at 14.605 -1.27 270) (layer B.SilkS))
    (fp_text value .1uF (at 14.605 -7.62 270) (layer B.Fab))
    (fp_text user %R (at 14.605 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58DB481D)
    (at 114.935 108.585)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C63 (at -0.635 19.685) (layer F.SilkS))
    (fp_text value .1uF (at -1.27 18.415) (layer F.Fab))
    (fp_text user %R (at -0.635 19.05) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58DB4818)
    (at 114.935 111.125)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C64 (at -2.54 16.51) (layer F.SilkS))
    (fp_text value .1uF (at -3.81 17.145) (layer F.Fab))
    (fp_text user %R (at -0.635 16.51) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58DB47B3)
    (at 85.725 107.315 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C65 (at 19.685 0 270) (layer F.SilkS))
    (fp_text value .1uF (at 19.685 3.81 270) (layer F.Fab))
    (fp_text user %R (at 19.685 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58DB47B0)
    (at 88.265 107.315 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C66 (at 19.685 0 270) (layer F.SilkS))
    (fp_text value .1uF (at 19.685 6.985 270) (layer F.Fab))
    (fp_text user %R (at 20.32 -0.635 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer F.Cu) (tedit 58DB4795)
    (at 92.71 120.015 180)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference P8 (at -0.635 -6.35 180) (layer F.SilkS))
    (fp_text value CONN_02X03 (at -2.54 -6.985 180) (layer F.Fab))
    (fp_text user %R (at 0 -7.62 180) (layer F.Fab))
    (pad 1 smd rect (at -2.77 -2.54 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2.77 -2.54 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.77 0 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 63 D2))
    (pad 4 smd rect (at 2.77 0 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 63 D2))
    (pad 5 smd rect (at -2.77 2.54 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.77 2.54 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer B.Cu) (tedit 58DB4A98)
    (at 227.33 120.015)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference P9 (at 0.635 9.525) (layer B.SilkS))
    (fp_text value CONN_02X03 (at 0.635 8.255) (layer B.Fab))
    (fp_text user %R (at 0 11.43) (layer B.Fab))
    (pad 1 smd rect (at -2.77 2.54) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2.77 2.54) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.77 0) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 63 D2))
    (pad 4 smd rect (at 2.77 0) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 63 D2))
    (pad 5 smd rect (at -2.77 -2.54) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.77 -2.54) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_A_Vertical (layer B.Cu) (tedit 58DB47FC)
    (at 109.855 92.075 90)
    (descr "USB A vertical female connector, right angle")
    (tags "USB_A_Vertical female connector angled 73725-0110BLF")
    (fp_text reference P2 (at 16.51 -10.795 90) (layer B.SilkS))
    (fp_text value USB_A (at 19.685 0.635 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 65 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at 0 -4 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 64 "Net-(P2-Pad3)"))
    (pad 5 thru_hole circle (at 2.72 0.73 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 0 -6 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 2.72 -6.27 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -2.72 0.73 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -2.72 -6.27 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors.3dshapes/USB_A_Vertical.wrl
      (at (xyz 0.01 -0.02 0.05))
      (scale (xyz 0.41 0.41 0.41))
      (rotate (xyz 0 -90 180))
    )
  )
  (module Connect:USB_A_Vertical (layer B.Cu) (tedit 58DB48D2)
    (at 109.855 100.965 90)
    (descr "USB A vertical female connector, right angle")
    (tags "USB_A_Vertical female connector angled 73725-0110BLF")
    (fp_text reference P3 (at -26.035 -5.715 90) (layer B.SilkS))
    (fp_text value USB_A (at 28.575 14.605 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 67 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at 0 -4 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 66 "Net-(P3-Pad3)"))
    (pad 5 thru_hole circle (at 2.72 0.73 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 0 -6 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 2.72 -6.27 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -2.72 0.73 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -2.72 -6.27 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors.3dshapes/USB_A_Vertical.wrl
      (at (xyz 0.01 -0.02 0.05))
      (scale (xyz 0.41 0.41 0.41))
      (rotate (xyz 0 -90 180))
    )
  )
  (module Connect:USB_A_Vertical (layer B.Cu) (tedit 58DB4821)
    (at 109.855 109.855 90)
    (descr "USB A vertical female connector, right angle")
    (tags "USB_A_Vertical female connector angled 73725-0110BLF")
    (fp_text reference P4 (at -17.145 -8.255 90) (layer B.SilkS))
    (fp_text value USB_A (at -18.415 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 69 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 0 -4 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 68 "Net-(P4-Pad3)"))
    (pad 5 thru_hole circle (at 2.72 0.73 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 0 -6 90) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 2.72 -6.27 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -2.72 0.73 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -2.72 -6.27 90) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors.3dshapes/USB_A_Vertical.wrl
      (at (xyz 0.01 -0.02 0.05))
      (scale (xyz 0.41 0.41 0.41))
      (rotate (xyz 0 -90 180))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB4959)
    (at 191.77 81.915)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at -1.905 -6.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB47EF)
    (at 130.81 81.915)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at -1.27 -6.985) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at -3.175 -6.985) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB483A)
    (at 130.81 120.015)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0.635 8.255) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 1.905 8.255) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB49FC)
    (at 191.77 120.015)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 1.905 14.605) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at -0.635 17.145) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB4AD6)
    (at 252.73 120.015)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 1.27 10.795) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at -1.27 9.525) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB4B85)
    (at 252.73 81.915)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0.635 -8.89) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 -9.525) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB4763)
    (at 57.15 81.915)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 5.08 -6.985) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB47C9)
    (at 118.11 81.915)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -6.985) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at -3.81 -6.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB480A)
    (at 118.11 120.015)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 7.62) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58DB477B)
    (at 57.15 120.015)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0.635 6.985) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0.635 5.715) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Libraries:BARREL_JACK (layer F.Cu) (tedit 58DB538E)
    (at 62.23 92.71)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at -13.335 5.715 180) (layer F.SilkS))
    (fp_text value BARREL_JACK (at -17.145 -6.35) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 9 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole circle (at -6 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -3 4.7) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_text Program (at 95.885 107.95) (layer B.SilkS))
  (gr_text Reset (at 104.14 120.65) (layer B.SilkS))
  (gr_line (start 123.19 90.805) (end 125.73 90.805) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 93.345) (end 125.73 93.345) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 108.585) (end 123.19 108.585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 111.125) (end 125.73 111.125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 93.345) (end 125.73 108.585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 90.805) (end 125.73 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 111.125) (end 125.73 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 108.585) (end 123.19 93.345) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 124.46) (end 123.19 111.125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 77.47) (end 123.19 90.805) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 52.07 77.47) (end 123.19 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 52.07 124.46) (end 52.07 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 124.46) (end 52.07 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 257.81 124.46) (end 125.73 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 257.81 77.47) (end 257.81 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 77.47) (end 257.81 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.73 77.47) (xy 257.81 77.47) (xy 257.81 124.46) (xy 125.73 124.46)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.73 77.47) (xy 257.81 77.47) (xy 257.81 124.46) (xy 125.73 124.46)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.07 77.47) (xy 123.19 77.47) (xy 123.19 124.46) (xy 52.07 124.46)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.07 77.47) (xy 123.19 77.47) (xy 123.19 124.46) (xy 52.07 124.46)
      )
    )
  )
)
