(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 514)
    (zones 0)
    (modules 32)
    (nets 36)
  )
  (page A)
  (title_block
    (title "Internet Interrupter v1")
    (rev 1)
    (company "Edje Electronics")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.508 0.381)
    (user_via 0.635 0.381)
    (user_via 0.762 0.508)
    (user_via 1.27 0.762)
    (user_via 2.032 1.016)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "outputs/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(A1-Pad9)")
  (net 4 +3V3)
  (net 5 "Net-(A1-Pad10)")
  (net 6 "Net-(A1-Pad3)")
  (net 7 "Net-(A1-Pad11)")
  (net 8 "Net-(A1-Pad4)")
  (net 9 "Net-(A1-Pad12)")
  (net 10 "Net-(A1-Pad5)")
  (net 11 "Net-(A1-Pad13)")
  (net 12 "Net-(A1-Pad6)")
  (net 13 "Net-(A1-Pad14)")
  (net 14 "Net-(A1-Pad15)")
  (net 15 "Net-(A1-Pad16)")
  (net 16 "Net-(D1-Pad1)")
  (net 17 MOSI)
  (net 18 MISO)
  (net 19 SCK)
  (net 20 "Net-(J3-Pad2)")
  (net 21 "Net-(R1-Pad2)")
  (net 22 +12V)
  (net 23 "Net-(C6-Pad1)")
  (net 24 "Net-(C8-Pad1)")
  (net 25 "Net-(D2-Pad2)")
  (net 26 SDA)
  (net 27 SCL)
  (net 28 INT)
  (net 29 ~CS)
  (net 30 "Net-(J2-Pad2)")
  (net 31 "Net-(J2-Pad1)")
  (net 32 "Net-(J5-Pad4)")
  (net 33 "Net-(J5-Pad3)")
  (net 34 "Net-(U1-Pad4)")
  (net 35 "Net-(U1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net INT)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net ~CS)
  )
  (net_class 10mil ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 20mil ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 1.016)
    (via_drill 0.635)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 50mil ""
    (clearance 0.1524)
    (trace_width 1.27)
    (via_dia 1.905)
    (via_drill 1.016)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 6mil ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Ethernet ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2)
    (diff_pair_gap 0.2)
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 130.048 79.502 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.524) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 138.43 98.552 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value "SL54-TP 5A" (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mouser_Parts:214450554 (layer F.Cu) (tedit 0)
    (at 143.51 117.094)
    (descr 2-1445055-4-2)
    (tags Connector)
    (fp_text reference J4 (at 5.842 6.35) (layer F.SilkS))
    (fp_text value Conn_01x04 (at -4.5 4.077) (layer F.SilkS) hide)
    (fp_text user %R (at -4.5 4.077) (layer F.Fab))
    (pad MH2 np_thru_hole circle (at -6.85 4.32) (size 3 0) (drill 3) (layers *.Cu *.Mask))
    (pad MH1 np_thru_hole circle (at -2.15 4.32) (size 3 0) (drill 3) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -9 0) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad3)"))
    (pad 3 thru_hole circle (at -6 0) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad4)"))
    (pad 2 thru_hole circle (at -3 0) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad5)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad6)"))
    (model C:\Users\WirickD\Documents\KiCad\SamacSys_Parts.3dshapes\2-1445055-4.stp
      (offset (xyz -4.499999932416815 -8.879999981076789 2.190000024329962))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Crystal:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5A1AD3B8)
    (at 125.222 95.758)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at -4.572 0) (layer F.SilkS))
    (fp_text value 8Mhz (at 2.44 3.525) (layer F.Fab))
    (fp_text user %R (at 2.44 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5F3E4A84)
    (at 118.364 84.328 90)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U5 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value ADS1013IDGS (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 10 smd rect (at 2.15 -1 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 SCL))
    (pad 9 smd rect (at 2.15 -0.5 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 SDA))
    (pad 8 smd rect (at 2.15 0 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 7 smd rect (at 2.15 0.5 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.15 1 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.15 1 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J5-Pad3)"))
    (pad 4 smd rect (at -2.15 0.5 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J5-Pad4)"))
    (pad 3 smd rect (at -2.15 0 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.15 -0.5 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.15 -1 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 126.238 86.614 90)
    (descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U4 (at -3.81 7.112 180) (layer F.SilkS))
    (fp_text value MCP2515-xSO (at 0 6.72 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 18 smd roundrect (at 4.65 -5.08 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 17 smd roundrect (at 4.65 -3.81 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(R1-Pad2)"))
    (pad 16 smd roundrect (at 4.65 -2.54 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 ~CS))
    (pad 15 smd roundrect (at 4.65 -1.27 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 MISO))
    (pad 14 smd roundrect (at 4.65 0 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 MOSI))
    (pad 13 smd roundrect (at 4.65 1.27 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 SCK))
    (pad 12 smd roundrect (at 4.65 2.54 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 INT))
    (pad 11 smd roundrect (at 4.65 3.81 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 4.65 5.08 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -4.65 5.08 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at -4.65 3.81 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C8-Pad1)"))
    (pad 7 smd roundrect (at -4.65 2.54 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C6-Pad1)"))
    (pad 6 smd roundrect (at -4.65 1.27 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -4.65 0 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -4.65 -1.27 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -4.65 -2.54 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -4.65 -3.81 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(U1-Pad4)"))
    (pad 1 smd roundrect (at -4.65 -5.08 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 125.984 100.076 270)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 5.588 -2.794 180) (layer F.SilkS))
    (fp_text value MCP2551-I_P (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad4)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 116.078 120.396 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -2.032 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 25 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 118.364 88.392)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.794 -0.762) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 26 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 118.355 90.424)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.785 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 27 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Local_Transistors:TRANS_AONR21321 (layer F.Cu) (tedit 61A6BE04)
    (at 119.126 113.03 90)
    (fp_text reference Q1 (at 2.54 -0.254 180) (layer F.SilkS))
    (fp_text value AONR21321 (at 6.985 3.175 90) (layer F.Fab))
    (pad 5 smd rect (at 1.5 0.975 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 +12V))
    (pad 6 smd rect (at 1.5 0.325 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 +12V))
    (pad 8 smd rect (at 1.5 -0.975 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 +12V))
    (pad 7 smd rect (at 1.5 -0.325 90) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 +12V))
    (pad 9 smd rect (at 0.36 0 90) (size 1.98 2.45) (layers F.Cu F.Mask)
      (net 22 +12V))
    (pad 9_2 smd rect (at 0 1.415 90) (size 0.43 0.38) (layers F.Cu F.Paste F.Mask)
      (net 22 +12V))
    (pad 9_1 smd rect (at 0 -1.415 90) (size 0.43 0.38) (layers F.Cu F.Paste F.Mask)
      (net 22 +12V))
    (pad 4 smd rect (at -1.4 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.4 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at -1.4 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at -1.4 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad2)"))
  )
  (module Mouser_Parts:214450554 (layer F.Cu) (tedit 0)
    (at 114.554 91.948 270)
    (descr 2-1445055-4-2)
    (tags Connector)
    (fp_text reference J5 (at -13.97 4.572 180) (layer F.SilkS))
    (fp_text value Conn_01x04 (at -4.572 7.112 90) (layer F.SilkS) hide)
    (fp_text user %R (at -4.5 4.077 90) (layer F.Fab))
    (pad MH2 np_thru_hole circle (at -6.85 4.32 270) (size 3 0) (drill 3) (layers *.Cu *.Mask))
    (pad MH1 np_thru_hole circle (at -2.15 4.32 270) (size 3 0) (drill 3) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -9 0 270) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad4)"))
    (pad 3 thru_hole circle (at -6 0 270) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-Pad3)"))
    (pad 2 thru_hole circle (at -3 0 270) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (model C:\Users\WirickD\Documents\KiCad\SamacSys_Parts.3dshapes\2-1445055-4.stp
      (offset (xyz -4.499999932416815 -8.879999981076789 2.190000024329962))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Mouser_Parts:214450552 (layer F.Cu) (tedit 0)
    (at 124.968 117.094)
    (descr 2-1445055-2-1)
    (tags Connector)
    (fp_text reference J3 (at -8.89 6.604) (layer F.SilkS))
    (fp_text value Conn_01x02 (at -1.5 4.078) (layer F.SilkS) hide)
    (fp_text user %R (at -1.5 4.078) (layer F.Fab))
    (pad MH1 np_thru_hole circle (at -1.5 4.32) (size 3.05 0) (drill 3.05) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -3 0) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (model C:\Users\WirickD\Documents\KiCad\SamacSys_Parts.3dshapes\2-1445055-2.stp
      (offset (xyz -1.499999977472255 -8.879999981076789 2.269999946834539))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Mouser_Parts:214450552 (layer F.Cu) (tedit 0)
    (at 114.554 104.394 270)
    (descr 2-1445055-2-1)
    (tags Connector)
    (fp_text reference J2 (at 5.842 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at -1.524 7.366 90) (layer F.SilkS) hide)
    (fp_text user %R (at -1.5 4.078 90) (layer F.Fab))
    (pad MH1 np_thru_hole circle (at -1.5 4.32 270) (size 3.05 0) (drill 3.05) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -3 0 270) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad1)"))
    (model C:\Users\WirickD\Documents\KiCad\SamacSys_Parts.3dshapes\2-1445055-2.stp
      (offset (xyz -1.499999977472255 -8.879999981076789 2.269999946834539))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323F (layer F.Cu) (tedit 590A48EB)
    (at 116.078 116.84 270)
    (descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
    (tags SOD-323F)
    (attr smd)
    (fp_text reference D2 (at 0.254 2.032 180) (layer F.SilkS))
    (fp_text value D3Z10BF-7 (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 +12V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 118.355 80.264)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at -3.547 0) (layer F.SilkS))
    (fp_text value ".1uF 50V" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 118.364 78.232)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at -4.064 0) (layer F.SilkS))
    (fp_text value "1uF 50V" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 131.064 100.584 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 3.048 0.508 90) (layer F.SilkS))
    (fp_text value "22pF 50V" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 24 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 122.428 79.502)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.65) (layer F.SilkS))
    (fp_text value ".1uF 50V" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.032 100.584 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 3.048 -0.254 90) (layer F.SilkS))
    (fp_text value "22pF 50V" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 128.27 113.03 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -2.794 0 180) (layer F.SilkS))
    (fp_text value ".1uF 50V" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.238 79.502)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value "10uF 50V" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 137.668 82.804 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 8.636 0 180) (layer F.SilkS))
    (fp_text value "220uF 10V" (at 2.5 6.25 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 125.476 112.014 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.064 2.286) (layer F.SilkS))
    (fp_text value "100uF 50V" (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 +12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical locked (layer B.Cu) (tedit 5C623400)
    (at 112.8 75.55 270)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference J1 (at -3.414 2.564) (layer F.SilkS))
    (fp_text value Raspberry_Pi_2_3 (at -1.27 -51.03 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -24.13 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 SDA))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 SCL))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad15)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad16)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 MOSI))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 MISO))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 INT))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 SCK))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 ~CS))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad10)"))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad11)"))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad9)"))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad12)"))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad14)"))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad13)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:Pololu_Breakout-16_15.2x20.3mm (layer F.Cu) (tedit 58AB602C)
    (at 149.86 117.856 90)
    (descr "Pololu Breakout 16-pin 15.2x20.3mm 0.6x0.8\\")
    (tags "Pololu Breakout")
    (fp_text reference A1 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value Pololu_Breakout_A4988 (at 6.35 20.17 90) (layer F.Fab))
    (fp_text user %R (at 6.35 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 12.7 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad9)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 10 thru_hole oval (at 12.7 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad3)"))
    (pad 11 thru_hole oval (at 12.7 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad11)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad4)"))
    (pad 12 thru_hole oval (at 12.7 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad12)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad5)"))
    (pad 13 thru_hole oval (at 12.7 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad6)"))
    (pad 14 thru_hole oval (at 12.7 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad14)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 12.7 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad15)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 +12V))
    (pad 16 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad16)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Pololu_Breakout-16_15.2x20.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mouser_Parts:PE54040SNL (layer F.Cu) (tedit 0)
    (at 156.21 90.424 90)
    (descr PE-54040SNL-1)
    (tags Inductor)
    (attr smd)
    (fp_text reference L1 (at -1.27 -13.97 90) (layer F.SilkS))
    (fp_text value PE-54040SNL (at 0 0 90) (layer Cmts.User) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd oval (at -10.54 0 90) (size 2.03 17.78) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad1)"))
    (pad 2 smd oval (at 10.54 0 90) (size 2.03 17.78) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model C:\Users\WirickD\Documents\KiCad\SamacSys_Parts.3dshapes\PE-54040SNL.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-5_TabPin3 (layer F.Cu) (tedit 5A70FBB6)
    (at 139.626999 109.474002)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (attr smd)
    (fp_text reference U3 (at -6.022999 -5.080002) (layer F.SilkS))
    (fp_text value LM2596S-5 (at 0 6.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -3.4) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 22 +12V))
    (pad 2 smd rect (at -5.775 -1.7) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at -5.775 0) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -5.775 1.7) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -5.775 3.4) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 3.375 0) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-5_TabPin3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 108 74.25)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference H1 (at -3.606 -3.892) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 166 74.25)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 3.672 -4.4) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 108 123.25)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference H5 (at -4.368 4.766) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 166 123.25)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference H6 (at 4.434 4.766) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text ADC (at 106.68 77.978) (layer F.SilkS))
  (gr_text CAN (at 106.68 110.236) (layer F.SilkS))
  (gr_text PWR (at 115.316 125.476) (layer F.SilkS))
  (gr_text STEPPER (at 152.4 125.222) (layer F.SilkS))
  (gr_line (start 169.5 73.75) (end 169.5 123.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 104.5 73.75) (end 104.5 123.75) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 107.5 73.75) (end 107.5 70.75) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 166.5 73.75) (end 169.5 73.75) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 166.5 70.75) (end 107.5 70.75) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 166.5 123.75) (end 166.5 126.75) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 107.5 126.75) (end 166.5 126.75) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 107.5 123.75) (end 104.5 123.75) (angle -90) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.14 69.85) (xy 170.18 69.85) (xy 170.18 127.254) (xy 104.14 127.254)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.196 69.088) (xy 151.384 69.088) (xy 147.32 69.088) (xy 145.288 69.088) (xy 143.256 69.088)
        (xy 141.732 69.088) (xy 139.7 69.088) (xy 137.668 69.088) (xy 134.62 69.088) (xy 132.588 69.088)
        (xy 130.556 69.088) (xy 128.016 69.088) (xy 124.46 69.088) (xy 118.364 69.088) (xy 113.284 69.088)
        (xy 103.632 69.088) (xy 103.632 128.016) (xy 141.224 128.016) (xy 171.196 128.016)
      )
    )
  )
)
