(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 5)
    (no_connects 0)
    (area -7.695001 -8.965001 7.695001 12.775001)
    (thickness 1.6)
    (drawings 17)
    (tracks 18)
    (zones 0)
    (modules 2)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ./gerber))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
  )
  (net_class Edge ""
    (clearance 0.6858)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class Power ""
    (clearance 0.2032)
    (trace_width 0.381)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 59F10479)
    (at 3.81 10.16 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value CONN_01X04 (at -2.54 -3.81 360) (layer B.Fab) hide)
    (fp_text user %R (at 0 -3.81 360) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RetroJDM_Pots_Encoders:PEC11R (layer F.Cu) (tedit 59F10473)
    (at 0 0)
    (fp_text reference SW1 (at 0 -7.62) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 0 10.16) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 2.5 7.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 7.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.5 7.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at -2.5 -7) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 2.5 -7) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at -5.7 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.7 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text "RetroJDM.com\nPEC11R\nBreakout\nv1.0" (at 0 0) (layer B.SilkS))
  (gr_text G (at 3.81 12.065) (layer F.SilkS))
  (gr_text A (at 1.27 12.065) (layer F.SilkS))
  (gr_text B (at -1.27 12.065) (layer F.SilkS))
  (gr_text S (at -3.81 12.065) (layer F.SilkS))
  (gr_text S (at -3.81 12.065) (layer B.SilkS))
  (gr_text B (at -1.27 12.065) (layer B.SilkS))
  (gr_text A (at 1.27 12.125) (layer B.SilkS))
  (gr_text G (at 3.81 12.125) (layer B.SilkS))
  (gr_arc (start 5.08 10.16) (end 7.62 10.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start -5.08 10.16) (end -5.08 12.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start -5.08 -6.35) (end -7.62 -6.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -7.62 10.16) (end -7.62 -6.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 5.08 12.7) (end -5.08 12.7) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 5.08 -6.35) (end 5.08 -8.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 5.08 -8.89) (end -5.08 -8.89) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 7.62 10.16) (end 7.62 -6.35) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -7.62 -8.89) (xy 7.62 -8.89) (xy 7.62 12.7) (xy -7.62 12.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -7.62 -8.89) (xy 7.62 -8.89) (xy 7.62 12.7) (xy -7.62 12.7)
      )
    )
  )
)
