<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="39.294" y2="0" width="0" layer="20"/>
<wire x1="39.294" y1="0" x2="39.294" y2="26.66" width="0" layer="20"/>
<wire x1="39.294" y1="26.66" x2="0" y2="26.66" width="0" layer="20"/>
<wire x1="0" y1="26.66" x2="0" y2="0" width="0" layer="20"/>
<text>12VDC</text>
<text>12VDC</text>
<text>GND</text>
<text>GND</text>
<text>Battery</text>
<text>Load</text>
<text>RV-Project.Com
Switch Adapter
SWINT-1B
1-12-2021</text>
<text>12VDC</text>
<text>GND</text>
<text>LED Terminal</text>
<text>LED Terminal</text>
<text>R1 (or Jumper)</text>
</plain>
<libraries>
<library name="a-lib">
<description>Archive Library (for old designs) - do not use for new components.</description>
<packages>
<package name="D041-3.5MIL">
<description>Pitch: 0.35"</description>
</package>
<package name="251SMALL">
<description>Pitch: 0.45"&lt;br&gt;
Drill: 0.027" dia</description>
</package>
<package name="KEYSTONE_4919">
</package>
<package name="MO1-18AWG">
</package>
<package name="1/4W_AXIAL_RESISTOR_3.5MIL(V2)">
<description>Axial 1/4Watt Resistor&lt;p&gt;Pitch: 0.35"</description>
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="KEYSTONE3528">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="F1" library="a-lib" package="251SMALL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="a-lib_Connectors" package="KEYSTONE3528" value=""/>
<element name="JP2" library="a-lib_Connectors" package="KEYSTONE3528" value=""/>
<element name="JP3" library="a-lib_Connectors" package="KEYSTONE3528" value=""/>
<element name="JP4" library="a-lib" package="KEYSTONE_4919" value=""/>
<element name="JP5" library="a-lib" package="KEYSTONE_4919" value=""/>
<element name="JP6" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP7" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="R1" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP5" pad="T1"/>
<contactref element="JP5" pad="T2"/>
<contactref element="JP5" pad="T3"/>
<contactref element="R1" pad="1"/>
<contactref element="JP7" pad="P$1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="JP4" pad="T1"/>
<contactref element="JP4" pad="T2"/>
<contactref element="JP4" pad="T3"/>
<contactref element="JP3" pad="P$2"/>
<contactref element="JP3" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="F1" pad="P$1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="P$1"/>
<contactref element="JP1" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="JP6" pad="P$1"/>
<contactref element="F1" pad="P$2"/>
<contactref element="JP2" pad="P$2"/>
<contactref element="JP2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
