(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 179)
    (zones 0)
    (modules 7)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(SW1-Pad2)")
  (net 2 /COL0)
  (net 3 /ROW0)
  (net 4 /ROW2)
  (net 5 "Net-(SW2-Pad2)")
  (net 6 "Net-(SW3-Pad2)")
  (net 7 /COL1)
  (net 8 "Net-(SW4-Pad2)")
  (net 9 "Net-(SW5-Pad2)")
  (net 10 "Net-(A1-Pad1)")
  (net 11 "Net-(A1-Pad2)")
  (net 12 "Net-(A1-Pad3)")
  (net 13 "Net-(A1-Pad5)")
  (net 14 "Net-(A1-Pad17)")
  (net 15 "Net-(A1-Pad6)")
  (net 16 "Net-(A1-Pad18)")
  (net 17 "Net-(A1-Pad7)")
  (net 18 "Net-(A1-Pad19)")
  (net 19 "Net-(A1-Pad8)")
  (net 20 "Net-(A1-Pad20)")
  (net 21 "Net-(A1-Pad9)")
  (net 22 "Net-(A1-Pad21)")
  (net 23 "Net-(A1-Pad10)")
  (net 24 "Net-(A1-Pad11)")
  (net 25 "Net-(A1-Pad12)")
  (net 26 "Net-(A1-Pad13)")
  (net 27 "Net-(A1-Pad14)")
  (net 28 "Net-(A1-Pad15)")
  (net 29 "Net-(A1-Pad27)")
  (net 30 "Net-(A1-Pad16)")
  (net 31 "Net-(A1-Pad28)")
  (net 32 /ROW1)
  (net 33 GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /COL0)
    (add_net /COL1)
    (add_net /ROW0)
    (add_net /ROW1)
    (add_net /ROW2)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(SW3-Pad2)")
    (add_net "Net-(SW4-Pad2)")
    (add_net "Net-(SW5-Pad2)")
  )
  (module alphadox:Feather_M0_Bluefruit (layer F.Cu) (tedit 5B7E2337)
    (at 58.42 101.6 90)
    (descr "Through hole straight pin header, 2x16, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x16 2.54mm double row")
    (fp_text reference A1 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value Feather_M0_Bluefruit (at 0 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -10.16 -19.05 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad1)"))
    (pad 2 thru_hole oval (at -10.16 -16.51 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad2)"))
    (pad 3 thru_hole oval (at -10.16 -13.97 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad3)"))
    (pad 4 thru_hole oval (at -10.16 -11.43 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 5 thru_hole oval (at -10.16 -8.89 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad5)"))
    (pad 17 thru_hole oval (at 10.16 -8.89 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad17)"))
    (pad 6 thru_hole oval (at -10.16 -6.35 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad6)"))
    (pad 18 thru_hole oval (at 10.16 -6.35 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad18)"))
    (pad 7 thru_hole oval (at -10.16 -3.81 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad7)"))
    (pad 19 thru_hole oval (at 10.16 -3.81 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad19)"))
    (pad 8 thru_hole oval (at -10.16 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad8)"))
    (pad 20 thru_hole oval (at 10.16 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad20)"))
    (pad 9 thru_hole oval (at -10.16 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad9)"))
    (pad 21 thru_hole oval (at 10.16 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad21)"))
    (pad 10 thru_hole oval (at -10.16 3.81 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad10)"))
    (pad 22 thru_hole oval (at 10.16 3.81 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /COL0))
    (pad 11 thru_hole oval (at -10.16 6.35 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad11)"))
    (pad 23 thru_hole oval (at 10.16 6.35 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /COL1))
    (pad 12 thru_hole oval (at -10.16 8.89 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad12)"))
    (pad 24 thru_hole oval (at 10.16 8.89 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /ROW2))
    (pad 13 thru_hole oval (at -10.16 11.43 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad13)"))
    (pad 25 thru_hole oval (at 10.16 11.43 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /ROW1))
    (pad 14 thru_hole oval (at -10.16 13.97 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad14)"))
    (pad 26 thru_hole oval (at 10.16 13.97 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /ROW0))
    (pad 15 thru_hole oval (at -10.16 16.51 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad15)"))
    (pad 27 thru_hole oval (at 10.16 16.51 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-Pad27)"))
    (pad 16 thru_hole oval (at -10.16 19.05 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(A1-Pad16)"))
    (pad 28 thru_hole oval (at 10.16 19.05 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(A1-Pad28)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module alphadox:MX_SOCKET_FLIP_DIODE (layer F.Cu) (tedit 5B7C1802)
    (at 69 78.5)
    (fp_text reference SW5 (at 0 3.302) (layer F.SilkS))
    (fp_text value 2:1 (at 0 3.302) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 9 "Net-(SW5-Pad2)"))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 9 "Net-(SW5-Pad2)"))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL1))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at 7.36 -2.54) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /ROW2))
    (pad 2 smd rect (at -6.09 -5.08) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(SW5-Pad2)"))
    (pad 2 smd rect (at -7.36 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(SW5-Pad2)"))
    (pad 1 smd rect (at 6.09 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /ROW2))
  )
  (module alphadox:MX_SOCKET_FLIP_DIODE (layer F.Cu) (tedit 5B7C1802)
    (at 69 59.5)
    (fp_text reference SW4 (at 0 3.302) (layer F.SilkS))
    (fp_text value 1:1 (at 0 3.302) (layer B.SilkS))
    (pad 1 smd rect (at 6.09 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 32 /ROW1))
    (pad 2 smd rect (at -7.36 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(SW4-Pad2)"))
    (pad 2 smd rect (at -6.09 -5.08) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(SW4-Pad2)"))
    (pad 1 smd rect (at 7.36 -2.54) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 32 /ROW1))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 8 "Net-(SW4-Pad2)"))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL1))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 8 "Net-(SW4-Pad2)"))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module alphadox:MX_SOCKET_FLIP_DIODE (layer F.Cu) (tedit 5B7C1802)
    (at 69 40.5)
    (fp_text reference SW3 (at 0 3.302) (layer F.SilkS))
    (fp_text value 0:1 (at 0 3.302) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 "Net-(SW3-Pad2)"))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL1))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 "Net-(SW3-Pad2)"))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 /COL1))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at 7.36 -2.54) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /ROW0))
    (pad 2 smd rect (at -6.09 -5.08) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(SW3-Pad2)"))
    (pad 2 smd rect (at -7.36 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(SW3-Pad2)"))
    (pad 1 smd rect (at 6.09 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /ROW0))
  )
  (module alphadox:MX_SOCKET_FLIP_DIODE (layer F.Cu) (tedit 5B7C1802)
    (at 50 78.5)
    (fp_text reference SW2 (at 0 3.302) (layer F.SilkS))
    (fp_text value 2:0 (at 0 3.302) (layer B.SilkS))
    (pad 1 smd rect (at 6.09 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /ROW2))
    (pad 2 smd rect (at -7.36 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(SW2-Pad2)"))
    (pad 2 smd rect (at -6.09 -5.08) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(SW2-Pad2)"))
    (pad 1 smd rect (at 7.36 -2.54) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /ROW2))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL0))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 "Net-(SW2-Pad2)"))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL0))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 "Net-(SW2-Pad2)"))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module alphadox:MX_SOCKET_FLIP_DIODE (layer F.Cu) (tedit 5B7C1802)
    (at 50 50)
    (fp_text reference SW1 (at 0 3.302) (layer F.SilkS))
    (fp_text value 0:0 (at 0 3.302) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 "Net-(SW1-Pad2)"))
    (pad 4 thru_hole rect (at 3.81 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL0))
    (pad 3 thru_hole circle (at -3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 "Net-(SW1-Pad2)"))
    (pad 4 thru_hole rect (at 3.81 7.62) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 /COL0))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at -1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers F.Cu F.Paste F.Mask))
    (pad 99 smd rect (at 1.6637 7.62) (size 0.8382 0.8382) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at 7.36 -2.54) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /ROW0))
    (pad 2 smd rect (at -6.09 -5.08) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at -7.36 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at 6.09 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /ROW0))
  )
  (module alphadox:Feather_M0_Bluefruit (layer F.Cu) (tedit 5B7F5B6B)
    (at 59.69 52.07 270)
    (descr "Through hole straight pin header, 2x16, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x16 2.54mm double row")
    (fp_text reference REF** (at 0 1.27 270) (layer F.SilkS))
    (fp_text value Feather_M0_Bluefruit (at 0 -1.27 270) (layer F.Fab))
    (pad 28 thru_hole oval (at 10.16 19.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at -10.16 19.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 10.16 16.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at -10.16 16.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at 10.16 13.97 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /ROW0))
    (pad 14 thru_hole oval (at -10.16 13.97 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 10.16 11.43 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /ROW1))
    (pad 13 thru_hole oval (at -10.16 11.43 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 10.16 8.89 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /ROW2))
    (pad 12 thru_hole oval (at -10.16 8.89 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 10.16 6.35 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /COL1))
    (pad 11 thru_hole oval (at -10.16 6.35 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 10.16 3.81 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /COL0))
    (pad 10 thru_hole oval (at -10.16 3.81 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 10.16 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at -10.16 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 10.16 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -10.16 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 10.16 -3.81 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at -10.16 -3.81 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 10.16 -6.35 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -10.16 -6.35 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 10.16 -8.89 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at -10.16 -8.89 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -10.16 -11.43 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 3 thru_hole oval (at -10.16 -13.97 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -10.16 -16.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -10.16 -19.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 80.01 31.75) (end 38.1 31.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 38.1 113.03) (end 38.1 31.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 80.01 113.03) (end 38.1 113.03) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 80.01 31.75) (end 80.01 113.03) (layer Edge.Cuts) (width 0.2))
  (zone (net 33) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.1 31.75) (xy 80.01 31.75) (xy 80.01 111.76) (xy 38.1 111.76)
      )
    )
  )
  (zone (net 33) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.1 31.75) (xy 80.01 31.75) (xy 80.01 111.76) (xy 38.1 111.76)
      )
    )
  )
)
