(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 2562)
    (zones 0)
    (modules 228)
    (nets 176)
  )
  (page A4 portrait)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FEFDAE7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VEE)
  (net 3 VCC)
  (net 4 /DSDATA)
  (net 5 "Net-(C50-Pad1)")
  (net 6 /+3V3_A)
  (net 7 "Net-(C48-Pad2)")
  (net 8 /IN4N)
  (net 9 /IN4P)
  (net 10 /IN3N)
  (net 11 /IN3P)
  (net 12 /IN2N)
  (net 13 /IN2P)
  (net 14 /IN1N)
  (net 15 /IN1P)
  (net 16 /FILTR)
  (net 17 /OUT4)
  (net 18 /OUT3)
  (net 19 /OUT2)
  (net 20 /OUT1)
  (net 21 /CS)
  (net 22 /SCK)
  (net 23 /MISO)
  (net 24 /MOSI)
  (net 25 /LRCLK)
  (net 26 /BCLK)
  (net 27 /ASDATA)
  (net 28 "Net-(U$3-PadP$18)")
  (net 29 "Net-(U$3-PadP$17)")
  (net 30 /+3V3)
  (net 31 /RESET)
  (net 32 "Net-(U$3-PadP$9)")
  (net 33 "Net-(U$3-PadP$8)")
  (net 34 "Net-(U$3-PadP$7)")
  (net 35 "Net-(U$3-PadP$6)")
  (net 36 "Net-(R58-Pad1)")
  (net 37 "Net-(C12-Pad1)")
  (net 38 "Net-(J9-PadP2)")
  (net 39 "Net-(C52-Pad1)")
  (net 40 "Net-(J10-PadP2)")
  (net 41 "Net-(C61-Pad1)")
  (net 42 "Net-(J11-PadP2)")
  (net 43 "Net-(C70-Pad1)")
  (net 44 "Net-(J12-PadP2)")
  (net 45 "Net-(C10-Pad2)")
  (net 46 "Net-(J13-PadP2)")
  (net 47 "Net-(C40-Pad2)")
  (net 48 "Net-(J15-PadP2)")
  (net 49 "Net-(C33-Pad2)")
  (net 50 "Net-(J14-PadP2)")
  (net 51 "Net-(C46-Pad2)")
  (net 52 "Net-(J16-PadP2)")
  (net 53 /JOY_Y3)
  (net 54 /JOY_X3)
  (net 55 /SW_3)
  (net 56 /JOY_Y1)
  (net 57 /JOY_X1)
  (net 58 /SW_1)
  (net 59 /JOY_Y2)
  (net 60 /JOY_X2)
  (net 61 /SW_2)
  (net 62 /JOY_Y4)
  (net 63 /JOY_X4)
  (net 64 /SW_4)
  (net 65 /CV_X4)
  (net 66 /CV_Y1)
  (net 67 "Net-(C29-Pad1)")
  (net 68 "Net-(C38-Pad1)")
  (net 69 "Net-(C28-Pad1)")
  (net 70 "Net-(C36-Pad1)")
  (net 71 /CV_Y4)
  (net 72 /CV_X1)
  (net 73 "Net-(J5-PadP3)")
  (net 74 /AREF_-10)
  (net 75 "Net-(J6-PadP3)")
  (net 76 "Net-(J2-PadP3)")
  (net 77 "Net-(J3-PadP3)")
  (net 78 "Net-(J3-PadP2)")
  (net 79 "Net-(J7-PadP3)")
  (net 80 "Net-(J7-PadP2)")
  (net 81 "Net-(J8-PadP3)")
  (net 82 "Net-(J8-PadP2)")
  (net 83 "Net-(J1-PadP3)")
  (net 84 "Net-(J6-PadP2)")
  (net 85 "Net-(J5-PadP2)")
  (net 86 "Net-(J1-PadP2)")
  (net 87 "Net-(J4-PadP3)")
  (net 88 "Net-(J4-PadP2)")
  (net 89 "Net-(J2-PadP2)")
  (net 90 /CV_X3)
  (net 91 /CV_Y2)
  (net 92 "Net-(C4-Pad1)")
  (net 93 "Net-(C26-Pad1)")
  (net 94 "Net-(C5-Pad1)")
  (net 95 "Net-(C14-Pad1)")
  (net 96 /CV_Y3)
  (net 97 /CV_X2)
  (net 98 "Net-(C6-Pad1)")
  (net 99 /+5V)
  (net 100 "Net-(D1-PadA)")
  (net 101 "Net-(D2-PadC)")
  (net 102 "Net-(C9-Pad1)")
  (net 103 "Net-(C7-Pad1)")
  (net 104 "Net-(C10-Pad1)")
  (net 105 "Net-(C7-Pad2)")
  (net 106 "Net-(U$1-PadA26)")
  (net 107 /ATT_Y1)
  (net 108 /ATT_Y4)
  (net 109 /ATT_X2)
  (net 110 /ATT_Y2)
  (net 111 /ATT_Y3)
  (net 112 /ATT_X3)
  (net 113 /ATT_X1)
  (net 114 /LED_1)
  (net 115 /LED_3)
  (net 116 "Net-(U$1-Pad25)")
  (net 117 "Net-(U$1-Pad24)")
  (net 118 "Net-(U$1-Pad3V3_LO)")
  (net 119 "Net-(U$1-Pad0/RX)")
  (net 120 /ATT_X4)
  (net 121 /LED_4)
  (net 122 /LED_2)
  (net 123 "Net-(U$1-Pad2)")
  (net 124 "Net-(U$1-Pad1/TX)")
  (net 125 "Net-(C13-Pad2)")
  (net 126 "Net-(C16-Pad1)")
  (net 127 "Net-(C16-Pad2)")
  (net 128 "Net-(IC11-Pad6)")
  (net 129 "Net-(IC11-Pad7)")
  (net 130 "Net-(C17-Pad1)")
  (net 131 "Net-(C18-Pad1)")
  (net 132 "Net-(LED1-PadA)")
  (net 133 "Net-(LED2-PadA)")
  (net 134 "Net-(LED3-PadA)")
  (net 135 "Net-(LED4-PadA)")
  (net 136 "Net-(C32-Pad1)")
  (net 137 "Net-(C31-Pad1)")
  (net 138 "Net-(C31-Pad2)")
  (net 139 "Net-(C33-Pad1)")
  (net 140 "Net-(C39-Pad1)")
  (net 141 "Net-(C35-Pad1)")
  (net 142 "Net-(C40-Pad1)")
  (net 143 "Net-(C35-Pad2)")
  (net 144 "Net-(C45-Pad1)")
  (net 145 "Net-(C44-Pad1)")
  (net 146 "Net-(C44-Pad2)")
  (net 147 "Net-(C46-Pad1)")
  (net 148 "Net-(C51-Pad1)")
  (net 149 "Net-(C49-Pad2)")
  (net 150 "Net-(C53-Pad2)")
  (net 151 "Net-(C54-Pad1)")
  (net 152 "Net-(C54-Pad2)")
  (net 153 "Net-(IC5-Pad6)")
  (net 154 "Net-(IC5-Pad7)")
  (net 155 "Net-(C55-Pad1)")
  (net 156 "Net-(C56-Pad1)")
  (net 157 "Net-(C62-Pad2)")
  (net 158 "Net-(C63-Pad1)")
  (net 159 "Net-(C63-Pad2)")
  (net 160 "Net-(IC6-Pad6)")
  (net 161 "Net-(IC6-Pad7)")
  (net 162 "Net-(C64-Pad1)")
  (net 163 "Net-(C65-Pad1)")
  (net 164 "Net-(C71-Pad2)")
  (net 165 "Net-(C72-Pad1)")
  (net 166 "Net-(C72-Pad2)")
  (net 167 "Net-(IC8-Pad6)")
  (net 168 "Net-(IC8-Pad7)")
  (net 169 "Net-(C73-Pad1)")
  (net 170 "Net-(C74-Pad1)")
  (net 171 "Net-(D2-PadA)")
  (net 172 "Net-(C1-Pad1)")
  (net 173 "Net-(C23-Pad1)")
  (net 174 "Net-(C25-Pad1)")
  (net 175 "Net-(U$1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /+3V3)
    (add_net /+3V3_A)
    (add_net /+5V)
    (add_net /AREF_-10)
    (add_net /ASDATA)
    (add_net /ATT_X1)
    (add_net /ATT_X2)
    (add_net /ATT_X3)
    (add_net /ATT_X4)
    (add_net /ATT_Y1)
    (add_net /ATT_Y2)
    (add_net /ATT_Y3)
    (add_net /ATT_Y4)
    (add_net /BCLK)
    (add_net /CS)
    (add_net /CV_X1)
    (add_net /CV_X2)
    (add_net /CV_X3)
    (add_net /CV_X4)
    (add_net /CV_Y1)
    (add_net /CV_Y2)
    (add_net /CV_Y3)
    (add_net /CV_Y4)
    (add_net /DSDATA)
    (add_net /FILTR)
    (add_net /IN1N)
    (add_net /IN1P)
    (add_net /IN2N)
    (add_net /IN2P)
    (add_net /IN3N)
    (add_net /IN3P)
    (add_net /IN4N)
    (add_net /IN4P)
    (add_net /JOY_X1)
    (add_net /JOY_X2)
    (add_net /JOY_X3)
    (add_net /JOY_X4)
    (add_net /JOY_Y1)
    (add_net /JOY_Y2)
    (add_net /JOY_Y3)
    (add_net /JOY_Y4)
    (add_net /LED_1)
    (add_net /LED_2)
    (add_net /LED_3)
    (add_net /LED_4)
    (add_net /LRCLK)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /OUT1)
    (add_net /OUT2)
    (add_net /OUT3)
    (add_net /OUT4)
    (add_net /RESET)
    (add_net /SCK)
    (add_net /SW_1)
    (add_net /SW_2)
    (add_net /SW_3)
    (add_net /SW_4)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C31-Pad2)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(C33-Pad2)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C35-Pad2)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C38-Pad1)")
    (add_net "Net-(C39-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C40-Pad1)")
    (add_net "Net-(C40-Pad2)")
    (add_net "Net-(C44-Pad1)")
    (add_net "Net-(C44-Pad2)")
    (add_net "Net-(C45-Pad1)")
    (add_net "Net-(C46-Pad1)")
    (add_net "Net-(C46-Pad2)")
    (add_net "Net-(C48-Pad2)")
    (add_net "Net-(C49-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C50-Pad1)")
    (add_net "Net-(C51-Pad1)")
    (add_net "Net-(C52-Pad1)")
    (add_net "Net-(C53-Pad2)")
    (add_net "Net-(C54-Pad1)")
    (add_net "Net-(C54-Pad2)")
    (add_net "Net-(C55-Pad1)")
    (add_net "Net-(C56-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(C62-Pad2)")
    (add_net "Net-(C63-Pad1)")
    (add_net "Net-(C63-Pad2)")
    (add_net "Net-(C64-Pad1)")
    (add_net "Net-(C65-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C70-Pad1)")
    (add_net "Net-(C71-Pad2)")
    (add_net "Net-(C72-Pad1)")
    (add_net "Net-(C72-Pad2)")
    (add_net "Net-(C73-Pad1)")
    (add_net "Net-(C74-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(D2-PadA)")
    (add_net "Net-(D2-PadC)")
    (add_net "Net-(IC11-Pad6)")
    (add_net "Net-(IC11-Pad7)")
    (add_net "Net-(IC5-Pad6)")
    (add_net "Net-(IC5-Pad7)")
    (add_net "Net-(IC6-Pad6)")
    (add_net "Net-(IC6-Pad7)")
    (add_net "Net-(IC8-Pad6)")
    (add_net "Net-(IC8-Pad7)")
    (add_net "Net-(J1-PadP2)")
    (add_net "Net-(J1-PadP3)")
    (add_net "Net-(J10-PadP2)")
    (add_net "Net-(J11-PadP2)")
    (add_net "Net-(J12-PadP2)")
    (add_net "Net-(J13-PadP2)")
    (add_net "Net-(J14-PadP2)")
    (add_net "Net-(J15-PadP2)")
    (add_net "Net-(J16-PadP2)")
    (add_net "Net-(J2-PadP2)")
    (add_net "Net-(J2-PadP3)")
    (add_net "Net-(J3-PadP2)")
    (add_net "Net-(J3-PadP3)")
    (add_net "Net-(J4-PadP2)")
    (add_net "Net-(J4-PadP3)")
    (add_net "Net-(J5-PadP2)")
    (add_net "Net-(J5-PadP3)")
    (add_net "Net-(J6-PadP2)")
    (add_net "Net-(J6-PadP3)")
    (add_net "Net-(J7-PadP2)")
    (add_net "Net-(J7-PadP3)")
    (add_net "Net-(J8-PadP2)")
    (add_net "Net-(J8-PadP3)")
    (add_net "Net-(J9-PadP2)")
    (add_net "Net-(LED1-PadA)")
    (add_net "Net-(LED2-PadA)")
    (add_net "Net-(LED3-PadA)")
    (add_net "Net-(LED4-PadA)")
    (add_net "Net-(R58-Pad1)")
    (add_net "Net-(U$1-Pad0/RX)")
    (add_net "Net-(U$1-Pad1/TX)")
    (add_net "Net-(U$1-Pad2)")
    (add_net "Net-(U$1-Pad24)")
    (add_net "Net-(U$1-Pad25)")
    (add_net "Net-(U$1-Pad3V3_LO)")
    (add_net "Net-(U$1-Pad7)")
    (add_net "Net-(U$1-PadA26)")
    (add_net "Net-(U$3-PadP$17)")
    (add_net "Net-(U$3-PadP$18)")
    (add_net "Net-(U$3-PadP$6)")
    (add_net "Net-(U$3-PadP$7)")
    (add_net "Net-(U$3-PadP$8)")
    (add_net "Net-(U$3-PadP$9)")
    (add_net VCC)
    (add_net VEE)
  )
  (module orbits_v10:LED3MM (layer Bottom) (tedit 5CF6811F)
    (at 25.527 -70.104)
    (descr "<B>LED</B><p>\n3 mm, round")
    (fp_text reference LED1 (at -2.159 0.508) (layer B.SilkS))
    (fp_text value "" (at 1.905 -1.651) (layer B.SilkS))
    (pad K thru_hole circle (at 1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad A thru_hole circle (at -1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 132 "Net-(LED1-PadA)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:LED3MM (layer Bottom) (tedit 0)
    (at 16.129 -23.114)
    (descr "<B>LED</B><p>\n3 mm, round")
    (fp_text reference LED3 (at 6.985 1.143) (layer B.SilkS))
    (fp_text value "" (at 9.779 -1.397) (layer Cmts.User))
    (pad K thru_hole circle (at 1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad A thru_hole circle (at -1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 134 "Net-(LED3-PadA)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SPARKFUN-ELECTROMECHANICAL_JOYSTICK (layer Bottom) (tedit 5C7AC46B)
    (at 67.31 -11.43 270)
    (fp_text reference U4 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value SPARKFUN-ELECTROMECHANICAL_JOYSTICKPTH (at 0 0 270) (layer B.SilkS) hide)
    (fp_text user >Value (at -5.08 -6.35 270) (layer Cmts.User))
    (fp_text user >Name (at -5.08 -5.08 270) (layer Cmts.User))
    (pad V3 thru_hole circle (at -10.16 -2.54 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad V2 thru_hole circle (at -10.16 0 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 /JOY_Y4) (solder_mask_margin 0.0635))
    (pad V1 thru_hole circle (at -10.16 2.54 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad MOUNT4 thru_hole circle (at 7.62 6.6675 270) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT3 thru_hole circle (at 7.62 -6.6675 270) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT2 thru_hole circle (at -7.62 -6.6675 270) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT1 thru_hole circle (at -7.62 6.6675 270) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad H3 thru_hole circle (at 2.54 -10.16 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad H2 thru_hole circle (at 0 -10.16 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 63 /JOY_X4) (solder_mask_margin 0.0635))
    (pad H1 thru_hole circle (at -2.54 -10.16 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B2B thru_hole circle (at 3.175 7.62 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B2A thru_hole circle (at -3.175 7.62 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B1B thru_hole circle (at 3.175 12.7 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 64 /SW_4) (solder_mask_margin 0.0635))
    (pad B1A thru_hole circle (at -3.175 12.7 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 64 /SW_4) (solder_mask_margin 0.0635))
  )
  (module Crystal:Crystal_SMD_Abracon_ABM3B-4Pin_5.0x3.2mm (layer Top) (tedit 5A0FD1B2)
    (at 45.2816 -106.0004)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3B http://www.abracon.com/Resonators/abm3b.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Q1 (at 2.0132 2.5716) (layer F.SilkS))
    (fp_text value XTAL-4-3225 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -2 -1.2) (size 1.8 1.2) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2 -1.2) (size 1.8 1.2) (layers Top F.Paste F.Mask)
      (net 148 "Net-(C51-Pad1)"))
    (pad 2 smd rect (at 2 1.2) (size 1.8 1.2) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2 1.2) (size 1.8 1.2) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C50-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM3B-4Pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 55.626 -102.0064 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C48 (at 2.54 0.6731) (layer F.SilkS))
    (fp_text value 390p (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 7 "Net-(C48-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 51.308 -97.116 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C68 (at -0.6477 -0.8382 90) (layer F.SilkS))
    (fp_text value 100p (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 8 /IN4N) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 9 /IN4P) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:TEENSY_3.5_3.6_FULL (layer Top) (tedit 0)
    (at 34.29 -80.899 180)
    (fp_text reference U$1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value TEENSY_3.5/3.6_FULL (at 0 0 180) (layer F.SilkS) hide)
    (pad A25 thru_hole circle (at -16.51 4.445 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 60 /JOY_X2) (solder_mask_margin 0.0635))
    (pad A26 thru_hole circle (at -19.05 4.445 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 106 "Net-(U$1-PadA26)") (solder_mask_margin 0.0635))
    (pad A24 thru_hole circle (at 20.32 -2.54 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 53 /JOY_Y3) (solder_mask_margin 0.0635))
    (pad A23 thru_hole circle (at 22.86 -2.54 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 112 /ATT_X3) (solder_mask_margin 0.0635))
    (pad A11 thru_hole circle (at -15.24 -5.08 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 63 /JOY_X4) (solder_mask_margin 0.0635))
    (pad A10 thru_hole circle (at -17.78 -5.08 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 59 /JOY_Y2) (solder_mask_margin 0.0635))
    (pad A22/DAC1 thru_hole circle (at 10.16 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 66 /CV_Y1) (solder_mask_margin 0.0635))
    (pad 21/DAC0 thru_hole circle (at 12.7 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 97 /CV_X2) (solder_mask_margin 0.0635))
    (pad 39/A20 thru_hole circle (at 15.24 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 110 /ATT_Y2) (solder_mask_margin 0.0635))
    (pad 38/A19 thru_hole circle (at 17.78 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 107 /ATT_Y1) (solder_mask_margin 0.0635))
    (pad 37/A18 thru_hole circle (at 20.32 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 91 /CV_Y2) (solder_mask_margin 0.0635))
    (pad 36/A17 thru_hole circle (at 22.86 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 72 /CV_X1) (solder_mask_margin 0.0635))
    (pad 35/A16 thru_hole circle (at 25.4 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 111 /ATT_Y3) (solder_mask_margin 0.0635))
    (pad 34/A15 thru_hole circle (at 27.94 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 56 /JOY_Y1) (solder_mask_margin 0.0635))
    (pad 33/A14 thru_hole circle (at 30.48 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 57 /JOY_X1) (solder_mask_margin 0.0635))
    (pad 32/A13 thru_hole circle (at 30.48 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 54 /JOY_X3) (solder_mask_margin 0.0635))
    (pad 31/A12 thru_hole circle (at 27.94 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 113 /ATT_X1) (solder_mask_margin 0.0635))
    (pad 30 thru_hole circle (at 25.4 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 115 /LED_3) (solder_mask_margin 0.0635))
    (pad 29 thru_hole circle (at 22.86 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 114 /LED_1) (solder_mask_margin 0.0635))
    (pad 28 thru_hole circle (at 20.32 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 55 /SW_3) (solder_mask_margin 0.0635))
    (pad 27 thru_hole circle (at 17.78 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 22 /SCK) (solder_mask_margin 0.0635))
    (pad 26 thru_hole circle (at 15.24 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 58 /SW_1) (solder_mask_margin 0.0635))
    (pad 25 thru_hole circle (at 12.7 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 116 "Net-(U$1-Pad25)") (solder_mask_margin 0.0635))
    (pad 24 thru_hole circle (at 10.16 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 117 "Net-(U$1-Pad24)") (solder_mask_margin 0.0635))
    (pad GND2 thru_hole circle (at 7.62 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3V3 thru_hole circle (at 7.62 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 30 /+3V3) (solder_mask_margin 0.0635))
    (pad VIN thru_hole circle (at -27.94 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 99 /+5V) (solder_mask_margin 0.0635))
    (pad GND thru_hole circle (at -27.94 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad AGND thru_hole circle (at -25.4 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3V3_LO thru_hole circle (at -22.86 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 118 "Net-(U$1-Pad3V3_LO)") (solder_mask_margin 0.0635))
    (pad 0/RX thru_hole circle (at -25.4 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 119 "Net-(U$1-Pad0/RX)") (solder_mask_margin 0.0635))
    (pad 23/A9 thru_hole circle (at -20.32 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 25 /LRCLK) (solder_mask_margin 0.0635))
    (pad 22/A8 thru_hole circle (at -17.78 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 4 /DSDATA) (solder_mask_margin 0.0635))
    (pad 21/A7 thru_hole circle (at -15.24 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 109 /ATT_X2) (solder_mask_margin 0.0635))
    (pad 20/A6 thru_hole circle (at -12.7 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 120 /ATT_X4) (solder_mask_margin 0.0635))
    (pad 19/A5/SCL thru_hole circle (at -10.16 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 62 /JOY_Y4) (solder_mask_margin 0.0635))
    (pad 18/A4/SDA thru_hole circle (at -7.62 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 108 /ATT_Y4) (solder_mask_margin 0.0635))
    (pad 17/A3 thru_hole circle (at -5.08 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 96 /CV_Y3) (solder_mask_margin 0.0635))
    (pad 16/A2 thru_hole circle (at -2.54 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 90 /CV_X3) (solder_mask_margin 0.0635))
    (pad 15/A1 thru_hole circle (at 0 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 71 /CV_Y4) (solder_mask_margin 0.0635))
    (pad 14/A0 thru_hole circle (at 2.54 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 65 /CV_X4) (solder_mask_margin 0.0635))
    (pad 13/SCK thru_hole circle (at 5.08 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 27 /ASDATA) (solder_mask_margin 0.0635))
    (pad 12/MISO thru_hole circle (at 5.08 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 23 /MISO) (solder_mask_margin 0.0635))
    (pad 11/MOSI thru_hole circle (at 2.54 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 24 /MOSI) (solder_mask_margin 0.0635))
    (pad 10/CS thru_hole circle (at 0 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 21 /CS) (solder_mask_margin 0.0635))
    (pad 9/CS thru_hole circle (at -2.54 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 26 /BCLK) (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at -5.08 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 31 /RESET) (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at -7.62 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 175 "Net-(U$1-Pad7)") (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -10.16 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 61 /SW_2) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -12.7 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 64 /SW_4) (solder_mask_margin 0.0635))
    (pad 4/CANRX thru_hole circle (at -15.24 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 121 /LED_4) (solder_mask_margin 0.0635))
    (pad 3/CANTX thru_hole circle (at -17.78 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 122 /LED_2) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -20.32 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 123 "Net-(U$1-Pad2)") (solder_mask_margin 0.0635))
    (pad 1/TX thru_hole circle (at -22.86 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 124 "Net-(U$1-Pad1/TX)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 11.7856 -81.2936 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C44 (at 0.7865 0.9906 270) (layer F.SilkS))
    (fp_text value 68p (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 146 "Net-(C44-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 145 "Net-(C44-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 6.604 -94.83 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R51 (at -0.0245 1.397 270) (layer F.SilkS))
    (fp_text value 49.9k (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 47 "Net-(C40-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 8.89 -94.234 270)
    (fp_text reference J15 (at 4.5 -5 270) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 270) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "Net-(C40-Pad2)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 "Net-(J15-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 23.495 -94.234 270)
    (fp_text reference J16 (at 4.5 -5 270) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 270) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "Net-(C46-Pad2)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 "Net-(J16-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SO08 (layer Top) (tedit 5C7AC4A5)
    (at 17.2628 -100.0506 270)
    (descr "<b>Small Outline Package 8</b><br>\nNS Package M08A")
    (fp_text reference IC9 (at 0.3556 3.9278 90) (layer F.SilkS))
    (fp_text value TL072D (at 3.937 1.905 180) (layer Cmts.User))
    (pad 5 smd rect (at 1.905 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.635 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 137 "Net-(C31-Pad1)") (solder_mask_margin 0.0635))
    (pad 8 smd rect (at -1.905 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 1.905 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 2 VEE) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.635 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -1.905 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 105 "Net-(C7-Pad2)") (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -0.635 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 138 "Net-(C31-Pad2)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -0.635 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 103 "Net-(C7-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 51.4096 -106.26 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C51 (at -2.0456 -1.2192 270) (layer F.SilkS))
    (fp_text value 22p (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 148 "Net-(C51-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 43.9556 -102.87)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C87 (at 1.5104 0.762) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 69.85 -94.234 270)
    (fp_text reference J12 (at 4.5 -5 270) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 270) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(C70-Pad1)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "Net-(J12-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 63.158 -96.3295 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R66 (at 1.0795 0.6985) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 157 "Net-(C62-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 158 "Net-(C63-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 10.5292 -105.6132)
    (descr <b>RESISTOR</b>)
    (fp_text reference R17 (at -0.7484 -0.7493) (layer F.SilkS))
    (fp_text value 604 (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 105 "Net-(C7-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 104 "Net-(C10-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 12.6365 -97.37 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C30 (at 1.4215 -1.4605 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VEE) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 8.89 -103.632 270)
    (fp_text reference J13 (at 4.5 -5 270) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 270) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(C10-Pad2)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "Net-(J13-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 14.9216 -83.6676 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C46 (at -0.674 1.397) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 51 "Net-(C46-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 147 "Net-(C46-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 22.264 -93.98)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C45 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 144 "Net-(C45-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 16.51 -93.638 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C47 (at 0.928 -1.27 270) (layer F.SilkS))
    (fp_text value 2.2n (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 51 "Net-(C46-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 24.765 -104.2026 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R45 (at -2.0964 -0.889 90) (layer F.SilkS))
    (fp_text value 604 (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 138 "Net-(C31-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 139 "Net-(C33-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 54.19 -99.9744 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C49 (at -0.2286 1.2954 180) (layer F.SilkS))
    (fp_text value 5.6n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 149 "Net-(C49-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 38.227 -93.003 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C89 (at 2.071 1.016 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:TQFP-48 (layer Top) (tedit 0)
    (at 37.139 -99.786 180)
    (fp_text reference U$3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value AD1938-QFP (at 0 0 180) (layer F.SilkS) hide)
    (pad P$16 smd rect (at 4.5 1.25) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 4 /DSDATA) (solder_mask_margin 0.0635))
    (pad P$15 smd rect (at 4.5 1.75) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$2 smd rect (at -2.25 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C50-Pad1)") (solder_mask_margin 0.0635))
    (pad P$1 smd rect (at -2.75 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$48 smd rect (at -4.5 2.75 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad P$47 smd rect (at -4.5 2.25 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 7 "Net-(C48-Pad2)") (solder_mask_margin 0.0635))
    (pad P$46 smd rect (at -4.5 1.75 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 8 /IN4N) (solder_mask_margin 0.0635))
    (pad P$45 smd rect (at -4.5 1.25 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 9 /IN4P) (solder_mask_margin 0.0635))
    (pad P$44 smd rect (at -4.5 0.75 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 10 /IN3N) (solder_mask_margin 0.0635))
    (pad P$43 smd rect (at -4.5 0.25 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 11 /IN3P) (solder_mask_margin 0.0635))
    (pad P$42 smd rect (at -4.5 -0.25 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 12 /IN2N) (solder_mask_margin 0.0635))
    (pad P$41 smd rect (at -4.5 -0.75 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 13 /IN2P) (solder_mask_margin 0.0635))
    (pad P$40 smd rect (at -4.5 -1.25 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 14 /IN1N) (solder_mask_margin 0.0635))
    (pad P$39 smd rect (at -4.5 -1.75 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 15 /IN1P) (solder_mask_margin 0.0635))
    (pad P$38 smd rect (at -4.5 -2.25 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 172 "Net-(C1-Pad1)") (solder_mask_margin 0.0635))
    (pad P$37 smd rect (at -4.5 -2.75 180) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad P$36 smd rect (at -2.75 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$35 smd rect (at -2.25 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad P$34 smd rect (at -1.75 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$33 smd rect (at -1.25 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad P$32 smd rect (at -0.75 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$31 smd rect (at -0.25 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 17 /OUT4) (solder_mask_margin 0.0635))
    (pad P$30 smd rect (at 0.25 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 18 /OUT3) (solder_mask_margin 0.0635))
    (pad P$29 smd rect (at 0.75 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 19 /OUT2) (solder_mask_margin 0.0635))
    (pad P$28 smd rect (at 1.25 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 20 /OUT1) (solder_mask_margin 0.0635))
    (pad P$27 smd rect (at 1.75 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 21 /CS) (solder_mask_margin 0.0635))
    (pad P$26 smd rect (at 2.25 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 22 /SCK) (solder_mask_margin 0.0635))
    (pad P$25 smd rect (at 2.75 -4.5 90) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$24 smd rect (at 4.5 -2.75) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 23 /MISO) (solder_mask_margin 0.0635))
    (pad P$23 smd rect (at 4.5 -2.25) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 24 /MOSI) (solder_mask_margin 0.0635))
    (pad P$22 smd rect (at 4.5 -1.75) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 25 /LRCLK) (solder_mask_margin 0.0635))
    (pad P$21 smd rect (at 4.5 -1.25) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 26 /BCLK) (solder_mask_margin 0.0635))
    (pad P$20 smd rect (at 4.5 -0.75) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 27 /ASDATA) (solder_mask_margin 0.0635))
    (pad P$19 smd rect (at 4.5 -0.25) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$18 smd rect (at 4.5 0.25) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 28 "Net-(U$3-PadP$18)") (solder_mask_margin 0.0635))
    (pad P$17 smd rect (at 4.5 0.75) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 29 "Net-(U$3-PadP$17)") (solder_mask_margin 0.0635))
    (pad P$14 smd rect (at 4.5 2.25) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$13 smd rect (at 4.5 2.75) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 30 /+3V3) (solder_mask_margin 0.0635))
    (pad P$12 smd rect (at 2.75 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$11 smd rect (at 2.25 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$10 smd rect (at 1.75 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 31 /RESET) (solder_mask_margin 0.0635))
    (pad P$9 smd rect (at 1.25 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 32 "Net-(U$3-PadP$9)") (solder_mask_margin 0.0635))
    (pad P$8 smd rect (at 0.75 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 33 "Net-(U$3-PadP$8)") (solder_mask_margin 0.0635))
    (pad P$7 smd rect (at 0.25 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 34 "Net-(U$3-PadP$7)") (solder_mask_margin 0.0635))
    (pad P$6 smd rect (at -0.25 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 35 "Net-(U$3-PadP$6)") (solder_mask_margin 0.0635))
    (pad P$5 smd rect (at -0.75 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad P$4 smd rect (at -1.25 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad P$3 smd rect (at -1.75 4.5 270) (size 1 0.254) (layers Top F.Paste F.Mask)
      (net 36 "Net-(R58-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 42.252 -41.275 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C26 (at -0.42 1.27) (layer F.SilkS))
    (fp_text value 10n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 91 /CV_Y2) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 93 "Net-(C26-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 63.5 -99.187 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C63 (at -0.8255 1.3335 90) (layer F.SilkS))
    (fp_text value 120p (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 159 "Net-(C63-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 158 "Net-(C63-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 23.495 -103.632 270)
    (fp_text reference J14 (at 4.5 -5 270) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 270) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 "Net-(C33-Pad2)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 "Net-(J14-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 26.3516 -101.4476)
    (descr <b>RESISTOR</b>)
    (fp_text reference R44 (at -0.9516 1.3716 -180) (layer F.SilkS))
    (fp_text value 10k (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 136 "Net-(C32-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 138 "Net-(C31-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 40.005 -93.003 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C96 (at 0.166 -1.4605 270) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 3.937 -91.528 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C40 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 47 "Net-(C40-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 142 "Net-(C40-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SPARKFUN-ELECTROMECHANICAL_JOYSTICK (layer Bottom) (tedit 5C7AC46B)
    (at 11.43 -63.119 90)
    (fp_text reference U1 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value SPARKFUN-ELECTROMECHANICAL_JOYSTICKPTH (at 0 0 90) (layer B.SilkS) hide)
    (fp_text user >Value (at -5.08 -6.35 90) (layer Cmts.User))
    (fp_text user >Name (at -5.08 -5.08 90) (layer Cmts.User))
    (pad V3 thru_hole circle (at -10.16 -2.54 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad V2 thru_hole circle (at -10.16 0 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 56 /JOY_Y1) (solder_mask_margin 0.0635))
    (pad V1 thru_hole circle (at -10.16 2.54 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad MOUNT4 thru_hole circle (at 7.62 6.6675 90) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT3 thru_hole circle (at 7.62 -6.6675 90) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT2 thru_hole circle (at -7.62 -6.6675 90) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT1 thru_hole circle (at -7.62 6.6675 90) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad H3 thru_hole circle (at 2.54 -10.16 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad H2 thru_hole circle (at 0 -10.16 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 57 /JOY_X1) (solder_mask_margin 0.0635))
    (pad H1 thru_hole circle (at -2.54 -10.16 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B2B thru_hole circle (at 3.175 7.62 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B2A thru_hole circle (at -3.175 7.62 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B1B thru_hole circle (at 3.175 12.7 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 /SW_1) (solder_mask_margin 0.0635))
    (pad B1A thru_hole circle (at -3.175 12.7 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 /SW_1) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:9MM_SNAP-IN_POT (layer Bottom) (tedit 5C7AC443)
    (at 71.628 -30.607 180)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VR3 (at -3.81 2.54 180) (layer B.SilkS))
    (fp_text value 9MM_SNAP-IN_POT_ (at -3.81 -3.81 180) (layer Cmts.User))
    (pad CHASSIS2 thru_hole rect (at 4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad CHASSIS1 thru_hole rect (at -4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 120 /ATT_X4) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at -2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SO14 (layer Top) (tedit 5C78AC32)
    (at 34.29 -35.687 180)
    (descr "<b>Small Outline package</b> 150 mil")
    (fp_text reference IC7 (at 4.7625 -1.2065) (layer F.SilkS))
    (fp_text value MCP6004 (at -3.556 0.635) (layer Cmts.User))
    (pad 8 smd rect (at 3.81 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 65 /CV_X4) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 3.81 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 66 /CV_Y1) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 2.54 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 67 "Net-(C29-Pad1)") (solder_mask_margin 0.0635))
    (pad 10 smd rect (at 1.27 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 2.54 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 68 "Net-(C38-Pad1)") (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 1.27 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 0 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 0 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 12 smd rect (at -1.27 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 13 smd rect (at -2.54 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 69 "Net-(C28-Pad1)") (solder_mask_margin 0.0635))
    (pad 3 smd rect (at -1.27 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -2.54 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 70 "Net-(C36-Pad1)") (solder_mask_margin 0.0635))
    (pad 14 smd rect (at -3.81 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 71 /CV_Y4) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -3.81 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 72 /CV_X1) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SO14 (layer Top) (tedit 5C78AC32)
    (at 45.466 -35.814 180)
    (descr "<b>Small Outline package</b> 150 mil")
    (fp_text reference IC2 (at -4.6355 -1.905) (layer F.SilkS))
    (fp_text value MCP6004 (at -3.556 0.635) (layer Cmts.User))
    (pad 8 smd rect (at 3.81 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 90 /CV_X3) (solder_mask_margin 0.0635))
    (pad 7 smd rect (at 3.81 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 91 /CV_Y2) (solder_mask_margin 0.0635))
    (pad 9 smd rect (at 2.54 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 92 "Net-(C4-Pad1)") (solder_mask_margin 0.0635))
    (pad 10 smd rect (at 1.27 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 2.54 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 93 "Net-(C26-Pad1)") (solder_mask_margin 0.0635))
    (pad 5 smd rect (at 1.27 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 11 smd rect (at 0 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 0 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 12 smd rect (at -1.27 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 13 smd rect (at -2.54 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 94 "Net-(C5-Pad1)") (solder_mask_margin 0.0635))
    (pad 3 smd rect (at -1.27 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -2.54 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 95 "Net-(C14-Pad1)") (solder_mask_margin 0.0635))
    (pad 14 smd rect (at -3.81 -3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 96 /CV_Y3) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -3.81 3.0734 180) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 97 /CV_X2) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 67.476 -77.724 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C6 (at 0.928 0.889 180) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 98 "Net-(C6-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SPARKFUN-ELECTROMECHANICAL_JOYSTICK (layer Bottom) (tedit 5C7AC46B)
    (at 67.31 -63.119 270)
    (fp_text reference U2 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value SPARKFUN-ELECTROMECHANICAL_JOYSTICKPTH (at 0 0 270) (layer B.SilkS) hide)
    (fp_text user >Value (at -5.08 -6.35 270) (layer Cmts.User))
    (fp_text user >Name (at -5.08 -5.08 270) (layer Cmts.User))
    (pad V3 thru_hole circle (at -10.16 -2.54 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad V2 thru_hole circle (at -10.16 0 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 59 /JOY_Y2) (solder_mask_margin 0.0635))
    (pad V1 thru_hole circle (at -10.16 2.54 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad MOUNT4 thru_hole circle (at 7.62 6.6675 270) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT3 thru_hole circle (at 7.62 -6.6675 270) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT2 thru_hole circle (at -7.62 -6.6675 270) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT1 thru_hole circle (at -7.62 6.6675 270) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad H3 thru_hole circle (at 2.54 -10.16 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad H2 thru_hole circle (at 0 -10.16 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 60 /JOY_X2) (solder_mask_margin 0.0635))
    (pad H1 thru_hole circle (at -2.54 -10.16 270) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B2B thru_hole circle (at 3.175 7.62 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B2A thru_hole circle (at -3.175 7.62 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B1B thru_hole circle (at 3.175 12.7 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 /SW_2) (solder_mask_margin 0.0635))
    (pad B1A thru_hole circle (at -3.175 12.7 270) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 /SW_2) (solder_mask_margin 0.0635))
  )
  (module Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT (layer Top) (tedit 5B741BB0)
    (at 69.977 -52.324 180)
    (descr "DCDC-Converter, RECOM, RECOM_R-78E-0.5, SIP-3, pitch 2.54mm, package size 11.6x8.5x10.4mm^3, https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf")
    (tags "dc-dc recom buck sip-3 pitch 2.54mm")
    (fp_text reference U5 (at 2.54 -7.55 180) (layer F.SilkS))
    (fp_text value R-78E5.0-0.5 (at 2 3.5 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.25 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 99 /+5V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 174 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R-78E-0.5_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module orbits_v10:SPARKFUN-ELECTROMECHANICAL_JOYSTICK (layer Bottom) (tedit 5C7AC46B)
    (at 11.43 -11.43 90)
    (fp_text reference U3 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value SPARKFUN-ELECTROMECHANICAL_JOYSTICKPTH (at 0 0 90) (layer B.SilkS) hide)
    (fp_text user >Value (at -5.08 -6.35 90) (layer Cmts.User))
    (fp_text user >Name (at -5.08 -5.08 90) (layer Cmts.User))
    (pad V3 thru_hole circle (at -10.16 -2.54 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad V2 thru_hole circle (at -10.16 0 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 53 /JOY_Y3) (solder_mask_margin 0.0635))
    (pad V1 thru_hole circle (at -10.16 2.54 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad MOUNT4 thru_hole circle (at 7.62 6.6675 90) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT3 thru_hole circle (at 7.62 -6.6675 90) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT2 thru_hole circle (at -7.62 -6.6675 90) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad MOUNT1 thru_hole circle (at -7.62 6.6675 90) (size 2.0955 2.0955) (drill 1.397) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad H3 thru_hole circle (at 2.54 -10.16 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad H2 thru_hole circle (at 0 -10.16 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 54 /JOY_X3) (solder_mask_margin 0.0635))
    (pad H1 thru_hole circle (at -2.54 -10.16 90) (size 1.3335 1.3335) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B2B thru_hole circle (at 3.175 7.62 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B2A thru_hole circle (at -3.175 7.62 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad B1B thru_hole circle (at 3.175 12.7 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 /SW_3) (solder_mask_margin 0.0635))
    (pad B1A thru_hole circle (at -3.175 12.7 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 /SW_3) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 37.846 -46.14 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C15 (at -0.5724 1.27 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 -90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 34.29 -41.744 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C19 (at -0.635 -0.8255 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 35.902 -27.686)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C28 (at 1.563 0.381) (layer F.SilkS))
    (fp_text value 10n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 71 /CV_Y4) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 69 "Net-(C28-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 27.813 -27.559 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C29 (at 1.397 0.889) (layer F.SilkS))
    (fp_text value 10n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 65 /CV_X4) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 67 "Net-(C29-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 27.559 -53.848 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C36 (at -0.508 1.2065 180) (layer F.SilkS))
    (fp_text value 10n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 72 /CV_X1) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 70 "Net-(C36-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 45.466 -41.744 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C37 (at -0.85 1.524 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 25.058 -39.37)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C38 (at -0.547 -0.8255) (layer F.SilkS))
    (fp_text value 10n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 66 /CV_Y1) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 68 "Net-(C38-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SOD123 (layer Top) (tedit 5C78AD6B)
    (at 43.561 -50.8 270)
    (descr <b>Diode</b>)
    (fp_text reference D1 (at -1.016 -1.016 270) (layer F.SilkS))
    (fp_text value 1N5819HW (at -1.1 2.3 270) (layer Cmts.User))
    (pad A smd rect (at 1.9 0 270) (size 1.4 1.4) (layers Top F.Paste F.Mask)
      (net 100 "Net-(D1-PadA)") (solder_mask_margin 0.0635))
    (pad C smd rect (at -1.9 0 270) (size 1.4 1.4) (layers Top F.Paste F.Mask)
      (net 173 "Net-(C23-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SOD123 (layer Top) (tedit 5C78AD6B)
    (at 35.433 -54.864 270)
    (descr <b>Diode</b>)
    (fp_text reference D2 (at 1.9685 1.016 90) (layer F.SilkS))
    (fp_text value 1N5819HW (at -1.1 2.3 90) (layer Cmts.User))
    (pad A smd rect (at 1.9 0 270) (size 1.4 1.4) (layers Top F.Paste F.Mask)
      (net 171 "Net-(D2-PadA)") (solder_mask_margin 0.0635))
    (pad C smd rect (at -1.9 0 270) (size 1.4 1.4) (layers Top F.Paste F.Mask)
      (net 101 "Net-(D2-PadC)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:DBZ_R-PDSO-G3 (layer Top) (tedit 5C78ACC5)
    (at 40.894 -45.974 270)
    (descr "<b>DBZ (R-PDSO-G3)</b> SOT-23<p>\nSource: http://focus.ti.com/lit/ds/slcs146e/slcs146e.pdf")
    (fp_text reference IC3 (at 1.397 -3.175 270) (layer F.SilkS))
    (fp_text value LM4040B10 (at -1.905 3.175 270) (layer Cmts.User))
    (pad 1 smd rect (at -0.95 1.1 270) (size 0.7 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.95 1.1 270) (size 0.7 1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0 -1.1 270) (size 0.7 1) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 22.86 -30.607 270)
    (fp_text reference J5 (at -1.397 -5 270) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 270) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "Net-(J5-PadP3)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 85 "Net-(J5-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 46.736 -50.165 180)
    (fp_text reference J4 (at 4.5 -5 180) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 180) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 "Net-(J4-PadP3)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 88 "Net-(J4-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 32.004 -50.165 180)
    (fp_text reference J2 (at -1.905 -5.08 180) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 180) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "Net-(J2-PadP3)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 "Net-(J2-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 55.88 -43.942 90)
    (fp_text reference J3 (at -3.683 -6.35 90) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 90) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "Net-(J3-PadP3)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 "Net-(J3-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 55.88 -30.607 90)
    (fp_text reference J7 (at 2.54 -6.096 90) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 90) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 "Net-(J7-PadP3)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(J7-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 46.736 -24.384)
    (fp_text reference J8 (at -3.683 -6.096) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 "Net-(J8-PadP3)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 "Net-(J8-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 32.004 -24.384)
    (fp_text reference J6 (at 2.54 -6.096) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "Net-(J6-PadP3)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 "Net-(J6-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 22.86 -43.942 270)
    (fp_text reference J1 (at 4.5 -5 270) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 270) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 "Net-(J1-PadP3)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 86 "Net-(J1-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:AVR_ICSP (layer Top) (tedit 5C78ADA2)
    (at 39.37 -54.356 180)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference JP3 (at -3.302 3.683 270) (layer F.SilkS))
    (fp_text value M05X2PTH (at -2.794 0.254 270) (layer Cmts.User))
    (pad 10 thru_hole circle (at 1.27 5.08 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 101 "Net-(D2-PadC)") (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at -1.27 5.08 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 101 "Net-(D2-PadC)") (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.27 2.54 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at -1.27 2.54 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at 1.27 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -1.27 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at 1.27 -2.54 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -1.27 -2.54 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 1.27 -5.08 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 100 "Net-(D1-PadA)") (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -1.27 -5.08 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 100 "Net-(D1-PadA)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:0603 (layer Top) (tedit 5C7AC422)
    (at 43.307 -55.626 270)
    (descr "Multilayer SMD")
    (fp_text reference L1 (at 0.3175 -1.3335 90) (layer F.SilkS))
    (fp_text value WE-CBF_0603 (at -1.5875 -0.635 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.7 0 270) (size 0.85 0.7) (layers Top F.Paste F.Mask)
      (net 173 "Net-(C23-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.9 0 270) (size 0.85 0.7) (layers Top F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:0603 (layer Top) (tedit 5C7AC422)
    (at 35.433 -50.546 90)
    (descr "Multilayer SMD")
    (fp_text reference L2 (at -0.3175 1.2065 90) (layer F.SilkS))
    (fp_text value WE-CBF_0603 (at -1.5875 -0.635 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.7 0 90) (size 0.85 0.7) (layers Top F.Paste F.Mask)
      (net 171 "Net-(D2-PadA)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.9 0 90) (size 0.85 0.7) (layers Top F.Paste F.Mask)
      (net 2 VEE) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 35.56 -46.14 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R12 (at 0.547 -1.397 90) (layer F.SilkS))
    (fp_text value 1k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 2 VEE) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 34.29 -25.058 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R21 (at -0.596 1.3335 90) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 75 "Net-(J6-PadP3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 69 "Net-(C28-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 24.511 -26.924 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R22 (at -1.0795 -0.889 90) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 73 "Net-(J5-PadP3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 67 "Net-(C29-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 36.449 -25.058 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R23 (at -0.6595 -0.889 90) (layer F.SilkS))
    (fp_text value 120k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 69 "Net-(C28-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 28.956 -22.479 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R24 (at -0.8255 -1.016 90) (layer F.SilkS))
    (fp_text value 120k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 67 "Net-(C29-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 35.941 -29.845 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R25 (at -1.5875 -0.254) (layer F.SilkS))
    (fp_text value 20k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 69 "Net-(C28-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 71 /CV_Y4) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 27.813 -25.273)
    (descr <b>RESISTOR</b>)
    (fp_text reference R26 (at -0.127 0.889) (layer F.SilkS))
    (fp_text value 20k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 67 "Net-(C29-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 65 /CV_X4) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 26.074 -55.88)
    (descr <b>RESISTOR</b>)
    (fp_text reference R31 (at -0.635 -0.635 -180) (layer F.SilkS))
    (fp_text value 20k (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 70 "Net-(C36-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 72 /CV_X1) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 28.1686 -37.846 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R32 (at 1.7526 0.127) (layer F.SilkS))
    (fp_text value 20k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 68 "Net-(C38-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 66 /CV_Y1) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 29.376 -55.88)
    (descr <b>RESISTOR</b>)
    (fp_text reference R34 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 76 "Net-(J2-PadP3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 70 "Net-(C36-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 21.248 -40.132 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R35 (at 0.293 0.8255) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 83 "Net-(J1-PadP3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 68 "Net-(C38-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 37.504 -43.688)
    (descr <b>RESISTOR</b>)
    (fp_text reference R36 (at -0.166 0.762 -180) (layer F.SilkS))
    (fp_text value 120k (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 70 "Net-(C36-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 28.155 -35.941)
    (descr <b>RESISTOR</b>)
    (fp_text reference R37 (at -1.739 -0.254 -180) (layer F.SilkS))
    (fp_text value 120k (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 68 "Net-(C38-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 55.245 -103.632 90)
    (fp_text reference J9 (at -4.191 6.35 90) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 90) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(C12-Pad1)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(J9-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 69.85 -103.632 90)
    (fp_text reference J10 (at -4.445 6.477 90) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 90) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(C52-Pad1)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(J10-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:OG-PJ301_WQP_PJ_301M6 (layer Bottom) (tedit 0)
    (at 55.245 -94.234 270)
    (fp_text reference J11 (at 4.5 -5 270) (layer B.SilkS))
    (fp_text value OG-PJ301_PJ301_THONKICONN6 (at 0 0 270) (layer B.SilkS) hide)
    (pad P3 thru_hole circle (at 0 4.445 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(C61-Pad1)") (solder_mask_margin 0.0635))
    (pad P2 thru_hole circle (at 0 -3.175 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(J11-PadP2)") (solder_mask_margin 0.0635))
    (pad P1 thru_hole circle (at 0 -5.715 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 44.577 -25.146 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R1 (at -0.635 -0.8255 90) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 81 "Net-(J8-PadP3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 92 "Net-(C4-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 42.965 -27.813)
    (descr <b>RESISTOR</b>)
    (fp_text reference R3 (at -3.087 0.381) (layer F.SilkS))
    (fp_text value 20k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 92 "Net-(C4-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 90 /CV_X3) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 42.418 -25.185 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R4 (at 0.547 0.8255 270) (layer F.SilkS))
    (fp_text value 120k (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 92 "Net-(C4-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 42.965 -29.972 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C4 (at 3.087 -0.381) (layer F.SilkS))
    (fp_text value 10n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 90 /CV_X3) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 92 "Net-(C4-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 55.411 -28.194)
    (descr <b>RESISTOR</b>)
    (fp_text reference R5 (at -0.635 -0.762) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 79 "Net-(J7-PadP3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 94 "Net-(C5-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 51.689 -25.019 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R6 (at 0.127 -1.651) (layer F.SilkS))
    (fp_text value 20k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 94 "Net-(C5-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 96 /CV_Y3) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 48.641 -22.313 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R7 (at -0.635 -0.889 90) (layer F.SilkS))
    (fp_text value 120k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 94 "Net-(C5-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 51.689 -27.432)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C5 (at -0.381 -0.762) (layer F.SilkS))
    (fp_text value 10n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 96 /CV_Y3) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 94 "Net-(C5-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 51.777 -41.529)
    (descr <b>RESISTOR</b>)
    (fp_text reference R8 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 77 "Net-(J3-PadP3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 95 "Net-(C14-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 49.364 -46.228 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R9 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 20k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 95 "Net-(C14-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 97 /CV_X2) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 49.364 -48.26)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C14 (at 0.166 -1.3335) (layer F.SilkS))
    (fp_text value 10n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 97 /CV_X2) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 95 "Net-(C14-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 51.777 -39.37)
    (descr <b>RESISTOR</b>)
    (fp_text reference R10 (at 0.801 1.016 -180) (layer F.SilkS))
    (fp_text value 120k (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 95 "Net-(C14-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 46.6725 -51.093 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R11 (at 0.596 0.889 90) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 87 "Net-(J4-PadP3)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 93 "Net-(C26-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 42.252 -43.434)
    (descr <b>RESISTOR</b>)
    (fp_text reference R13 (at -1.104 -0.762) (layer F.SilkS))
    (fp_text value 20k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 93 "Net-(C26-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 91 /CV_Y2) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 38.95 -41.656 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R14 (at 0.85 -1.524) (layer F.SilkS))
    (fp_text value 120k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 74 /AREF_-10) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 93 "Net-(C26-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SOT223 (layer Top) (tedit 5C78AD7F)
    (at 73.8124 -79.248 270)
    (descr "<b>Smal Outline Transistor</b>")
    (fp_text reference IC4 (at 3.302 -1.6256) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at -2.794 5.842 90) (layer Cmts.User))
    (pad 4 smd rect (at 0 -3.1496 270) (size 3.81 2.0066) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 2.3114 3.1496 270) (size 1.4986 2.0066) (layers Top F.Paste F.Mask)
      (net 98 "Net-(C6-Pad1)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at 0.0254 3.1496 270) (size 1.4986 2.0066) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -2.2606 3.1496 270) (size 1.4986 2.0066) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 22.9752 -98.2218)
    (descr <b>RESISTOR</b>)
    (fp_text reference R15 (at -0.635 -0.635 -180) (layer F.SilkS))
    (fp_text value 1.65k (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 20 /OUT1) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 102 "Net-(C9-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 7.0476 -101.5238 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R16 (at 0.8246 0.7112) (layer F.SilkS))
    (fp_text value 3.32k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 102 "Net-(C9-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 103 "Net-(C7-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 7.0612 -103.5812 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R18 (at 0.8382 0.7493 180) (layer F.SilkS))
    (fp_text value 10k (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 102 "Net-(C9-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 105 "Net-(C7-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 4.572 -100.6484 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R19 (at 3.3029 -0.3175 270) (layer F.SilkS))
    (fp_text value 49.9k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 45 "Net-(C10-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 9.8552 -102.2486 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C7 (at -0.7756 1.4478 270) (layer F.SilkS))
    (fp_text value 68p (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 105 "Net-(C7-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 103 "Net-(C7-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 7.0494 -99.441)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C9 (at -0.5724 1.397) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 102 "Net-(C9-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 7.0476 -105.6132 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C10 (at -0.889 1.27) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 45 "Net-(C10-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 104 "Net-(C10-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 2.7432 -100.6484 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C11 (at 1.5884 0.3937 270) (layer F.SilkS))
    (fp_text value 2.2n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 45 "Net-(C10-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 74.676 -106.26 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R20 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 125 "Net-(C13-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 126 "Net-(C16-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 76.2 -91.274 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R27 (at 0.7865 0.6985 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 126 "Net-(C16-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 127 "Net-(C16-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 63.627 -85.559 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R28 (at -0.635 -0.8255 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 128 "Net-(IC11-Pad6)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 127 "Net-(C16-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 65.532 -85.559 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R29 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 128 "Net-(IC11-Pad6)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 129 "Net-(IC11-Pad7)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 67.4125 -89.408 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R30 (at 0.928 0.6985 180) (layer F.SilkS))
    (fp_text value 237 (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 127 "Net-(C16-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 130 "Net-(C17-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 70.954 -89.408 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R33 (at 1.612 0.6985 180) (layer F.SilkS))
    (fp_text value 237 (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 129 "Net-(IC11-Pad7)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 131 "Net-(C18-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 68.58 -106.26 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R38 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 37 "Net-(C12-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 70.612 -106.26 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C12 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 180p (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 37 "Net-(C12-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 72.644 -106.26 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C13 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 125 "Net-(C13-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 37 "Net-(C12-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 74.295 -91.274 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C16 (at -0.85 -0.6985 90) (layer F.SilkS))
    (fp_text value 120p (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 127 "Net-(C16-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 126 "Net-(C16-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 67.4125 -91.44 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C17 (at -0.9135 1.3335) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 11 /IN3P) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 130 "Net-(C17-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 70.954 -91.44 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C18 (at 1.6755 0.762) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 10 /IN3N) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 131 "Net-(C18-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 62.2545 -91.313)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C20 (at 0.7375 -1.397) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 11 /IN3P) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 58.8908 -92.1512 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C21 (at 1.2328 -1.3462) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 10 /IN3N) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 54.5592 -91.4273 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C22 (at -0.8128 -0.8128 180) (layer F.SilkS))
    (fp_text value 100p (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 10 /IN3N) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 11 /IN3P) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:0603 (layer Top) (tedit 5C7AC422)
    (at 67.7308 -75.8444 180)
    (descr "Multilayer SMD")
    (fp_text reference L3 (at 1.7035 -1.27 180) (layer F.SilkS))
    (fp_text value WE-CBF_0603 (at -1.5875 -0.635 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.7 0 180) (size 0.85 0.7) (layers Top F.Paste F.Mask)
      (net 98 "Net-(C6-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.9 0 180) (size 0.85 0.7) (layers Top F.Paste F.Mask)
      (net 173 "Net-(C23-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 67.476 -80.01 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C24 (at 1.055 0.762 180) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:LED3MM (layer Bottom) (tedit 0)
    (at 57.0992 -54.5592 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (fp_text reference LED2 (at -2.286 -3.81 180) (layer B.SilkS))
    (fp_text value "" (at 1.905 -1.651 180) (layer B.SilkS))
    (pad K thru_hole circle (at 1.27 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad A thru_hole circle (at -1.27 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 133 "Net-(LED2-PadA)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:LED3MM (layer Bottom) (tedit 0)
    (at 55.753 -3.048 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (fp_text reference LED4 (at -6.477 -2.032 180) (layer B.SilkS))
    (fp_text value "" (at 1.905 -1.651 180) (layer B.SilkS))
    (pad K thru_hole circle (at 1.27 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad A thru_hole circle (at -1.27 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 135 "Net-(LED4-PadA)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 21.297 -70.104)
    (descr <b>RESISTOR</b>)
    (fp_text reference R2 (at 0.1025 0.889 -180) (layer F.SilkS))
    (fp_text value 2.2k (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 132 "Net-(LED1-PadA)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 114 /LED_1) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 59.309 -62.904 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R39 (at 0.7375 -1.524 270) (layer F.SilkS))
    (fp_text value 2.2k (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 133 "Net-(LED2-PadA)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 122 /LED_2) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 16.129 -26.416 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R40 (at -0.6985 -0.8255 90) (layer F.SilkS))
    (fp_text value 2.2k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 134 "Net-(LED3-PadA)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 115 /LED_3) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 65.0104 -9.144 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R41 (at -0.547 -0.8255) (layer F.SilkS))
    (fp_text value 2.2k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 135 "Net-(LED4-PadA)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 121 /LED_4) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 16.764 -103.974 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C27 (at 1.9694 -1.5494 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 26.328 -97.2312 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R42 (at -0.85 -0.8382 180) (layer F.SilkS))
    (fp_text value 1.65k (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 19 /OUT2) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 136 "Net-(C32-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 26.328 -99.314)
    (descr <b>RESISTOR</b>)
    (fp_text reference R43 (at -0.928 1.3335 -180) (layer F.SilkS))
    (fp_text value 3.32k (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 136 "Net-(C32-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 137 "Net-(C31-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 23.4696 -101.0294 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C31 (at -0.635 -0.8001 90) (layer F.SilkS))
    (fp_text value 68p (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 138 "Net-(C31-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 137 "Net-(C31-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 29.0068 -100.418 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C32 (at -1.0296 1.4097 90) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 136 "Net-(C32-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 18.962 -106.172 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R46 (at 0.9788 0.6604) (layer F.SilkS))
    (fp_text value 49.9k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 49 "Net-(C33-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 21.9846 -103.7844 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C33 (at -0.9389 1.2446) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 49 "Net-(C33-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 139 "Net-(C33-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 22.2622 -105.918)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C34 (at -0.9262 -0.6985 -180) (layer F.SilkS))
    (fp_text value 2.2n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 49 "Net-(C33-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 21.932 -96.012)
    (descr <b>RESISTOR</b>)
    (fp_text reference R47 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 1.65k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 18 /OUT3) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 140 "Net-(C39-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 10.0838 -91.528 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R48 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 3.32k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 140 "Net-(C39-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 141 "Net-(C35-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 5.969 -91.528 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R49 (at 0.6595 0.762 90) (layer F.SilkS))
    (fp_text value 604 (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 143 "Net-(C35-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 142 "Net-(C40-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 8.0264 -91.528 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R50 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 10k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 140 "Net-(C39-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 143 "Net-(C35-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 8.47 -86.106)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C35 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 68p (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 143 "Net-(C35-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 141 "Net-(C35-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 17.946 -96.774 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C39 (at 0.4835 -1.3335 180) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 140 "Net-(C39-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 8.6995 -94.83 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C41 (at -0.0245 1.3335 90) (layer F.SilkS))
    (fp_text value 2.2n (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 47 "Net-(C40-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 7.9765 -76.581 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C42 (at -0.088 -1.4605 180) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 22.264 -92.202)
    (descr <b>RESISTOR</b>)
    (fp_text reference R52 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 1.65k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 17 /OUT4) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 144 "Net-(C45-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 11.6976 -83.82)
    (descr <b>RESISTOR</b>)
    (fp_text reference R53 (at -0.8881 -0.8636) (layer F.SilkS))
    (fp_text value 3.32k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 144 "Net-(C45-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 145 "Net-(C44-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 13.8938 -81.2936 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R54 (at -0.7865 -0.8128 90) (layer F.SilkS))
    (fp_text value 10k (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 144 "Net-(C45-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 146 "Net-(C44-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 15.9512 -81.2936 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R55 (at 0.7375 0.762 90) (layer F.SilkS))
    (fp_text value 604 (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 146 "Net-(C44-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 147 "Net-(C46-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 12.7644 -92.1004)
    (descr <b>RESISTOR</b>)
    (fp_text reference R56 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 49.9k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 51 "Net-(C46-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SO08 (layer Top) (tedit 5C7AC4A5)
    (at 7.366 -81.2165 180)
    (descr "<b>Small Outline Package 8</b><br>\nNS Package M08A")
    (fp_text reference IC10 (at 2.413 2.8575) (layer F.SilkS))
    (fp_text value TL072D (at 3.937 1.905 270) (layer Cmts.User))
    (pad 5 smd rect (at 1.905 -2.6 180) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.635 -2.6 180) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 145 "Net-(C44-Pad1)") (solder_mask_margin 0.0635))
    (pad 8 smd rect (at -1.905 -2.6 180) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 1.905 2.6 180) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 2 VEE) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.635 2.6 180) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -1.905 2.6 180) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 143 "Net-(C35-Pad2)") (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -0.635 -2.6 180) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 146 "Net-(C44-Pad2)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -0.635 2.6 180) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 141 "Net-(C35-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SO08 (layer Top) (tedit 5C7AC4A5)
    (at 70.672 -85.725 90)
    (descr "<b>Small Outline Package 8</b><br>\nNS Package M08A")
    (fp_text reference IC11 (at -1.905 0.956 -90) (layer F.SilkS))
    (fp_text value TL072D (at 3.937 1.905) (layer Cmts.User))
    (pad 5 smd rect (at 1.905 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.635 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 128 "Net-(IC11-Pad6)") (solder_mask_margin 0.0635))
    (pad 8 smd rect (at -1.905 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 1.905 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.635 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -1.905 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 127 "Net-(C16-Pad2)") (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -0.635 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 129 "Net-(IC11-Pad7)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -0.635 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 126 "Net-(C16-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 67.476 -82.296 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C43 (at 2.3885 0.6985 180) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 50.7628 -99.9744)
    (descr <b>RESISTOR</b>)
    (fp_text reference R57 (at 0.1642 -0.7366 180) (layer F.SilkS))
    (fp_text value 562 (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 149 "Net-(C49-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 7 "Net-(C48-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 49.3268 -106.26 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R58 (at 0.2676 1.3716 90) (layer F.SilkS))
    (fp_text value 100 (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 148 "Net-(C51-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 36 "Net-(R58-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 40.3488 -106.0704 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C50 (at -1.2056 0.9652) (layer F.SilkS))
    (fp_text value 22p (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C50-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 51.054 -81.954 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R59 (at 0.928 -1.397 90) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 -90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 150 "Net-(C53-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 151 "Net-(C54-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 51.054 -78.701 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R60 (at -0.723 -0.762 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 -90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 151 "Net-(C54-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 152 "Net-(C54-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 43.18 -77.128 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R61 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 153 "Net-(IC5-Pad6)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 152 "Net-(C54-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 37.2491 -77.128 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R62 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 153 "Net-(IC5-Pad6)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 154 "Net-(IC5-Pad7)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 46.4185 -77.685 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R63 (at 0.723 0.889 90) (layer F.SilkS))
    (fp_text value 237 (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 152 "Net-(C54-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 155 "Net-(C55-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 39.2176 -77.128 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R64 (at 0.6595 0.7239 90) (layer F.SilkS))
    (fp_text value 237 (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 154 "Net-(IC5-Pad7)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 156 "Net-(C56-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 53.887 -78.232)
    (descr <b>RESISTOR</b>)
    (fp_text reference R65 (at 0.723 -1.27 -180) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 39 "Net-(C52-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 53.887 -80.264)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C52 (at 0.723 -1.143 -180) (layer F.SilkS))
    (fp_text value 180p (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 39 "Net-(C52-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 53.887 -82.296 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C53 (at -0.723 1.397) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 150 "Net-(C53-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 39 "Net-(C52-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 49.022 -78.701 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C54 (at 0.723 0.762 270) (layer F.SilkS))
    (fp_text value 120p (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 152 "Net-(C54-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 151 "Net-(C54-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 45.212 -81.446 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C55 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 13 /IN2P) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 155 "Net-(C55-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 41.1988 -77.128 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C56 (at 0.6595 0.7112 90) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 12 /IN2N) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 156 "Net-(C56-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 47.2694 -81.446 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C57 (at 0.596 0.6604 90) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 13 /IN2P) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 47.2694 -84.8986 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C58 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 12 /IN2N) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 45.1866 -84.8986 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C59 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 100p (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 12 /IN2N) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 13 /IN2P) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SO08 (layer Top) (tedit 5C7AC4A5)
    (at 40.0304 -81.2292 90)
    (descr "<b>Small Outline Package 8</b><br>\nNS Package M08A")
    (fp_text reference IC5 (at -2.4892 -3.8989 90) (layer F.SilkS))
    (fp_text value TL072D (at 3.937 1.905) (layer Cmts.User))
    (pad 5 smd rect (at 1.905 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.635 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 153 "Net-(IC5-Pad6)") (solder_mask_margin 0.0635))
    (pad 8 smd rect (at -1.905 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 1.905 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.635 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -1.905 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 152 "Net-(C54-Pad2)") (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -0.635 -2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 154 "Net-(IC5-Pad7)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -0.635 2.6 90) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 151 "Net-(C54-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 35.2552 -77.128 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C60 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 61.341 -99.187 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R67 (at 0.8255 -1.397 270) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 158 "Net-(C63-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 159 "Net-(C63-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 68.5165 -101.473)
    (descr <b>RESISTOR</b>)
    (fp_text reference R68 (at -0.635 -0.635 -180) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 160 "Net-(IC6-Pad6)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 159 "Net-(C63-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 74.168 -98.1075 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R69 (at 0.762 -1.524 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 160 "Net-(IC6-Pad6)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 161 "Net-(IC6-Pad7)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 59.1185 -99.187 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R70 (at -0.8255 1.3335 90) (layer F.SilkS))
    (fp_text value 237 (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 159 "Net-(C63-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 162 "Net-(C64-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 65.0376 -101.727)
    (descr <b>RESISTOR</b>)
    (fp_text reference R71 (at -0.3175 1.2065) (layer F.SilkS))
    (fp_text value 237 (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 161 "Net-(IC6-Pad7)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 163 "Net-(C65-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 54.0512 -93.9673 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R72 (at 1.2573 0.8382 90) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 41 "Net-(C61-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 56.0832 -93.9673 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C61 (at 1.2573 0.7112 90) (layer F.SilkS))
    (fp_text value 180p (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 41 "Net-(C61-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 59.856 -96.3295)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C62 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 157 "Net-(C62-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 41 "Net-(C61-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 56.4896 -96.5073 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C64 (at 2.0066 0.7112) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 9 /IN4P) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 162 "Net-(C64-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 62.0132 -101.727 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C65 (at 0.1905 -1.143) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 8 /IN4N) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 163 "Net-(C65-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 53.6448 -97.116 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C66 (at 0.4191 0.7493 90) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 9 /IN4P) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 56.896 -99.2496 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C67 (at -0.7484 1.3208 90) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 8 /IN4N) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SO08 (layer Top) (tedit 5C7AC4A5)
    (at 69.1515 -98.1075 270)
    (descr "<b>Small Outline Package 8</b><br>\nNS Package M08A")
    (fp_text reference IC6 (at -2.3495 -2.2225 90) (layer F.SilkS))
    (fp_text value TL072D (at 3.937 1.905 180) (layer Cmts.User))
    (pad 5 smd rect (at 1.905 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.635 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 160 "Net-(IC6-Pad6)") (solder_mask_margin 0.0635))
    (pad 8 smd rect (at -1.905 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 1.905 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.635 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -1.905 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 159 "Net-(C63-Pad2)") (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -0.635 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 161 "Net-(IC6-Pad7)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -0.635 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 158 "Net-(C63-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 72.517 -102.997 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C69 (at -0.1905 0.762 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 57.3396 -77.3684)
    (descr <b>RESISTOR</b>)
    (fp_text reference R73 (at -0.8246 -0.7366) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 164 "Net-(C71-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 165 "Net-(C72-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 22.733 -83.1215 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R74 (at 0.6985 0.8255 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 165 "Net-(C72-Pad1)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 166 "Net-(C72-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 24.257 -85.725)
    (descr <b>RESISTOR</b>)
    (fp_text reference R75 (at -0.635 -0.6985) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 167 "Net-(IC8-Pad6)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 166 "Net-(C72-Pad2)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 32.131 -78.9305 270)
    (descr <b>RESISTOR</b>)
    (fp_text reference R76 (at 0.6985 -1.3335 90) (layer F.SilkS))
    (fp_text value 16.5k (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 167 "Net-(IC8-Pad6)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 168 "Net-(IC8-Pad7)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 26.9875 -85.1535 90)
    (descr <b>RESISTOR</b>)
    (fp_text reference R77 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 237 (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 166 "Net-(C72-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 169 "Net-(C73-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 31.9405 -81.9785 180)
    (descr <b>RESISTOR</b>)
    (fp_text reference R78 (at -1.524 -0.3175) (layer F.SilkS))
    (fp_text value 237 (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 168 "Net-(IC8-Pad7)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 170 "Net-(C74-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:R0603 (layer Top) (tedit 5C78ACAA)
    (at 57.316 -81.3308)
    (descr <b>RESISTOR</b>)
    (fp_text reference R79 (at 0.85 -1.3462 -180) (layer F.SilkS))
    (fp_text value 100k (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1 1.1) (layers Top F.Paste F.Mask)
      (net 43 "Net-(C70-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 57.316 -83.312)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C70 (at 0.85 -1.27 -180) (layer F.SilkS))
    (fp_text value 180p (at -0.635 1.905 -180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 43 "Net-(C70-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 57.3396 -79.3496)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C71 (at 0.8264 -1.1684) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 164 "Net-(C71-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 43 "Net-(C70-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 24.892 -83.1215 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C72 (at -0.635 -0.6985 90) (layer F.SilkS))
    (fp_text value 120p (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 166 "Net-(C72-Pad2)") (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 165 "Net-(C72-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 29.0195 -85.1535 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C73 (at -0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 15 /IN1P) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 169 "Net-(C73-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 33.4636 -83.9724)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C74 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 10u (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 14 /IN1N) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 170 "Net-(C74-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 31.0515 -85.1535 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C75 (at 1.016 0.762 270) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 15 /IN1P) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 37.9612 -85.598)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C76 (at -0.635 -0.635 -180) (layer F.SilkS))
    (fp_text value 1n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 14 /IN1N) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 33.821 -85.852)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C77 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 100p (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 14 /IN1N) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 15 /IN1P) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:SO08 (layer Top) (tedit 5C7AC4A5)
    (at 26.0985 -78.867 270)
    (descr "<b>Small Outline Package 8</b><br>\nNS Package M08A")
    (fp_text reference IC8 (at -2.0955 5.207 90) (layer F.SilkS))
    (fp_text value TL072D (at 3.937 1.905) (layer Cmts.User))
    (pad 5 smd rect (at 1.905 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 6 smd rect (at 0.635 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 167 "Net-(IC8-Pad6)") (solder_mask_margin 0.0635))
    (pad 8 smd rect (at -1.905 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 4 smd rect (at 1.905 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 3 smd rect (at 0.635 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -1.905 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 166 "Net-(C72-Pad2)") (solder_mask_margin 0.0635))
    (pad 7 smd rect (at -0.635 -2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 168 "Net-(IC8-Pad7)") (solder_mask_margin 0.0635))
    (pad 2 smd rect (at -0.635 2.6 270) (size 0.6 2.2) (layers Top F.Paste F.Mask)
      (net 165 "Net-(C72-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 28.1305 -82.423 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C78 (at -0.5715 0.5715 180) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 5.168 -86.0552)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C79 (at 0.4436 -1.8288) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 VEE) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 30.6705 -75.565)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C80 (at -0.635 -0.635 -180) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 75.3364 -87.083 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C81 (at -0.977 1.4605 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 41.441 -84.709)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C82 (at -0.635 -0.635) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 4.064 -79.922 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C83 (at 1.4995 0.889 270) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 10.2498 -99.441 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C84 (at -1.1802 -0.889) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 69.596 -94.234 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C86 (at 1.3843 0.75184) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 16 /FILTR) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 36.068 -105.664 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C85 (at 2.159 0.762 180) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 43.84712 -95.50654)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C88 (at -0.6105 1.397) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 31.3055 -103.5685 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C90 (at 0.8255 -0.8255 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 270) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 30 /+3V3) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 44.157 -97.409)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C94 (at 0.6105 -1.397 -180) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 180) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 172 "Net-(C1-Pad1)") (solder_mask_margin 0.0635))
  )
  (module orbits_v10:9MM_SNAP-IN_POT (layer Bottom) (tedit 5C7AC443)
    (at 7.112 -43.942 180)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VR1 (at -3.81 2.54 180) (layer B.SilkS))
    (fp_text value 9MM_SNAP-IN_POT_ (at -3.81 -3.81 180) (layer Cmts.User))
    (pad CHASSIS2 thru_hole rect (at 4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad CHASSIS1 thru_hole rect (at -4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 113 /ATT_X1) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at -2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:9MM_SNAP-IN_POT (layer Bottom) (tedit 5C7AC443)
    (at 7.112 -30.607 180)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VR2 (at -3.81 2.54 180) (layer B.SilkS))
    (fp_text value 9MM_SNAP-IN_POT_ (at -3.81 -3.81 180) (layer Cmts.User))
    (pad CHASSIS2 thru_hole rect (at 4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad CHASSIS1 thru_hole rect (at -4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 112 /ATT_X3) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at -2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:9MM_SNAP-IN_POT (layer Bottom) (tedit 5C7AC443)
    (at 71.628 -43.942 180)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VR4 (at -3.81 2.54 180) (layer B.SilkS))
    (fp_text value 9MM_SNAP-IN_POT_ (at -3.81 -3.81 180) (layer Cmts.User))
    (pad CHASSIS2 thru_hole rect (at 4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad CHASSIS1 thru_hole rect (at -4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 109 /ATT_X2) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at -2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:9MM_SNAP-IN_POT (layer Bottom) (tedit 5C7AC443)
    (at 46.736 -65.913 180)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VR5 (at -3.81 2.54 180) (layer B.SilkS))
    (fp_text value 9MM_SNAP-IN_POT_ (at -3.81 -3.81 180) (layer Cmts.User))
    (pad CHASSIS2 thru_hole rect (at 4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad CHASSIS1 thru_hole rect (at -4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 110 /ATT_Y2) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at -2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:9MM_SNAP-IN_POT (layer Bottom) (tedit 5C7AC443)
    (at 32.004 -65.913 180)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VR6 (at -3.81 2.54 180) (layer B.SilkS))
    (fp_text value 9MM_SNAP-IN_POT_ (at -3.81 -3.81 180) (layer Cmts.User))
    (pad CHASSIS2 thru_hole rect (at 4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad CHASSIS1 thru_hole rect (at -4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 107 /ATT_Y1) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at -2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:9MM_SNAP-IN_POT (layer Bottom) (tedit 5C7AC443)
    (at 32.004 -8.636 180)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VR7 (at -3.81 2.54 180) (layer B.SilkS))
    (fp_text value 9MM_SNAP-IN_POT_ (at -3.81 -3.81 180) (layer Cmts.User))
    (pad CHASSIS2 thru_hole rect (at 4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad CHASSIS1 thru_hole rect (at -4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 111 /ATT_Y3) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at -2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module orbits_v10:9MM_SNAP-IN_POT (layer Bottom) (tedit 5C7AC443)
    (at 46.736 -8.636 180)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VR8 (at -3.81 2.54 180) (layer B.SilkS))
    (fp_text value 9MM_SNAP-IN_POT_ (at -3.81 -3.81 180) (layer Cmts.User))
    (pad CHASSIS2 thru_hole rect (at 4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad CHASSIS1 thru_hole rect (at -4.5 0 270) (size 3.116 3.116) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at 2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /+3V3_A) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 108 /ATT_Y4) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at -2.5 -7 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
  )
  (module Capacitor_SMD:CP_Elec_4x5.4 (layer Top) (tedit 5A841F9D)
    (at 30.861 -50.8)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.4, Panasonic A5, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C8 (at -3.6195 1.8415) (layer F.SilkS))
    (fp_text value 22u (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 2 VEE))
    (pad 1 smd rect (at -1.8 0) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module orbits_v10:C0603 (layer Top) (tedit 5C78AC6A)
    (at 63.119 -56.388 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C92 (at -0.254 -0.889 90) (layer F.SilkS))
    (fp_text value 100n (at -0.635 1.905 90) (layer Cmts.User))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0635))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 99 /+5V) (solder_mask_margin 0.0635))
  )
  (module Inductor_SMD:L_0805_2012Metric (layer Top) (tedit 5B36C52B)
    (at 75.429 -52.578 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L4 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 33u (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 174 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 173 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.4 (layer Top) (tedit 5A841F9D)
    (at 55.9088 -105.5624)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.4, Panasonic A5, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C1 (at 3.5907 -1.6891) (layer F.SilkS))
    (fp_text value 47u (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.8 0) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 172 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.4 (layer Top) (tedit 5A841F9D)
    (at 31.623 -63.754 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.4, Panasonic A5, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C3 (at -0.762 -3.2 90) (layer F.SilkS))
    (fp_text value 47u (at 0 3.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0 90) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.8 0 90) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.4 (layer Top) (tedit 5A841F9D)
    (at 63.5 -78.97 90)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.4, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C91 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 2.2 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 2.2 1.6) (layers Top F.Paste F.Mask)
      (net 98 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.4 (layer Top) (tedit 5A841F9D)
    (at 75.414 -73.914)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.4, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C95 (at 1.421 2.794) (layer F.SilkS))
    (fp_text value 10u (at 0 2.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 2.2 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0) (size 2.2 1.6) (layers Top F.Paste F.Mask)
      (net 6 /+3V3_A))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.4 (layer Top) (tedit 5A841F9D)
    (at 48.617 -91.313)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.4, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C2 (at 0 -2.7) (layer F.SilkS))
    (fp_text value 10u (at 0 2.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 2.2 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0) (size 2.2 1.6) (layers Top F.Paste F.Mask)
      (net 16 /FILTR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.4 (layer Top) (tedit 5A841F9D)
    (at 71.628 -64.008 180)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.4, Panasonic A5, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C23 (at 4.0005 1.905 180) (layer F.SilkS))
    (fp_text value 22u (at 0 3.2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0 180) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.8 0 180) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 173 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.4 (layer Top) (tedit 5A841F9D)
    (at 70.485 -58.061 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.4, Panasonic A5, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C25 (at 0.1685 3.2385 90) (layer F.SilkS))
    (fp_text value 22u (at 0 3.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0 90) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.8 0 90) (size 2.6 1.6) (layers Top F.Paste F.Mask)
      (net 174 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.4 (layer Top) (tedit 5A841F9D)
    (at 65.913 -57.658 90)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.4, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C93 (at 2.286 -2.6035 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 2.2 1.6) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 2.2 1.6) (layers Top F.Paste F.Mask)
      (net 99 /+5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "we are like dwarves perched on the shoulders of giants" (at 39.37 -5.8928) (layer F.SilkS))
  (gr_text "folly v01\n2018-2019\nBrian Leu" (at 39.37 -36.9316) (layer B.SilkS))
  (gr_text "inestimable thanks to\nBrett Sceli, Mutable Instruments, Samsung, Madrona Labs, Buchla, Moog\nAnimal Collective, Wendy Carlos,\nSuzanne Ciani, Viki Viktoria, Trinosophes, Laurie Spiegel, Cornelius Cardew, Negativland, Erik Santos" (at 39.37 -15.4) (layer F.SilkS))
  (gr_arc (start 73.66 -5.08) (end 73.66 0) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 5.08 -103.378) (end 5.08 -108.458) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 73.66 -103.378) (end 78.74 -103.378) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 5.08 0) (end 73.66 0) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 -5.08) (end 78.74 -103.378) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 5.08 -108.458) (end 73.66 -108.458) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0 -5.08) (end 0 -103.378) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 5.08 -5.08) (end 0 -5.08) (angle -90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy -2.6289 1.778) (xy -2.6289 -109.982) (xy 81.407 -109.982) (xy 81.407 1.778)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy -4.064 -111.413992) (xy -3.81 2.794) (xy 82.804 3.302) (xy 82.55 -110.998)
      )
    )
  )
)
