(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 33)
    (zones 0)
    (modules 18)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.508)
    (trace_clearance 0.381)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.250000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(J3-Pad1)")
  (net 4 "Net-(J5-Pad1)")
  (net 5 "Net-(J6-Pad1)")
  (net 6 "Net-(J8-Pad1)")
  (net 7 "Net-(J9-Pad1)")
  (net 8 "Net-(J10-Pad1)")
  (net 9 "Net-(J12-Pad1)")
  (net 10 "Net-(Q1-Pad2)")
  (net 11 "Net-(Q2-Pad2)")
  (net 12 Earth)
  (net_class Default "This is the default net class."
    (clearance 0.381)
    (trace_width 0.508)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5EA4D402)
    (at 139.954 114.046)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference BFG591 (at 0.127 -0.0889 90) (layer F.SilkS))
    (fp_text value BFG591 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J9-Pad1)"))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J12-Pad1)"))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5EA4D3E9)
    (at 139.954 105.664)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference BFG591 (at 0.0889 -0.1397 90) (layer F.SilkS))
    (fp_text value BFG591 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J5-Pad1)"))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5EA4D3B6)
    (at 132.334 105.664 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference 36 (at -1.4732 1.7653 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5EA4D2F2)
    (at 132.334 110.744 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference 36 (at 3.429 -0.0635 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4DCC4)
    (at 128.905 108.585)
    (fp_text reference C92 (at -0.127 -2.413 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4DA52)
    (at 152.4 106.68)
    (fp_text reference * (at -2.286 0.381) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4DAA6)
    (at 152.4 110.49)
    (fp_text reference * (at -3.556 -2.159) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4D9BC)
    (at 153.67 103.505)
    (fp_text reference C98 (at -2.286 -0.8382) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0.381 -3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4DA69)
    (at 142.24 109.855)
    (fp_text reference R79 (at 1.905 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J5-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4DC6F)
    (at 145.415 106.045)
    (fp_text reference Q4 (at 1.397 -1.524) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 1.27 2.032 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J6-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4CF71)
    (at 146.685 106.68)
    (fp_text reference J7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J6-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4DCA5)
    (at 133.35 108.585)
    (fp_text reference C91 (at -1.524 -0.381 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(J8-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4DA4E)
    (at 152.4 114.3)
    (fp_text reference * (at -2.286 -3.175) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(J9-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4DC7A)
    (at 145.415 114.935)
    (fp_text reference Q3 (at 1.524 1.397) (layer F.SilkS))
    (fp_text value GND (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J10-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4CF71)
    (at 146.685 114.3)
    (fp_text reference J11 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J10-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4D524)
    (at 142.24 118.11)
    (fp_text reference R77 (at 2.4765 0.6096) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J12-Pad1)"))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4D289)
    (at 126.492 102.87)
    (fp_text reference GND (at 4.318 -0.254) (layer F.SilkS))
    (fp_text value GND (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.778 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 Earth))
  )
  (module 1111:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5EA4D2BF)
    (at 152.654 118.11)
    (fp_text reference GND (at 0.508 0.762) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.159 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 Earth))
  )
  (gr_text "mcHF driver mod by LY2BOK\nPCB design by UTØUM\nwww.mcHF.AT" (at 129.921 104.394) (layer B.SilkS))
  (gr_text T' (at 149.733 105.029) (layer F.SilkS))
  (gr_text c (at 148.209 111.76 180) (layer F.SilkS))
  (gr_text c (at 148.209 109.22 180) (layer F.SilkS))
  (gr_text c (at 148.209 110.49 180) (layer F.SilkS))
  (gr_text c (at 151.13 113.411) (layer F.SilkS))
  (gr_text c (at 151.13 112.141) (layer F.SilkS))
  (gr_text c (at 151.13 110.871) (layer F.SilkS))
  (gr_text c (at 151.13 109.601) (layer F.SilkS))
  (gr_text c (at 151.13 107.061) (layer F.SilkS))
  (gr_text c (at 151.13 108.331) (layer F.SilkS))
  (gr_text 3T (at 152.654 112.522) (layer F.SilkS))
  (gr_text 3T (at 152.654 108.585) (layer F.SilkS))
  (gr_text 3T (at 146.558 110.363) (layer F.SilkS))
  (gr_line (start 134.62 113.665) (end 133.35 112.395) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.62 120.015) (end 134.62 113.665) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.21 120.015) (end 134.62 120.015) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 112.395) (end 133.35 112.395) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 101.6) (end 127 112.395) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.21 101.6) (end 156.21 120.015) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 101.6) (end 156.21 101.6) (angle 90) (layer Edge.Cuts) (width 0.05))
  (zone (net 12) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 156.21 101.6) (xy 126.746 101.346) (xy 125.222 105.664) (xy 124.968 113.03) (xy 132.08 114.046)
        (xy 133.858 118.618) (xy 133.35 122.682) (xy 155.956 123.19) (xy 160.274 120.904) (xy 163.83 102.108)
        (xy 160.782 98.806) (xy 156.21 101.346)
      )
    )
  )
)
