(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 56)
    (zones 0)
    (modules 26)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.381)
    (via_min_drill 0.127)
    (user_via 0.4064 0.1524)
    (uvia_size 0.3556)
    (uvia_drill 0.1016)
    (uvias_allowed no)
    (uvia_min_size 0.3556)
    (uvia_min_drill 0.1016)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +6V)
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "Net-(D4-Pad1)")
  (net 6 "Net-(D5-Pad1)")
  (net 7 "Net-(D6-Pad1)")
  (net 8 "Net-(D7-Pad1)")
  (net 9 "Net-(D8-Pad1)")
  (net 10 "Net-(D9-Pad1)")
  (net 11 "Net-(D10-Pad1)")
  (net 12 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3556)
    (uvia_drill 0.1016)
    (add_net +6V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
  )
  (module Customparts:date (layer F.Cu) (tedit 0)
    (at 123.19 127)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Customparts:Forrest (layer F.Cu) (tedit 0)
    (at 168.91 123.19)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Customparts:Diane (layer F.Cu) (tedit 0)
    (at 128.27 113.03)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Customparts:ampersand (layer F.Cu) (tedit 5CBB7EF4)
    (at 149.86 116.84)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 144.78 109.22 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 124.46 121.92 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 130.81 109.22 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 139.7 124.46 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 168.91 109.22 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0 -1.25 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 184.15 114.3 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.25 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 158.75 124.46)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 158.75 111.76 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 176.06 116.84 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 149.86 125.73 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D10 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 146.05 109.22)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 124.46 123.19 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 131.572 110.49 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 137.922 123.19 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 166.878 110.998 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 181.61 115.57 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 158.75 125.73)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 160.02 113.03)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 176.53 114.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 151.13 124.46 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value 300 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 56C35FC6)
    (at 116.84 114.3)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference 6V (at 0 3) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 +6V))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 56C35FC6)
    (at 116.84 125.73)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference GND (at 0 3) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 12 GND))
  )
  (gr_line (start 189.23 105.41) (end 113.03 105.41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 189.23 130.81) (end 189.23 105.41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.03 130.81) (end 189.23 130.81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.03 105.41) (end 113.03 130.81) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name +6V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.03 109.22) (xy 110.49 109.22) (xy 110.49 105.41) (xy 189.23 105.41) (xy 189.23 130.81)
        (xy 113.03 130.81)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.03 114.3) (xy 110.49 114.3) (xy 110.49 110.49) (xy 113.03 110.49) (xy 113.03 105.41)
        (xy 189.23 105.41) (xy 189.23 130.81) (xy 113.03 130.81)
      )
    )
  )
)
