<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="65" y1="69" x2="58" y2="69" width="0" layer="20"/>
<wire x1="58" y1="69" x2="56" y2="67" width="0" layer="20" curve="90"/>
<wire x1="56" y1="67" x2="56" y2="37" width="0" layer="20"/>
<wire x1="56" y1="37" x2="58" y2="35" width="0" layer="20" curve="90"/>
<wire x1="58" y1="35" x2="118.023390625" y2="35" width="0" layer="20"/>
<wire x1="118.023390625" y1="35" x2="120.023253125" y2="36.976515625" width="0" layer="20" curve="89.327207"/>
<wire x1="120.023253125" y1="36.976515625" x2="120.1" y2="43.5" width="0" layer="20"/>
<wire x1="120.1" y1="43.5" x2="118.5" y2="45.1" width="0" layer="20"/>
<wire x1="118.5" y1="45.1" x2="118.5" y2="55" width="0" layer="20"/>
<wire x1="118.5" y1="55" x2="120" y2="56.5" width="0" layer="20"/>
<wire x1="120" y1="56.5" x2="120" y2="67" width="0" layer="20"/>
<wire x1="120" y1="67" x2="118" y2="69" width="0" layer="20" curve="90"/>
<wire x1="118" y1="69" x2="75" y2="69" width="0" layer="20"/>
<wire x1="75" y1="69" x2="74.5" y2="68.5" width="0" layer="20" curve="90"/>
<wire x1="74.5" y1="68.5" x2="74.5" y2="67.5" width="0" layer="20"/>
<wire x1="74.5" y1="67.5" x2="65.5" y2="67.5" width="0" layer="20"/>
<wire x1="65.5" y1="67.5" x2="65.5" y2="68.5" width="0" layer="20"/>
<wire x1="65.5" y1="68.5" x2="65" y2="69" width="0" layer="20" curve="90"/>
<text>RST</text>
<text>ERA</text>
<text>SWD</text>
<text>serial</text>
<text>SD card</text>
<text>USB</text>
<text>JAW 2016-05</text>
<text>www.amiketo.com</text>
<text>SE7EDUINO Rev. 0</text>
<text>JAW 2016-05</text>
<text>JAW 2016-05</text>
<text>use screw: M2.5,
No. 3, or 3/32"</text>
<text>CHRG</text>
<text>VBAT
GND</text>
<text>VUSB
GND</text>
<text>3V3
GND</text>
<text>D0
B13</text>
<text>B1
D31</text>
<text>A20
B0</text>
<text>A18
A19</text>
<text>B2
A17</text>
<text>A21
B3</text>
<text>A13
D30</text>
<text>A23
A16</text>
<text>A15
D27</text>
<text>D25
A14</text>
<text>A12
D26</text>
<text>3V3
GND</text>
<text>I2C
CK
DA</text>
<text>CSd
GND</text>
<text>MOSI
DC</text>
<text>MISO
SCK</text>
<text>3V3
nRST</text>
<text>se7eduino</text>
<text>+</text>
<text>piezo</text>
<text>64mm</text>
<text>34mm</text>
<text>Pb</text>
<text>ARM</text>
<text>Cortex</text>
<text>M7</text>
<text>AT SAM S70</text>
<text>VBAT, VUSB:  6V MAX
ALL IO PINS: 3.3V MAX</text>
</plain>
<libraries>
<library name="jaw">
<packages>
<package name="TQFP-100-14X14MM">
</package>
<package name="SMD0402">
</package>
<package name="SMD0603">
</package>
<package name="RESONATOR-CSTCE">
</package>
<package name="XTAL-32X15">
</package>
<package name="MICROSD/EJECTOR">
</package>
<package name="HEADER-3X2-POGO">
</package>
<package name="KMR211">
</package>
<package name="SMD-0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
<package name="SMD1206">
</package>
<package name="SMD0603D">
</package>
<package name="M127-5X2-F">
</package>
<package name="ROBOTMAN-LOGO2">
</package>
<package name="SOT-23-5">
</package>
<package name="SMD0805-DUAL">
</package>
<package name="SOT-23-6">
</package>
<package name="HEADER-1X1-SMALL">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="CONN_USB_MICRO-B">
<description>USB micro-b connector SMT 0.65 mm pitch,
1.45mm from center to PCB edge,
Based on TE part number 1981568-1</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="jaw" package="TQFP-100-14X14MM" value="ATSAME70">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="jaw" package="SMD0402" value="FB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="jaw" package="SMD0402" value="FB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="jaw" package="SMD0402" value="FB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jaw" package="SMD0402" value="5k62 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="jaw" package="SMD0402" value="10p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="jaw" package="RESONATOR-CSTCE" value="12MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="jaw" package="XTAL-32X15" value="32k768">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="jaw" package="SMD0402" value="4p7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="jaw" package="SMD0402" value="4p7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="dp_devices" package="CONN_USB_MICRO-B" value="CON-USB-F-MICRO-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="jaw" package="MICROSD/EJECTOR" value="MICROSD-EJECT">
<attribute name="NAME"/>
</element>
<element name="C19" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN2" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN5" library="adafruit" package="2X20" value="DO NOT PLACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN3" library="jaw" package="HEADER-3X2-POGO" value="DO NOT PLACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="jaw" package="KMR211" value="SWITCHKMR211">
<attribute name="NAME"/>
</element>
<element name="SW2" library="jaw" package="KMR211" value="SWITCHKMR211">
<attribute name="NAME"/>
</element>
<element name="C20" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jaw" package="SMD0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jaw" package="SMD0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="jaw" package="SMD-0603-ARV" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="jaw" package="SMD1206" value="750mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="jaw" package="SMD0603D" value="white">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="jaw" package="SMD0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="jaw" package="SMD-0603-ARV" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN4" library="jaw" package="M127-5X2-F" value="DO NOT PLACE"/>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$4" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$5" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$6" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$1" library="jaw" package="ROBOTMAN-LOGO2" value="ROBOTMAN-LOGO2"/>
<element name="U$3" library="jaw" package="ROBOTMAN-LOGO2" value="ROBOTMAN-LOGO2"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="U2" library="adafruit" package="SOT23-5L" value="MCP73831/OT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="jaw" package="SOT-23-5" value="3v3, 500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="jaw" package="SMD0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="jaw" package="SMD0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="jaw" package="SMD0805-DUAL" value="LED-DUAL0805">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="jaw" package="SOT-23-6" value="FDC6329S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="jaw" package="SMD0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="jaw" package="SMD0402" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="jaw" package="SMD0603D" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="jaw" package="SMD0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN6" library="jaw" package="HEADER-1X1-SMALL" value="DO NOT PLACE"/>
<element name="CN7" library="jaw" package="HEADER-1X1-SMALL" value="DO NOT PLACE"/>
<element name="C25" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="67"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="R2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="USB1" pad="P5"/>
<contactref element="C19" pad="1"/>
<contactref element="CN3" pad="2"/>
<contactref element="CN2" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="C23" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="73"/>
<contactref element="U1" pad="60"/>
<contactref element="USB1" pad="P4"/>
<contactref element="CN1" pad="6"/>
<contactref element="CN1" pad="SHELL1"/>
<contactref element="C24" pad="1"/>
<contactref element="CN4" pad="3"/>
<contactref element="CN4" pad="5"/>
<contactref element="CN5" pad="8"/>
<contactref element="CN5" pad="12"/>
<contactref element="CN5" pad="38"/>
<contactref element="CN5" pad="40"/>
<contactref element="CN5" pad="36"/>
<contactref element="VR1" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED2" pad="3"/>
<contactref element="R9" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="CN6" pad="P$1"/>
<contactref element="C25" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="68"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="81"/>
<contactref element="U1" pad="93"/>
<contactref element="U1" pad="5"/>
<contactref element="L1" pad="1"/>
<contactref element="L4" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="3"/>
<contactref element="CN1" pad="4"/>
<contactref element="R6" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R6" pad="3"/>
<contactref element="R6" pad="4"/>
<contactref element="R4" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R4" pad="3"/>
<contactref element="R4" pad="4"/>
<contactref element="C24" pad="2"/>
<contactref element="CN4" pad="1"/>
<contactref element="CN5" pad="1"/>
<contactref element="CN5" pad="11"/>
<contactref element="CN5" pad="35"/>
<contactref element="VR1" pad="5"/>
</signal>
<signal name="V1V2">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="39"/>
<contactref element="U1" pad="76"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="18"/>
<contactref element="L2" pad="1"/>
<contactref element="L3" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="L1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="90"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="96"/>
<contactref element="L2" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="86"/>
<contactref element="L3" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="VCCA">
<contactref element="U1" pad="9"/>
<contactref element="L4" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C19" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="97"/>
<contactref element="C5" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="98"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="99"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="25"/>
<contactref element="X2" pad="P$1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="24"/>
<contactref element="X2" pad="P$2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="USBDP">
<contactref element="U1" pad="95"/>
<contactref element="USB1" pad="P3"/>
</signal>
<signal name="USBDM">
<contactref element="U1" pad="94"/>
<contactref element="USB1" pad="P2"/>
</signal>
<signal name="NRST">
<contactref element="CN3" pad="6"/>
<contactref element="C23" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="2"/>
<contactref element="U1" pad="58"/>
<contactref element="CN4" pad="10"/>
<contactref element="CN5" pad="2"/>
</signal>
<signal name="VUSB">
<contactref element="CN3" pad="1"/>
<contactref element="USB1" pad="P1"/>
<contactref element="F1" pad="1"/>
<contactref element="CN5" pad="37"/>
</signal>
<signal name="TX">
<contactref element="CN3" pad="4"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="RX">
<contactref element="CN3" pad="3"/>
<contactref element="U1" pad="54"/>
</signal>
<signal name="VBAT">
<contactref element="CN2" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="CN5" pad="39"/>
<contactref element="U2" pad="3"/>
<contactref element="Q1" pad="4"/>
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="SWCLK">
<contactref element="U1" pad="63"/>
<contactref element="CN4" pad="4"/>
<contactref element="R6" pad="5"/>
</signal>
<signal name="SWDIO">
<contactref element="U1" pad="57"/>
<contactref element="CN4" pad="2"/>
<contactref element="R6" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="IOLED1">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="70"/>
</signal>
<signal name="ERASE">
<contactref element="SW2" pad="4"/>
<contactref element="SW2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="61"/>
<contactref element="CN3" pad="5"/>
</signal>
<signal name="SDIOD0">
<contactref element="CN1" pad="7"/>
<contactref element="U1" pad="82"/>
<contactref element="R4" pad="5"/>
</signal>
<signal name="SDIOD1">
<contactref element="CN1" pad="8"/>
<contactref element="U1" pad="83"/>
<contactref element="R4" pad="6"/>
</signal>
<signal name="SDIOD2">
<contactref element="CN1" pad="1"/>
<contactref element="U1" pad="42"/>
<contactref element="R4" pad="7"/>
</signal>
<signal name="SDIOD3">
<contactref element="CN1" pad="2"/>
<contactref element="U1" pad="50"/>
<contactref element="R4" pad="8"/>
</signal>
<signal name="SDIOCK">
<contactref element="CN1" pad="5"/>
<contactref element="U1" pad="40"/>
</signal>
<signal name="SDIOCM">
<contactref element="CN1" pad="3"/>
<contactref element="U1" pad="79"/>
<contactref element="R6" pad="8"/>
</signal>
<signal name="CARDIO">
<contactref element="CN1" pad="CD1"/>
<contactref element="R6" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="CN4" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="CN4" pad="9"/>
</signal>
<signal name="SWO">
<contactref element="CN4" pad="6"/>
<contactref element="U1" pad="77"/>
</signal>
<signal name="N$26">
<contactref element="CN4" pad="8"/>
</signal>
<signal name="SPIMISO">
<contactref element="CN5" pad="3"/>
<contactref element="U1" pad="45"/>
</signal>
<signal name="SPIMOSI">
<contactref element="CN5" pad="5"/>
<contactref element="U1" pad="43"/>
</signal>
<signal name="CSDPY">
<contactref element="CN5" pad="7"/>
<contactref element="U1" pad="65"/>
</signal>
<signal name="I2CCK">
<contactref element="CN5" pad="9"/>
<contactref element="U1" pad="55"/>
</signal>
<signal name="SPISCK">
<contactref element="CN5" pad="4"/>
<contactref element="U1" pad="41"/>
</signal>
<signal name="CSDC">
<contactref element="CN5" pad="6"/>
<contactref element="U1" pad="53"/>
</signal>
<signal name="I2CDA">
<contactref element="CN5" pad="10"/>
<contactref element="U1" pad="64"/>
</signal>
<signal name="PINB13">
<contactref element="U1" pad="100"/>
<contactref element="CN5" pad="34"/>
</signal>
<signal name="PIND0">
<contactref element="U1" pad="1"/>
<contactref element="CN5" pad="33"/>
</signal>
<signal name="PIND31">
<contactref element="U1" pad="2"/>
<contactref element="CN5" pad="32"/>
</signal>
<signal name="PINA13">
<contactref element="U1" pad="27"/>
<contactref element="CN5" pad="21"/>
</signal>
<signal name="PINA14">
<contactref element="U1" pad="34"/>
<contactref element="CN5" pad="16"/>
</signal>
<signal name="PINA15">
<contactref element="U1" pad="33"/>
<contactref element="CN5" pad="17"/>
</signal>
<signal name="PINA16">
<contactref element="U1" pad="30"/>
<contactref element="CN5" pad="20"/>
</signal>
<signal name="PINA23">
<contactref element="U1" pad="31"/>
<contactref element="CN5" pad="19"/>
</signal>
<signal name="PINA24">
<contactref element="U1" pad="38"/>
</signal>
<signal name="PIND24">
<contactref element="U1" pad="37"/>
</signal>
<signal name="PIND25">
<contactref element="U1" pad="35"/>
<contactref element="CN5" pad="15"/>
</signal>
<signal name="PIND26">
<contactref element="U1" pad="36"/>
<contactref element="CN5" pad="14"/>
</signal>
<signal name="PIND27">
<contactref element="U1" pad="32"/>
<contactref element="CN5" pad="18"/>
</signal>
<signal name="PINB0">
<contactref element="U1" pad="12"/>
<contactref element="CN5" pad="30"/>
</signal>
<signal name="PINB1">
<contactref element="U1" pad="11"/>
<contactref element="CN5" pad="31"/>
</signal>
<signal name="PINB2">
<contactref element="U1" pad="17"/>
<contactref element="CN5" pad="25"/>
</signal>
<signal name="PINB3">
<contactref element="U1" pad="20"/>
<contactref element="CN5" pad="24"/>
</signal>
<signal name="PINA17">
<contactref element="U1" pad="16"/>
<contactref element="CN5" pad="26"/>
</signal>
<signal name="PINA18">
<contactref element="U1" pad="15"/>
<contactref element="CN5" pad="27"/>
</signal>
<signal name="PINA19">
<contactref element="U1" pad="14"/>
<contactref element="CN5" pad="28"/>
</signal>
<signal name="PINA20">
<contactref element="U1" pad="13"/>
<contactref element="CN5" pad="29"/>
</signal>
<signal name="PINA21">
<contactref element="U1" pad="21"/>
<contactref element="CN5" pad="23"/>
</signal>
<signal name="PIND30">
<contactref element="U1" pad="23"/>
<contactref element="CN5" pad="22"/>
</signal>
<signal name="N$4">
<contactref element="LED2" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="LED2" pad="4"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="IOLED2">
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="IOLED3">
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="52"/>
</signal>
<signal name="VSYS">
<contactref element="VR1" pad="1"/>
<contactref element="VR1" pad="3"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="6"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="5"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="Q1" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="U2" pad="4"/>
<contactref element="F1" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="PIEZO">
<contactref element="U1" pad="72"/>
<contactref element="CN7" pad="P$1"/>
</signal>
<signal name="PINA12">
<contactref element="U1" pad="48"/>
<contactref element="CN5" pad="13"/>
</signal>
<signal name="N$15">
</signal>
<signal name="N$10">
<contactref element="U2" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R11" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$18">
</signal>
</signals>
</board>
</drawing>
</eagle>
