(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 80)
    (zones 0)
    (modules 6)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.5 0.85)
    (user_via 3.5 2.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad6)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
    (add_net VCC)
  )
  (module footprints:xt30_3 (layer F.Cu) (tedit 5C817DCB)
    (at 139 103)
    (fp_text reference J4 (at 0 20) (layer F.SilkS) hide)
    (fp_text value Conn_01x09_Male (at 0 -20) (layer F.Fab))
    (pad 9 thru_hole circle (at 0 -15) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 -10) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 0 -2.5) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 4 thru_hole circle (at 0 2.5) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 0 10) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at 0 15) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 8 thru_hole circle (at 5 -12.5) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 5 thru_hole circle (at 5 0) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 2 thru_hole circle (at 5 12.5) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
  )
  (module footprints:xt30_3 (layer F.Cu) (tedit 5C817DCB)
    (at 128 103)
    (fp_text reference J3 (at 0 20) (layer F.SilkS) hide)
    (fp_text value Conn_01x09_Male (at 0 -20) (layer F.Fab))
    (pad 9 thru_hole circle (at 0 -15) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 -10) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 0 -2.5) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 4 thru_hole circle (at 0 2.5) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 0 10) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at 0 15) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 8 thru_hole circle (at 5 -12.5) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 5 thru_hole circle (at 5 0) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 2 thru_hole circle (at 5 12.5) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
  )
  (module footprints:xt30_3 (layer F.Cu) (tedit 5C817DCB)
    (at 117 103)
    (fp_text reference J2 (at 0 20) (layer F.SilkS) hide)
    (fp_text value Conn_01x09_Male (at 0 -20) (layer F.Fab))
    (pad 9 thru_hole circle (at 0 -15) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 -10) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 0 -2.5) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 4 thru_hole circle (at 0 2.5) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 0 10) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at 0 15) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 8 thru_hole circle (at 5 -12.5) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 5 thru_hole circle (at 5 0) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 2 thru_hole circle (at 5 12.5) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
  )
  (module footprints:xt30_3 (layer F.Cu) (tedit 5C817DCB)
    (at 106 103)
    (fp_text reference J1 (at 0 20) (layer F.SilkS) hide)
    (fp_text value Conn_01x09_Male (at 0 -20) (layer F.Fab))
    (pad 9 thru_hole circle (at 0 -15) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 -10) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 0 -2.5) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 4 thru_hole circle (at 0 2.5) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 0 10) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at 0 15) (size 3.5 3.5) (drill 2.6) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 8 thru_hole circle (at 5 -12.5) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 5 thru_hole circle (at 5 0) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 2 thru_hole circle (at 5 12.5) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
  )
  (module custom:balance_plug (layer F.Cu) (tedit 5BAFA1EB)
    (at 150 94.37)
    (fp_text reference J6 (at 0 10.16) (layer F.SilkS) hide)
    (fp_text value Conn_01x07_Female (at 0 -8.89) (layer F.Fab))
    (pad 1 smd roundrect (at 0 7.62) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 2 smd roundrect (at 0 5.08) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad2)"))
    (pad 3 smd roundrect (at 0 2.54) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd roundrect (at 0 0) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad5)"))
    (pad 5 smd roundrect (at 0 -2.54) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad6)"))
    (pad 6 smd roundrect (at 0 -5.08) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(J1-Pad8)"))
    (pad 7 smd roundrect (at 0 -7.62) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
  )
  (module custom:xt60_pad (layer F.Cu) (tedit 5BAFA200)
    (at 150 114.4)
    (fp_text reference J5 (at 0 0.762) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 -0.762) (layer F.Fab))
    (pad 1 smd roundrect (at 0 3.6) (size 4 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 2 smd roundrect (at 0 -3.6) (size 4 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
  )
  (gr_text "2S XT30 Charging Board" (at 122 96.75) (layer B.SilkS))
  (gr_text "Created by Phobos" (at 122 109.25) (layer B.SilkS))
  (gr_text + (at 146.5 117.875) (layer F.SilkS))
  (gr_text + (at 147.25 102 90) (layer F.SilkS))
  (gr_text - (at 146.5 110.75 90) (layer F.SilkS))
  (gr_text - (at 147.25 86.75 90) (layer F.SilkS))
  (gr_line (start 102 122) (end 102 84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152 122) (end 102 122) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152 84) (end 152 122) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151 84) (end 152 84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 84) (end 151 84) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name "Net-(J1-Pad3)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 2) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 104 103.5) (xy 141 103.5) (xy 141 115) (xy 104 115)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pad6)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 2) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 104 91) (xy 141 91) (xy 140.75 102.5) (xy 104 102.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 2))
    (polygon
      (pts
        (xy 102 84) (xy 102 122) (xy 152 122) (xy 152 84)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 2) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 102 84) (xy 102 122) (xy 152 122) (xy 152 84)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pad8)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 110 89.5) (xy 110 97.5) (xy 145 97.5) (xy 145 89.5)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 110 98) (xy 145 98) (xy 145 110) (xy 110 110)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 110 110.5) (xy 145 110.5) (xy 145 122) (xy 110 122)
      )
    )
  )
)
