(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.63)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.025))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.025))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 150 100)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VDD")
  (net 2 "GND")
  (net 3 "/BlinkStick_R")
  (net 4 "Net-(U1-DOUT)")
  (net 5 "Net-(U2-DOUT)")
  (net 6 "unconnected-(U3-DOUT-Pad4)")
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 161.3 106.6 60)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "MFG PN" "FZ2812-5050")
    (property "Sheetfile" "Ring Light PCB BlinkStick.kicad_sch")
    (property "Sheetname" "")
    (property "Supplier PN" "4544-FZ2812-5050CT-ND")
    (property "Supplier URL" "https://www.digikey.com/en/products/detail/feztek/FZ2812-5050/18647407?s=N4IgTCBcDaIGYC8wA4CMYC0BWADLkAugL5A")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.5 60) (layer "F.SilkS"))
    (fp_text value "2812" (at 0 4 60) (layer "F.Fab"))
    (fp_text user "1" (at -4.001666 -1.731089 60) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 60) (layer "F.Fab"))
    (pad "1" smd rect (at -2.45 -1.65 60) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at -2.45 1.65 60) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(U2-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at 2.45 1.65 60) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at 2.45 -1.65 60) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(U3-DOUT-Pad4)") (pinfunction "DOUT") (pintype "output+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 160.6 88.92 -45)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Ring Light PCB BlinkStick.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -2.630437 2.460732 -135) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 7.41 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 45) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/BlinkStick_R") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 315) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 150.05 86.95 180)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "MFG PN" "FZ2812-5050")
    (property "Sheetfile" "Ring Light PCB BlinkStick.kicad_sch")
    (property "Sheetname" "")
    (property "Supplier PN" "4544-FZ2812-5050CT-ND")
    (property "Supplier URL" "https://www.digikey.com/en/products/detail/feztek/FZ2812-5050/18647407?s=N4IgTCBcDaIGYC8wA4CMYC0BWADLkAugL5A")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "2812" (at 0 4) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -2.65) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.45 -1.65 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at -2.45 1.65 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/BlinkStick_R") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at 2.45 1.65 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at 2.45 -1.65 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U1-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 163.5 102.5 150)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MFG PN" "")
    (property "Sheetfile" "Ring Light PCB BlinkStick.kicad_sch")
    (property "Sheetname" "")
    (property "Supplier PN" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 1.7 150) (layer "F.SilkS"))
    (fp_text value "4.7" (at 0 -1.6 150) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 150) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 150) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 150) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 154.5 87 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MFG PN" "")
    (property "Sheetfile" "Ring Light PCB BlinkStick.kicad_sch")
    (property "Sheetname" "")
    (property "Supplier PN" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "4.7" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:OSHPark_Logo" (layer "F.Cu")
    (at 138 95)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 -4.4) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0 4.7) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 136.25 102.25 30)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MFG PN" "")
    (property "Sheetfile" "Ring Light PCB BlinkStick.kicad_sch")
    (property "Sheetname" "")
    (property "Supplier PN" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68 30) (layer "F.SilkS"))
    (fp_text value "4.7" (at 0 1.68 30) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 30) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 30) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 30) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (at 138.6 106.3 -60)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "MFG PN" "FZ2812-5050")
    (property "Sheetfile" "Ring Light PCB BlinkStick.kicad_sch")
    (property "Sheetname" "")
    (property "Supplier PN" "4544-FZ2812-5050CT-ND")
    (property "Supplier URL" "https://www.digikey.com/en/products/detail/feztek/FZ2812-5050/18647407?s=N4IgTCBcDaIGYC8wA4CMYC0BWADLkAugL5A")
    (attr smd)
    (fp_text reference "U2" (at 0 -3.5 120) (layer "F.SilkS"))
    (fp_text value "2812" (at 0 4 120) (layer "F.Fab"))
    (fp_text user "1" (at -4.043524 -2.79641 120) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 120) (layer "F.Fab"))
    (pad "1" smd rect (at -2.45 -1.65 300) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" smd rect (at -2.45 1.65 300) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U1-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "3" smd rect (at 2.45 1.65 300) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at 2.45 -1.65 300) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(U2-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Berkeley_Lab_Logo" (layer "B.Cu")
    (at 137.5 100 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 6.4) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_circle (center 161 97) (end 161 98.5)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 144 112) (end 144 113.5)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 150 100) (end 158 100)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 156 112) (end 156 113.5)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 150 100) (end 168 100)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "NSIII RING LIGHT V1.2\nELAINE JEFFERY NOV/2023\nEAJEFFERY@LBL.GOV\nBERKELEY LAB" (at 150 91) (layer "B.SilkS"))
  (gr_text "  FABRICATED\nBY OSHPARK" (at 135.5 91) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layers "F.Cu" "F.SilkS") (name "screw_head") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 158.5 111)
        (xy 158.5 113)
        (xy 157 114.5)
        (xy 155 114.5)
        (xy 153.5 113)
        (xy 153.5 111)
        (xy 155 109.5)
        (xy 157 109.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F.Cu" "F.SilkS") (name "screw_head") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 146.5 111)
        (xy 146.5 113)
        (xy 145 114.5)
        (xy 143 114.5)
        (xy 141.5 113)
        (xy 141.5 111)
        (xy 143 109.5)
        (xy 145 109.5)
      )
    )
  )
)
