(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 1157)
    (zones 0)
    (modules 90)
    (nets 78)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.2 0.2)
    (mod_text_width 0.05)
    (pad_size 0.2 0.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.03)
    (solder_mask_min_width 0.0635)
    (pad_to_paste_clearance -0.0125)
    (aux_axis_origin 0 0)
    (grid_origin 123.444 99.7585)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "V44"))
  )
  (net 0 "")
  (net 1 BATT+)
  (net 2 BATT-)
  (net 3 Button1)
  (net 4 Button2)
  (net 5 Button3)
  (net 6 GND)
  (net 7 "Net-(C1-Pad2)")
  (net 8 3.3v)
  (net 9 "Net-(C7-Pad1)")
  (net 10 "Net-(C8-Pad1)")
  (net 11 5v)
  (net 12 RESET)
  (net 13 "Net-(C61-Pad1)")
  (net 14 VBUS)
  (net 15 FREE1)
  (net 16 FREE2)
  (net 17 boost_en)
  (net 18 id-neopixel_data)
  (net 19 "Net-(LED1-Pad1)")
  (net 20 "Net-(LED2-Pad1)")
  (net 21 "Net-(LED3-Pad1)")
  (net 22 "Net-(LED4-Pad1)")
  (net 23 "Net-(LED5-Pad1)")
  (net 24 "Net-(LED6-Pad1)")
  (net 25 neopixel_data2)
  (net 26 CH1)
  (net 27 CH2)
  (net 28 CH3)
  (net 29 CH4)
  (net 30 CH5)
  (net 31 CH6)
  (net 32 SDA)
  (net 33 SCL)
  (net 34 DP)
  (net 35 DM)
  (net 36 BTN)
  (net 37 sd_en)
  (net 38 amp_en)
  (net 39 RX)
  (net 40 miso)
  (net 41 sclk)
  (net 42 mosi)
  (net 43 "Net-(SP+1-Pad1)")
  (net 44 "Net-(SP-1-Pad1)")
  (net 45 SWDCLK)
  (net 46 SWDIO)
  (net 47 TX)
  (net 48 INT)
  (net 49 I2S_LRCLK)
  (net 50 I2S_BCLK)
  (net 51 I2S_DATA)
  (net 52 "Net-(SD1-Pad8)")
  (net 53 "Net-(SD1-Pad9)")
  (net 54 "Net-(SD1-Pad10)")
  (net 55 "Net-(SD1-Pad11)")
  (net 56 "Net-(SD1-Pad1)")
  (net 57 "Net-(U1-Pad5)")
  (net 58 "Net-(U1-Pad6)")
  (net 59 "Net-(U1-Pad12)")
  (net 60 "Net-(U1-Pad13)")
  (net 61 "Net-(U2-Pad9)")
  (net 62 "Net-(U2-Pad10)")
  (net 63 "Net-(U2-Pad11)")
  (net 64 "Net-(USB1-Pad4)")
  (net 65 "Net-(C5-Pad1)")
  (net 66 "Net-(L1-Pad2)")
  (net 67 sd_power_en)
  (net 68 sd_vdd)
  (net 69 "Net-(RN4-Pad1)")
  (net 70 "Net-(RN4-Pad2)")
  (net 71 fb)
  (net 72 "Net-(U3-Pad6)")
  (net 73 "Net-(C31-Pad1)")
  (net 74 vtest)
  (net 75 "Net-(U0-Pad1)")
  (net 76 "Net-(R1-Pad2)")
  (net 77 "Net-(ID1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BTN)
    (add_net Button1)
    (add_net Button2)
    (add_net Button3)
    (add_net CH1)
    (add_net CH2)
    (add_net CH3)
    (add_net CH4)
    (add_net CH5)
    (add_net CH6)
    (add_net DM)
    (add_net DP)
    (add_net FREE1)
    (add_net FREE2)
    (add_net I2S_BCLK)
    (add_net I2S_DATA)
    (add_net I2S_LRCLK)
    (add_net INT)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(ID1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(RN4-Pad1)")
    (add_net "Net-(RN4-Pad2)")
    (add_net "Net-(SD1-Pad1)")
    (add_net "Net-(SD1-Pad10)")
    (add_net "Net-(SD1-Pad11)")
    (add_net "Net-(SD1-Pad8)")
    (add_net "Net-(SD1-Pad9)")
    (add_net "Net-(U0-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(USB1-Pad4)")
    (add_net RESET)
    (add_net RX)
    (add_net SCL)
    (add_net SDA)
    (add_net SWDCLK)
    (add_net SWDIO)
    (add_net TX)
    (add_net amp_en)
    (add_net boost_en)
    (add_net fb)
    (add_net id-neopixel_data)
    (add_net miso)
    (add_net mosi)
    (add_net neopixel_data2)
    (add_net sclk)
    (add_net sd_en)
    (add_net sd_power_en)
    (add_net vtest)
  )
  (net_class LED ""
    (clearance 0.2)
    (trace_width 2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LED3-Pad1)")
    (add_net "Net-(LED4-Pad1)")
    (add_net "Net-(LED5-Pad1)")
    (add_net "Net-(LED6-Pad1)")
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.35)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3v)
    (add_net 5v)
    (add_net BATT+)
    (add_net BATT-)
    (add_net GND)
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(SP+1-Pad1)")
    (add_net "Net-(SP-1-Pad1)")
    (add_net VBUS)
    (add_net sd_vdd)
  )
  (module lightsaber_footprints:bridge (layer F.Cu) (tedit 5CFE18EC)
    (at 148.844 101.0285)
    (fp_text reference J1 (at 0 1.905) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -1.905) (layer F.Fab))
    (pad 2 thru_hole custom (at 1.27 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 BATT-) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_poly (pts
           (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875) (xy -0.5 -0.875)
           (xy -0.875 -0.5) (xy -0.875 0.5) (xy -0.5 0.875)) (width 0))
      ))
    (pad 2 connect rect (at 0.635 0) (size 0.85 1.5) (layers F.Cu F.Mask)
      (net 2 BATT-))
    (pad 1 connect rect (at -0.635 0) (size 0.85 1.5) (layers F.Cu F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 0 0) (size 0.51 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 thru_hole custom (at -1.27 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_poly (pts
           (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875) (xy -0.5 -0.875)
           (xy -0.875 -0.5) (xy -0.875 0.5) (xy -0.5 0.875)) (width 0))
      ))
  )
  (module lightsaber_footprints:XDFN4 (layer F.Cu) (tedit 5CB3BDFD)
    (at 146.05 104.3305 90)
    (fp_text reference U60 (at 0.7 0 180) (layer F.SilkS))
    (fp_text value NCP177 (at 0 -0.7 90) (layer F.Fab) hide)
    (pad 1 smd custom (at -0.325 0.48 90) (size 0.26 0.24) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.13 0.12) (xy 0.13 0.12) (xy 0.13 -0.12) (xy -0.02 -0.27) (xy -0.13 -0.27)
) (width 0))
      ))
    (pad 2 smd custom (at 0.325 0.48 270) (size 0.26 0.24) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.13 -0.12) (xy 0.13 -0.12) (xy 0.13 0.12) (xy -0.02 0.27) (xy -0.13 0.27)
) (width 0))
      ))
    (pad 3 smd custom (at 0.325 -0.48 270) (size 0.26 0.24) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C61-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.13 0.12) (xy 0.13 0.12) (xy 0.13 -0.12) (xy -0.02 -0.27) (xy -0.13 -0.27)
) (width 0))
      ))
    (pad 4 smd custom (at -0.325 -0.48 90) (size 0.26 0.24) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C61-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.13 -0.12) (xy 0.13 -0.12) (xy 0.13 0.12) (xy -0.02 0.27) (xy -0.13 0.27)
) (width 0))
      ))
    (pad 5 smd rect (at 0 0 135) (size 0.52 0.52) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/AMS_QFN-4-1EP_2x2mm_P0.95mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 144.5515 103.9495 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 0.0254 0.889 180) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C31-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:U-DFN2020-6 (layer B.Cu) (tedit 5C53ED36)
    (at 140.2842 107.9881 180)
    (descr "6-Lead Plastic Dual Flat, No Lead Package (MA) - 2x2x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.65")
    (attr smd)
    (fp_text reference Q7 (at -0.127 1.3716 180) (layer B.SilkS))
    (fp_text value DMP2075UFDB (at 0 -2.025 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0.65 180) (size 0.65 0.35) (layers B.Cu B.Paste B.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at -1.05 0 180) (size 0.65 0.35) (layers B.Cu B.Paste B.Mask)
      (net 67 sd_power_en))
    (pad 3 smd rect (at -1.05 -0.65 180) (size 0.65 0.35) (layers B.Cu B.Paste B.Mask)
      (net 1 BATT+))
    (pad 4 smd rect (at 1.05 -0.65 180) (size 0.65 0.35) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(C31-Pad1)"))
    (pad 5 smd rect (at 1.05 0 180) (size 0.65 0.35) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 6 smd rect (at 1.05 0.65 180) (size 0.65 0.35) (layers B.Cu B.Paste B.Mask)
      (net 68 sd_vdd))
    (pad 3 smd rect (at 0 -0.525 180) (size 1 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 BATT+) (solder_paste_margin_ratio -0.2))
    (pad 6 smd rect (at 0 0.525 180) (size 1 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 sd_vdd) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:2520 (layer B.Cu) (tedit 5C53E932)
    (at 147.574 103.3145)
    (fp_text reference L1 (at 0.0254 0.0762) (layer B.SilkS))
    (fp_text value "1.0 uH 4A" (at 0 0.5) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:uQFN6 (layer F.Cu) (tedit 5C53EBBF)
    (at 129.032 111.9505)
    (fp_text reference U40 (at -0.0254 -1.1684) (layer F.SilkS))
    (fp_text value HSP061-2M6 (at -0.025 -0.9) (layer F.Fab) hide)
    (pad 5 smd rect (at 0 -0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 VBUS))
    (pad 2 smd rect (at 0 0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 4 smd rect (at 0.5 -0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(RN4-Pad1)"))
    (pad 6 smd rect (at -0.5 -0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(RN4-Pad2)"))
    (pad 1 smd rect (at -0.5 0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(RN4-Pad2)"))
    (pad 3 smd rect (at 0.5 0.475) (size 0.25 0.65) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(RN4-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.75 0.5))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_footprints:ST2012SB (layer F.Cu) (tedit 5C53D731)
    (at 136.5286 103.1875 180)
    (fp_text reference Y1 (at 0 0 270) (layer F.SilkS))
    (fp_text value "ST2012SB 4pF" (at 0 -0.9 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.75 0 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C8-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_SeikoEpson_FA238V-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.7))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:LGA-14L (layer F.Cu) (tedit 5C53D684)
    (at 142.621 111.6965)
    (fp_text reference U2 (at -1.1938 -1.4478) (layer F.SilkS))
    (fp_text value LSM6DS3H (at 0 -0.3) (layer F.Fab))
    (pad 14 smd rect (at -0.5 -0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 SDA) (solder_paste_margin -0.0125))
    (pad 13 smd rect (at 0 -0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 SCL) (solder_paste_margin -0.0125))
    (pad 12 smd rect (at 0.5 -0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v) (solder_paste_margin -0.0125))
    (pad 11 smd rect (at 1.175 -0.75) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U2-Pad11)") (solder_paste_margin -0.0125))
    (pad 10 smd rect (at 1.175 -0.25) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U2-Pad10)") (solder_paste_margin -0.0125))
    (pad 9 smd rect (at 1.175 0.25) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U2-Pad9)") (solder_paste_margin -0.0125))
    (pad 8 smd rect (at 1.175 0.75) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v) (solder_paste_margin -0.0125))
    (pad 7 smd rect (at 0.5 0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin -0.0125))
    (pad 6 smd rect (at 0 0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin -0.0125))
    (pad 5 smd rect (at -0.5 0.925) (size 0.35 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v) (solder_paste_margin -0.0125))
    (pad 4 smd rect (at -1.175 0.75) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 48 INT) (solder_paste_margin -0.0125))
    (pad 3 smd rect (at -1.175 0.25) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin -0.0125))
    (pad 2 smd rect (at -1.175 -0.25) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin -0.0125))
    (pad 1 smd rect (at -1.175 -0.75) (size 0.55 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin -0.0125))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOD882D (layer F.Cu) (tedit 5C53D7CD)
    (at 144.272 104.3305 90)
    (fp_text reference D61 (at -0.9398 -0.1016 180) (layer F.SilkS))
    (fp_text value PMEG2005ELD (at 0.3 -0.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C61-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 BATT+) (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.step
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.17 0.17))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOD882D (layer F.Cu) (tedit 5C53D7CD)
    (at 142.24 104.3305 90)
    (fp_text reference D62 (at -0.9144 0 180) (layer F.SilkS))
    (fp_text value PMEG2005ELD (at 0.3 -0.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C61-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 VBUS) (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.step
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.17 0.17))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOD882D (layer F.Cu) (tedit 5C53D7CD)
    (at 143.256 104.3305 90)
    (fp_text reference D63 (at -0.9144 0 180) (layer F.SilkS))
    (fp_text value PMEG2005ELD (at 0.3 -0.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C61-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.4 0 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 5v) (solder_mask_margin 0.05) (solder_paste_margin -0.05))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.step
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.17 0.17))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:DMG7430LFG (layer F.Cu) (tedit 5C53D594)
    (at 152.4 103.9765)
    (fp_text reference Q1 (at 0 0.989) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.325) (size 2.37 1.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED1-Pad1)") (solder_paste_margin -0.1))
    (pad 1 smd rect (at -0.975 -1.3) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at 0.975 -1.3) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED1-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 CH1))
    (pad 3 smd rect (at 0.325 1.625) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 1.625) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.975 1.625) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_footprints:DMG7430LFG (layer B.Cu) (tedit 5C53D594)
    (at 152.4 103.9765 180)
    (fp_text reference Q2 (at 0 -0.9382 180) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 0.75 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.325 180) (size 2.37 1.9) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(LED2-Pad1)") (solder_paste_margin -0.1))
    (pad 1 smd rect (at -0.975 1.3 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at -0.325 1.3 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at 0.325 1.3 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at 0.975 1.3 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(LED2-Pad1)"))
    (pad 2 smd rect (at 0.975 -1.625 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 27 CH2))
    (pad 3 smd rect (at 0.325 -1.625 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 -1.625 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.975 -1.625 180) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_footprints:DMG7430LFG (layer F.Cu) (tedit 5C53D594)
    (at 154.432 108.6485 270)
    (fp_text reference Q3 (at 0 0.889 270) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.325 270) (size 2.37 1.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED3-Pad1)") (solder_paste_margin -0.1))
    (pad 1 smd rect (at -0.975 -1.3 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at 0.975 -1.3 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED3-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 28 CH3))
    (pad 3 smd rect (at 0.325 1.625 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 1.625 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.975 1.625 270) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_footprints:DMG7430LFG (layer B.Cu) (tedit 5C53D594)
    (at 154.432 108.6485 90)
    (fp_text reference Q4 (at 0 -0.889 90) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 0.75 90) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.325 90) (size 2.37 1.9) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(LED4-Pad1)") (solder_paste_margin -0.1))
    (pad 1 smd rect (at -0.975 1.3 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(LED4-Pad1)"))
    (pad 1 smd rect (at -0.325 1.3 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(LED4-Pad1)"))
    (pad 1 smd rect (at 0.325 1.3 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(LED4-Pad1)"))
    (pad 1 smd rect (at 0.975 1.3 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(LED4-Pad1)"))
    (pad 2 smd rect (at 0.975 -1.625 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 29 CH4))
    (pad 3 smd rect (at 0.325 -1.625 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 -1.625 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.975 -1.625 90) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_footprints:DMG7430LFG (layer F.Cu) (tedit 5C53D594)
    (at 152.4 113.4745 180)
    (fp_text reference Q5 (at 0 0.889 180) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.325 180) (size 2.37 1.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED5-Pad1)") (solder_paste_margin -0.1))
    (pad 1 smd rect (at -0.975 -1.3 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED5-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED5-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED5-Pad1)"))
    (pad 1 smd rect (at 0.975 -1.3 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LED5-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 30 CH5))
    (pad 3 smd rect (at 0.325 1.625 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 1.625 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.975 1.625 180) (size 0.42 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 BATT-))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_footprints:DMG7430LFG (layer B.Cu) (tedit 5C53D594)
    (at 152.4 113.4745)
    (fp_text reference Q6 (at 0 -0.9144) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 0.75) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0.325) (size 2.37 1.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED6-Pad1)") (solder_paste_margin -0.1))
    (pad 1 smd rect (at -0.975 1.3) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED6-Pad1)"))
    (pad 1 smd rect (at -0.325 1.3) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED6-Pad1)"))
    (pad 1 smd rect (at 0.325 1.3) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED6-Pad1)"))
    (pad 1 smd rect (at 0.975 1.3) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(LED6-Pad1)"))
    (pad 2 smd rect (at 0.975 -1.625) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 31 CH6))
    (pad 3 smd rect (at 0.325 -1.625) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.325 -1.625) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.975 -1.625) (size 0.42 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lightsaber_footprints:10118192 (layer F.Cu) (tedit 5C53D2EF)
    (at 124.714 108.6485 270)
    (fp_text reference USB1 (at 0 -1.4 270) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 -0.5 270) (layer F.Fab) hide)
    (pad 6 smd rect (at -3.1 -2.55 270) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 0 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(RN4-Pad2)"))
    (pad 6 smd rect (at 1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at -1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at -3.75 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at 3.75 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(RN4-Pad1)"))
    (pad 1 smd rect (at -1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 14 VBUS))
    (pad 4 smd rect (at 0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(USB1-Pad4)"))
    (pad 5 smd rect (at 1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at 3.1 -2.55 270) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (offset (xyz 0 1.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm (layer F.Cu) (tedit 5C52AE27)
    (at 135.03 109.1565 270)
    (descr "QFN, 48 Pin (http://www.st.com/resource/en/datasheet/stm32f042k6.pdf (Page 94)), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U0 (at -1.1684 -4.3144 270) (layer F.SilkS))
    (fp_text value STM32L433CCU6 (at 0 4.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 48 smd roundrect (at -2.75 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 3.3v))
    (pad 47 smd roundrect (at -2.25 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 46 smd roundrect (at -1.75 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 SDA))
    (pad 45 smd roundrect (at -1.25 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 CH2))
    (pad 44 smd roundrect (at -0.75 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 BTN))
    (pad 43 smd roundrect (at -0.25 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C5-Pad1)"))
    (pad 42 smd roundrect (at 0.25 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Button1))
    (pad 41 smd roundrect (at 0.75 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Button2))
    (pad 40 smd roundrect (at 1.25 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 Button3))
    (pad 39 smd roundrect (at 1.75 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 FREE2))
    (pad 38 smd roundrect (at 2.25 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 RX))
    (pad 37 smd roundrect (at 2.75 -3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 SWDCLK))
    (pad 36 smd roundrect (at 3.4375 -2.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 3.3v))
    (pad 35 smd roundrect (at 3.4375 -2.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 34 smd roundrect (at 3.4375 -1.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 SWDIO))
    (pad 33 smd roundrect (at 3.4375 -1.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 DP))
    (pad 32 smd roundrect (at 3.4375 -0.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 DM))
    (pad 31 smd roundrect (at 3.4375 -0.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 I2S_DATA))
    (pad 30 smd roundrect (at 3.4375 0.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 SCL))
    (pad 29 smd roundrect (at 3.4375 0.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 CH3))
    (pad 28 smd roundrect (at 3.4375 1.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CH5))
    (pad 27 smd roundrect (at 3.4375 1.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 sd_en))
    (pad 26 smd roundrect (at 3.4375 2.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 I2S_BCLK))
    (pad 25 smd roundrect (at 3.4375 2.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 I2S_LRCLK))
    (pad 24 smd roundrect (at 2.75 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 3.3v))
    (pad 23 smd roundrect (at 2.25 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 22 smd roundrect (at 1.75 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 sd_power_en))
    (pad 21 smd roundrect (at 1.25 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 neopixel_data2))
    (pad 20 smd roundrect (at 0.75 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 VBUS))
    (pad 19 smd roundrect (at 0.25 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CH4))
    (pad 18 smd roundrect (at -0.25 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CH6))
    (pad 17 smd roundrect (at -0.75 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 mosi))
    (pad 16 smd roundrect (at -1.25 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 miso))
    (pad 15 smd roundrect (at -1.75 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 sclk))
    (pad 14 smd roundrect (at -2.25 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 FREE1))
    (pad 13 smd roundrect (at -2.75 3.4375 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 vtest))
    (pad 12 smd roundrect (at -3.4375 2.75 270) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 TX))
    (pad 11 smd roundrect (at -3.4375 2.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 CH1))
    (pad 10 smd roundrect (at -3.4375 1.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 id-neopixel_data))
    (pad 9 smd roundrect (at -3.4375 1.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1-Pad2)"))
    (pad 8 smd roundrect (at -3.4375 0.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 7 smd roundrect (at -3.4375 0.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 RESET))
    (pad 6 smd roundrect (at -3.4375 -0.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 amp_en))
    (pad 5 smd roundrect (at -3.4375 -0.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 boost_en))
    (pad 4 smd roundrect (at -3.4375 -1.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C8-Pad1)"))
    (pad 3 smd roundrect (at -3.4375 -1.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C7-Pad1)"))
    (pad 2 smd roundrect (at -3.4375 -2.25 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT))
    (pad 1 smd roundrect (at -3.4375 -2.75 270) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(U0-Pad1)"))
    (pad "" smd roundrect (at 2.1 2.1 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 2.1 0.7 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 2.1 -0.7 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 2.1 -2.1 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.7 2.1 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.7 0.7 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.7 -0.7 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.7 -2.1 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.7 2.1 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.7 0.7 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.7 -0.7 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.7 -2.1 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -2.1 2.1 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -2.1 0.7 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -2.1 -0.7 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -2.1 -2.1 270) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad 49 smd roundrect (at 0 0 270) (size 5.55 5.55) (layers F.Cu F.Mask) (roundrect_rratio 0.045)
      (net 6 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 132.236 103.1875 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.1176 -0.0472) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 133.506 103.1875 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 1.1176 0.0036) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 139.446 106.1085 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 3.3v))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C53F0EF)
    (at 137.824 113.5575 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -0.7044 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 3.3v))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 140.11 108.9025)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.1234 -0.635) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 65 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C53F10E)
    (at 130.712 111.9505 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -0.664 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 3.3v))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 138.3955 103.1875 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0.0098 -0.6187 90) (layer F.SilkS))
    (fp_text value 5.6pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 134.649 103.1875 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -1.1108 0.0218 180) (layer F.SilkS))
    (fp_text value 5.6pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer B.Cu) (tedit 5C529E63)
    (at 148.336 114.1095 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 0.6604 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.55 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.55 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 11 5v))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 142.748 113.6015)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0.508 0.6858) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 3.3v))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 145.2292 111.5441)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at -0.0762 0.6604) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 3.3v))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 146.6088 109.4105 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C51 (at -0.2032 -0.6858 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 RESET))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E63)
    (at 146.05 102.9335)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C61 (at 0 -0.6604) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5 0) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(C61-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:fiduciary-small locked (layer B.Cu) (tedit 5A5A92F3)
    (at 143.51 110.0455)
    (attr virtual)
    (fp_text reference Ref** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0.5) (layer B.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer B.Cu) (tedit 5A5A92F3)
    (at 127.635 114.2365)
    (attr virtual)
    (fp_text reference Ref** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0.5) (layer B.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer B.Cu) (tedit 5A5A92F3)
    (at 127.254 103.3145)
    (attr virtual)
    (fp_text reference Ref** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0.5) (layer B.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers B.Cu B.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer F.Cu) (tedit 5A5A92F3)
    (at 143.383 107.1245)
    (attr virtual)
    (fp_text reference Ref** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer F.Cu) (tedit 5A5A92F3)
    (at 124.714 102.8065)
    (attr virtual)
    (fp_text reference Ref** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module lightsaber_footprints:fiduciary-small locked (layer F.Cu) (tedit 5A5A92F3)
    (at 124.7648 114.4397)
    (attr virtual)
    (fp_text reference Ref** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 0.75 0.75) (layers F.Cu F.Mask)
      (solder_mask_margin 0.3) (clearance 0.25))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 144.526 102.8065)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 0) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 5v))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 147.4724 110.1725 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at -0.0254 0 180) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 5v))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 147.4724 108.839 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 0.0127 180) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 5v))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.558 106.972 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C62 (at -0.0254 -0.9144 270) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 3.3v))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.966 103.1875 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at 0 -0.6132 90) (layer F.SilkS))
    (fp_text value "600 ferrite" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 3.3v))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_4x0402 (layer B.Cu) (tedit 58E0A888)
    (at 149.7965 109.9185)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 1.4) (layer B.SilkS))
    (fp_text value "100k 1%" (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -0.5 0.75) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 36 BTN))
    (pad 3 smd rect (at -0.5 -0.25) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 2 smd rect (at -0.5 0.25) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 4 smd rect (at -0.5 -0.75) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 7 smd rect (at 0.5 0.25) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 30 CH5))
    (pad 8 smd rect (at 0.5 0.75) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 6 smd rect (at 0.5 -0.25) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 28 CH3))
    (pad 5 smd rect (at 0.5 -0.75) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 29 CH4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_4x0402 (layer B.Cu) (tedit 58E0A888)
    (at 138.43 103.6193 180)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 1.4 180) (layer B.SilkS))
    (fp_text value "100k 1%" (at 0 -2.1 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 5 smd rect (at 0.5 -0.75 180) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 17 boost_en))
    (pad 6 smd rect (at 0.5 -0.25 180) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 27 CH2))
    (pad 8 smd rect (at 0.5 0.75 180) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 26 CH1))
    (pad 7 smd rect (at 0.5 0.25 180) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 31 CH6))
    (pad 4 smd rect (at -0.5 -0.75 180) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -0.5 0.25 180) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 3 smd rect (at -0.5 -0.25 180) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (pad 1 smd rect (at -0.5 0.75 180) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 2 BATT-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0402 (layer F.Cu) (tedit 58E0A89B)
    (at 143.4084 109.1565)
    (descr "Chip Resistor Network, ROHM MNR02 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at -0.0254 -1.016) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.8) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 4 smd rect (at 0.5 -0.35) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 3 smd rect (at 0.5 0.35) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at -0.5 0.35) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 SCL))
    (pad 1 smd rect (at -0.5 -0.35) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0402 (layer F.Cu) (tedit 58E0A89B)
    (at 127.508 113.9825 180)
    (descr "Chip Resistor Network, ROHM MNR02 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at 0.0508 -1.1176 180) (layer F.SilkS))
    (fp_text value 22ohm (at 0 1.8 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -0.5 -0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(RN4-Pad1)"))
    (pad 2 smd rect (at -0.5 0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(RN4-Pad2)"))
    (pad 3 smd rect (at 0.5 0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 DP))
    (pad 4 smd rect (at 0.5 -0.35 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 DM))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Concave_4x0402 (layer B.Cu) (tedit 58E0A888)
    (at 143.7894 107.7595 90)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN5 (at 0 -1.4224 90) (layer B.SilkS))
    (fp_text value "100k 1%" (at 0 -2.1 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.5 0.75 90) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 3 smd rect (at -0.5 -0.25 90) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 37 sd_en))
    (pad 2 smd rect (at -0.5 0.25 90) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 4 smd rect (at -0.5 -0.75 90) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 67 sd_power_en))
    (pad 7 smd rect (at 0.5 0.25 90) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 38 amp_en))
    (pad 8 smd rect (at 0.5 0.75 90) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 71 fb))
    (pad 6 smd rect (at 0.5 -0.25 90) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 68 sd_vdd))
    (pad 5 smd rect (at 0.5 -0.75 90) (size 0.5 0.32) (layers B.Cu B.Paste B.Mask)
      (net 8 3.3v))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP2.7x2.7mm_ThermalVias (layer B.Cu) (tedit 5A650620)
    (at 145.669 112.9665 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 2.85 270) (layer B.SilkS))
    (fp_text value MAX98357A_TQFN (at 0 -2.85 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 51 I2S_DATA))
    (pad 2 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 3 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 4 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 38 amp_en))
    (pad 5 smd oval (at -0.75 -1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(U1-Pad5)"))
    (pad 6 smd oval (at -0.25 -1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(U1-Pad6)"))
    (pad 7 smd oval (at 0.25 -1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 8 smd oval (at 0.75 -1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 9 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(SP+1-Pad1)"))
    (pad 10 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(SP-1-Pad1)"))
    (pad 11 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 12 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(U1-Pad12)"))
    (pad 13 smd oval (at 0.75 1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(U1-Pad13)"))
    (pad 14 smd oval (at 0.25 1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 49 I2S_LRCLK))
    (pad 15 smd oval (at -0.25 1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 16 smd oval (at -0.75 1.475 180) (size 0.75 0.3) (layers B.Cu B.Paste B.Mask)
      (net 50 I2S_BCLK))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers F.Cu)
      (net 6 GND))
    (pad "" smd rect (at 0.5 0.5 270) (size 0.73 0.73) (layers B.Paste))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers B.Cu B.Mask)
      (net 6 GND))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad 17 thru_hole circle (at -0.5 0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad 17 thru_hole circle (at 0.5 0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad 17 thru_hole circle (at 0.5 -0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad 17 thru_hole circle (at -0.5 -0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 6 GND))
    (pad "" smd rect (at -0.5 0.5 270) (size 0.73 0.73) (layers B.Paste))
    (pad "" smd rect (at -0.5 -0.5 270) (size 0.73 0.73) (layers B.Paste))
    (pad "" smd rect (at 0.5 -0.5 270) (size 0.73 0.73) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP2.7x2.7mm_ThermalVias.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm (layer B.Cu) (tedit 5A65EDEB)
    (at 147.447 106.3117 180)
    (descr "VSON 10 Thermal on 11 3x3mm Pitch 0.5mm http://chip.tomsk.ru/chip/chipdoc.nsf/Package/D8A64DD165C2AAD9472579400024FC41!OpenDocument")
    (tags "VSON 10 Thermal on 11 3x3mm Pitch 0.5mm")
    (attr smd)
    (fp_text reference U3 (at -2.3876 -0.1016) (layer B.SilkS))
    (fp_text value TPS61230DRCR (at 0 -3 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.475 1 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(L1-Pad2)"))
    (pad 2 smd rect (at -1.475 0.5 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(L1-Pad2)"))
    (pad 3 smd rect (at -1.475 0 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 4 smd rect (at -1.475 -0.5 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 11 5v))
    (pad 5 smd rect (at -1.475 -1 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R1-Pad2)"))
    (pad 6 smd rect (at 1.475 -1 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at 1.475 -0.5 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 71 fb))
    (pad 8 smd rect (at 1.475 0 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 1.475 0.5 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 17 boost_en))
    (pad 10 smd rect (at 1.475 1 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(C31-Pad1)"))
    (pad 11 smd rect (at 0 0 180) (size 1.65 2.4) (layers B.Cu B.Mask)
      (net 6 GND))
    (pad "" smd rect (at 0.4125 -0.8 180) (size 0.64 0.64) (layers B.Paste))
    (pad 11 smd rect (at -0.25 1.55 180) (size 0.28 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 11 smd rect (at -0.25 -1.55 180) (size 0.28 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 11 smd rect (at 0.25 1.55 180) (size 0.28 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 11 smd rect (at 0.25 -1.55 180) (size 0.28 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad "" smd rect (at -0.4125 -0.8 180) (size 0.64 0.64) (layers B.Paste))
    (pad "" smd rect (at -0.4125 0 180) (size 0.64 0.64) (layers B.Paste))
    (pad "" smd rect (at 0.4125 0 180) (size 0.64 0.64) (layers B.Paste))
    (pad "" smd rect (at -0.4125 0.8 180) (size 0.64 0.64) (layers B.Paste))
    (pad "" smd rect (at 0.4125 0.8 180) (size 0.64 0.64) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Card:microSD_HC_Hirose_DM3D-SF (layer B.Cu) (tedit 5B82D16A)
    (at 130.175 108.6485 90)
    (descr "Micro SD, SMD, right-angle, push-pull (https://media.digikey.com/PDF/Data%20Sheets/Hirose%20PDFs/DM3D-SF.pdf)")
    (tags "Micro SD")
    (attr smd)
    (fp_text reference SD1 (at -0.0762 7.1882 90) (layer B.SilkS))
    (fp_text value microsd_socket (at -0.025 -6.975 90) (layer B.Fab))
    (fp_text user KEEPOUT (at -0.275 0.525 90) (layer Cmts.User))
    (fp_text user %R (at -0.025 -1.475 90) (layer B.Fab))
    (fp_text user KEEPOUT (at -0.725 4.8 90) (layer Cmts.User))
    (pad 8 smd rect (at -4.525 -5.35 90) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(SD1-Pad8)"))
    (pad 11 smd rect (at -5.725 -5.225 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(SD1-Pad11)"))
    (pad 11 smd rect (at -5.975 2.375 90) (size 0.8 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(SD1-Pad11)"))
    (pad 9 smd rect (at -5.65 3.875 90) (size 1.45 1) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(SD1-Pad9)"))
    (pad 11 smd rect (at 5.975 3.025 90) (size 0.8 1.4) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(SD1-Pad11)"))
    (pad 7 smd rect (at -3.425 -5.35 90) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 40 miso))
    (pad 6 smd rect (at -2.325 -5.35 90) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 5 smd rect (at -1.225 -5.35 90) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 41 sclk))
    (pad 4 smd rect (at -0.125 -5.35 90) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 68 sd_vdd))
    (pad 3 smd rect (at 0.975 -5.35 90) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 42 mosi))
    (pad 2 smd rect (at 2.075 -5.35 90) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 37 sd_en))
    (pad 1 smd rect (at 3.175 -5.35 90) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(SD1-Pad1)"))
    (pad 11 smd rect (at 5.625 -5.225 90) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(SD1-Pad11)"))
    (pad 10 smd rect (at 5.575 5.45 90) (size 1 1.55) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(SD1-Pad10)"))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3D-SF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:hose (layer B.Cu) (tedit 5C551DA5)
    (at 150.114 103.251)
    (fp_text reference hose1 (at 0.25 -1.75) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 1.75) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.6 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 BATT-))
  )
  (module lightsaber_footprints:hose (layer B.Cu) (tedit 5D05BA8C)
    (at 150.114 113.919)
    (fp_text reference hose2 (at 0.25 -1.75) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 1.75) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.6 3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 BATT-))
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer B.Cu) (tedit 5C529E93)
    (at 142.375 105.8545 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R1 (at 0 0.75 180) (layer B.SilkS))
    (fp_text value "410k 1%" (at 0 -0.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.59 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.59 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 5v))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer B.Cu) (tedit 5C529E93)
    (at 144.264 105.9815)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R2 (at 0 0.7112) (layer B.SilkS))
    (fp_text value "410k 1%" (at 0 -0.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.5 0) (size 0.59 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 5v))
    (pad 2 smd roundrect (at 0.5 0) (size 0.59 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 fb))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer B.Cu) (tedit 5C529E93)
    (at 144.145 104.9655 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R3 (at 0 0.75 180) (layer B.SilkS))
    (fp_text value "410k 1%" (at 0 -0.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.59 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C31-Pad1)"))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.59 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 vtest))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer B.Cu) (tedit 5C529E93)
    (at 141.986 104.2115 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R4 (at 0 0.75 90) (layer B.SilkS))
    (fp_text value "410k 1%" (at 0 -0.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.59 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.59 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 vtest))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:KXT331LHS (layer F.Cu) (tedit 5CA2E0E7)
    (at 148.463 105.3465 270)
    (fp_text reference SW1 (at 0 0.5 270) (layer F.SilkS))
    (fp_text value SW_Push (at -0.1 -0.6 270) (layer F.Fab))
    (pad 1 smd rect (at -1.625 0 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 3.3v))
    (pad 2 smd rect (at 1.625 0 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 36 BTN))
    (model ${KIPRJMOD}/lightsaber_footprints.pretty/KXT331LHS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:KXT331LHS (layer F.Cu) (tedit 5CA2E0E7)
    (at 148.463 111.9505 90)
    (fp_text reference SW2 (at 0 0.5 90) (layer F.SilkS))
    (fp_text value SW_Push (at -0.1 -0.6 90) (layer F.Fab))
    (pad 2 smd rect (at 1.625 0 90) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 RESET))
    (pad 1 smd rect (at -1.625 0 90) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model ${KIPRJMOD}/lightsaber_footprints.pretty/KXT331LHS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 132.236 100.9845)
    (fp_text reference 33v1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 8 3.3v) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 142.494 101.0285)
    (fp_text reference 5V1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 5v) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 145.034 101.0285)
    (fp_text reference BATT+1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 BATT+) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCF5D)
    (at 150.114 116.2685)
    (fp_text reference BATT-2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 BATT-) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 155.194 101.0285)
    (fp_text reference BT1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 Button1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 155.096 116.2245)
    (fp_text reference BT2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 Button2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 142.494 116.2685)
    (fp_text reference BT3 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 Button3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 124.714 101.0285)
    (fp_text reference FR1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 FREE1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 139.954 116.2245)
    (fp_text reference FR2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 FREE2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCF7A)
    (at 134.776 100.9845)
    (fp_text reference gnd2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:hose (layer F.Cu) (tedit 5CFDE01B)
    (at 150.114 113.919)
    (fp_text reference hose3 (at 0.25 1.75) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.75) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.6 3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 BATT-))
  )
  (module lightsaber_footprints:hose (layer F.Cu) (tedit 5CFDE00F)
    (at 150.114 103.251)
    (fp_text reference hose4 (at 0.25 1.75) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.75) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.6 3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 BATT-))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 127.254 116.2245)
    (fp_text reference PX2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 neopixel_data2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 137.414 116.2245)
    (fp_text reference RX1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 39 RX) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 129.794 116.2685)
    (fp_text reference SCL1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 33 SCL) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 139.954 101.0285)
    (fp_text reference SDA1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 SDA) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 124.714 116.2685)
    (fp_text reference SDVDD1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 68 sd_vdd) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 147.574 116.2685)
    (fp_text reference SP+1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(SP+1-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 145.034 116.2685)
    (fp_text reference SP-1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(SP-1-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 134.874 116.2245)
    (fp_text reference SWDCLK1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 45 SWDCLK) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 132.334 116.2245)
    (fp_text reference SWDIO1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 46 SWDIO) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 127.156 100.9845)
    (fp_text reference TX1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 47 TX) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 129.696 100.9845)
    (fp_text reference ID1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(ID1-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-rounded_square (layer F.Cu) (tedit 5CFDCBD9)
    (at 137.316 100.9845)
    (fp_text reference RESET1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 RESET) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center -0.5 0.5) (end -0.125 0.5) (width 0))
        (gr_circle (center -0.5 -0.5) (end -0.125 -0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_poly (pts
           (xy -0.5 0.875) (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875)
           (xy -0.5 -0.875) (xy -0.875 -0.5) (xy -0.875 0.5)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-flatside-roundedcorners (layer F.Cu) (tedit 5CFE0825)
    (at 155.194 103.5685)
    (fp_text reference LED2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(LED2-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_circle (center -0.325 -0.5) (end 0.05 -0.5) (width 0))
        (gr_circle (center -0.325 0.5) (end 0.05 0.5) (width 0))
        (gr_poly (pts
           (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875) (xy -0.325 -0.875)
           (xy -0.7 -0.5) (xy -0.7 0.5) (xy -0.325 0.875)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-flatside-roundedcorners (layer F.Cu) (tedit 5CFE0825)
    (at 155.194 106.1085 90)
    (fp_text reference LED3 (at 0 1 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1 90) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0 90) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(LED3-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_circle (center -0.325 -0.5) (end 0.05 -0.5) (width 0))
        (gr_circle (center -0.325 0.5) (end 0.05 0.5) (width 0))
        (gr_poly (pts
           (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875) (xy -0.325 -0.875)
           (xy -0.7 -0.5) (xy -0.7 0.5) (xy -0.325 0.875)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-flatside-roundedcorners (layer F.Cu) (tedit 5CFE0825)
    (at 155.194 111.1885 270)
    (fp_text reference LED4 (at 0 1 270) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1 270) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0 270) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(LED4-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_circle (center -0.325 -0.5) (end 0.05 -0.5) (width 0))
        (gr_circle (center -0.325 0.5) (end 0.05 0.5) (width 0))
        (gr_poly (pts
           (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875) (xy -0.325 -0.875)
           (xy -0.7 -0.5) (xy -0.7 0.5) (xy -0.325 0.875)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-flatside-roundedcorners (layer F.Cu) (tedit 5CFE0825)
    (at 155.194 113.7285)
    (fp_text reference LED5 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(LED5-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_circle (center -0.325 -0.5) (end 0.05 -0.5) (width 0))
        (gr_circle (center -0.325 0.5) (end 0.05 0.5) (width 0))
        (gr_poly (pts
           (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875) (xy -0.325 -0.875)
           (xy -0.7 -0.5) (xy -0.7 0.5) (xy -0.325 0.875)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-flatside-roundedcorners (layer F.Cu) (tedit 5CFE0825)
    (at 152.556 101.0285 90)
    (fp_text reference LED1 (at 0 1 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1 90) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0 90) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(LED1-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_circle (center -0.325 -0.5) (end 0.05 -0.5) (width 0))
        (gr_circle (center -0.325 0.5) (end 0.05 0.5) (width 0))
        (gr_poly (pts
           (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875) (xy -0.325 -0.875)
           (xy -0.7 -0.5) (xy -0.7 0.5) (xy -0.325 0.875)) (width 0))
      ))
  )
  (module lightsaber_footprints:1pin-flatside-roundedcorners (layer F.Cu) (tedit 5CFE0825)
    (at 152.556 116.2245 270)
    (fp_text reference LED6 (at 0 1 270) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1 270) (layer F.Fab))
    (pad 1 thru_hole custom (at 0 0 270) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(LED6-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_circle (center 0.5 0.5) (end 0.875 0.5) (width 0))
        (gr_circle (center 0.5 -0.5) (end 0.875 -0.5) (width 0))
        (gr_circle (center -0.325 -0.5) (end 0.05 -0.5) (width 0))
        (gr_circle (center -0.325 0.5) (end 0.05 0.5) (width 0))
        (gr_poly (pts
           (xy 0.5 0.875) (xy 0.875 0.5) (xy 0.875 -0.5) (xy 0.5 -0.875) (xy -0.325 -0.875)
           (xy -0.7 -0.5) (xy -0.7 0.5) (xy -0.325 0.875)) (width 0))
      ))
  )
  (module lightsaber_footprints:C_0402_1005Metric (layer F.Cu) (tedit 5C529E93)
    (at 129.286 103.1875)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference R5 (at -0.508 -0.635) (layer F.SilkS))
    (fp_text value 470 (at 0 0.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 0) (size 0.59 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(ID1-Pad1)"))
    (pad 2 smd roundrect (at 0.5 0) (size 0.59 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 id-neopixel_data))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Made by\nFredrik\nHubinette" (at 139.954 112.5855) (layer B.SilkS))
  (gr_text "ProffieBoard    V2.2" (at 135.509 114.1095) (layer F.SilkS))
  (gr_line (start 155.829 117.5385) (end 124.079 117.5385) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.079 99.7585) (end 155.829 99.7585) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.464 100.3935) (end 156.464 116.9035) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.444 116.9035) (end 123.444 100.3935) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 155.829 100.3935) (end 155.829 99.7585) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 124.079 100.3935) (end 123.444 100.3935) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 124.079 116.9035) (end 124.079 117.5385) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 155.829 116.9035) (end 156.464 116.9035) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 8) (net_name 3.3v) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.444 101.6635) (xy 149.098 101.6635) (xy 149.098 115.6335) (xy 123.444 115.6335)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.444 101.6635) (xy 145.4785 101.6635) (xy 146.939 100.2665) (xy 148.336 101.6635) (xy 148.336 115.6335)
        (xy 123.444 115.6335)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.6325 105.5565) (xy 131.601 105.5565) (xy 131.601 113.621) (xy 129.6325 113.621)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.444 101.6635) (xy 136.144 101.6635) (xy 148.844 101.6635) (xy 148.844 115.6335) (xy 123.444 115.6335)
      )
    )
  )
  (zone (net 2) (net_name BATT-) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 104.3305) (xy 151.638 104.3305) (xy 151.638 99.7585) (xy 149.098 99.7585) (xy 149.098 102.2985)
        (xy 147.955 102.2985) (xy 147.955 117.5385) (xy 151.638 117.5385) (xy 151.638 112.9665) (xy 153.924 112.9665)
      )
    )
  )
  (zone (net 2) (net_name BATT-) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.464 99.7585) (xy 148.844 99.7585) (xy 148.844 117.5385) (xy 156.464 117.5385)
      )
    )
  )
  (zone (net 2) (net_name BATT-) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.464 99.7585) (xy 149.352 99.7585) (xy 149.352 117.5385) (xy 156.464 117.5385)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.8362 108.1727) (xy 135.8428 108.1727) (xy 135.8174 110.6873) (xy 133.8362 110.6873)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.444 101.6635) (xy 146.05 101.6635) (xy 146.812 100.7745) (xy 148.082 101.7905) (xy 147.574 102.2985)
        (xy 147.574 115.6335) (xy 123.444 115.6335)
      )
    )
  )
  (zone (net 2) (net_name BATT-) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.178 104.5845) (xy 151.638 104.5845) (xy 151.638 99.7585) (xy 149.098 99.7585) (xy 149.098 117.5385)
        (xy 151.638 117.5385) (xy 151.638 112.9665) (xy 154.178 112.9665)
      )
    )
  )
)
