(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4~bpo8+1)
  (general
    (links 0)
    (no_connects 0)
    (area 47.726189 64.995 91.973812 77.845)
    (thickness 1.6)
    (drawings 4)
    (tracks 250)
    (zones 0)
    (modules 3)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.16)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.16)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Pin_Headers:Pin_Header_Straight_1x20 (layer F.Cu) (tedit 0)
    (at 93.9546 79.4512 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x20 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 45.72 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 0 48.26 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x20.wrl
      (at (xyz 0 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Molex:Molex_SlimStack_Receptacle_02x20_0.5mm_52991-10408 (layer F.Cu) (tedit 55E7D192)
    (at 69.85 71.12)
    (descr "Molex Slimstack connector 02X20 contacts 0.5mm pitch 3mm mated height")
    (tags "Slimstack 3mm 02x20 0.5mm pitch")
    (attr smd)
    (fp_text reference REF** (at 0 5.75) (layer F.SilkS))
    (fp_text value Molex_SlimStack_Receptacle_02x20_0.5mm_52991-10408 (at 0 -5.25) (layer F.Fab))
    (pad 1 smd rect (at -4.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -3.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -3.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -3.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -3.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -2.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -2.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -2.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -1.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -1.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -0.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -0.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -0.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 0.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 0.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 0.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 0.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 1.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 1.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 1.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 1.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 2.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 2.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 2.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at 2.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 2.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 3.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 3.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at 3.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at 3.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at 4.25 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 4.25 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 4.75 -2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 4.75 2) (size 0.26 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x20 (layer F.Cu) (tedit 0)
    (at 45.7454 62.4332 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x20 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x20.wrl
      (at (xyz 0 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 97.79 83.82) (end 41.91 83.82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 58.42) (end 97.79 83.82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.91 58.42) (end 97.79 58.42) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.91 83.82) (end 41.91 58.42) (layer Edge.Cuts) (width 0.15))
)
