(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 0)
    (no_connects 7)
    (area 71.044999 68.504999 137.235001 102.945001)
    (thickness 1.6)
    (drawings 16)
    (tracks 33)
    (zones 0)
    (modules 7)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.016)
    (user_trace_width 1.2192)
    (user_trace_width 2.54)
    (user_trace_width 5.08)
    (trace_clearance 0.2032)
    (zone_clearance 1)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.9144)
    (via_drill 0.508)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.9144)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(K1-Pad4)")
  (net 3 "Net-(K1-Pad5)")
  (net 4 "Net-(K1-Pad3)")
  (net 5 VCC)
  (net 6 "Net-(P1-Pad2)")
  (net 7 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.9144)
    (via_drill 0.508)
    (uvia_dia 0.9144)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(K1-Pad5)")
    (add_net "Net-(P1-Pad2)")
    (add_net VCC)
  )
  (module Connectors:FCI_20020107-3p (layer F.Cu) (tedit 576B180E)
    (at 76.5556 80.0227 270)
    (fp_text reference P1 (at -6.35 -4.572 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -5 0 90) (size 2.5 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.5 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 90) (size 2.5 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 552FFCCE)
    (at 92.59316 78.8035 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D1 (at 5.38734 2.53746 270) (layer F.SilkS))
    (fp_text value 1n400x (at 4.37134 -3.55854 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
  )
  (module relays:JQX-15F (layer F.Cu) (tedit 57AD4BB1)
    (at 96.295905 77.939571 270)
    (fp_text reference K1 (at -6.082971 2.989005 450) (layer F.SilkS))
    (fp_text value RELAY_SPST (at -4.597071 -3.627695 360) (layer F.Fab))
    (pad 4 thru_hole oval (at 14.892029 -25.235795) (size 4 6) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(K1-Pad4)"))
    (pad 5 thru_hole oval (at 14.892029 -17.635795) (size 4 6) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(K1-Pad5)"))
    (pad 3 thru_hole oval (at -2.907971 -15.095795) (size 4 6) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(K1-Pad3)"))
    (pad 1 thru_hole circle (at 11.092029 -2.435795 90) (size 2.5 2.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 0.892029 -2.435795 90) (size 2.5 2.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
  )
  (module Connectors:FCI_20020107-3p (layer F.Cu) (tedit 576B180E)
    (at 131.1656 88.1596 90)
    (fp_text reference P2 (at -6.35 -4.572 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -5 0 270) (size 2.5 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(K1-Pad5)"))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.5 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(K1-Pad4)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 2.5 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(K1-Pad3)"))
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical_LargePads (layer F.Cu) (tedit 0)
    (at 85.9917 81.4197 270)
    (descr "TO-220, Neutral, Vertical, Large Pads,")
    (tags "TO-220, Neutral, Vertical, Large Pads,")
    (fp_text reference Q1 (at 0 -5.08 270) (layer F.SilkS))
    (fp_text value FQP30N06L (at 0 3.81 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 82.1055 77.1906 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.32892 -3.50012 360) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 57AD5154)
    (at 76.12 97.87)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text GND (at 73.025 85.09 90) (layer B.SilkS))
  (gr_text SIG (at 73.025 80.01 90) (layer B.SilkS))
  (gr_text 5V (at 73.025 74.93 90) (layer B.SilkS))
  (gr_text GND (at 73.025 85.09 90) (layer F.SilkS))
  (gr_text SIG (at 73.025 80.01 90) (layer F.SilkS))
  (gr_text 5V (at 73.025 74.93 90) (layer F.SilkS))
  (gr_line (start 71.12 102.87) (end 71.12 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 102.87) (end 71.12 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 68.58) (end 137.16 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.12 68.58) (end 137.16 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_text NO (at 134.62 92.964 90) (layer B.SilkS))
  (gr_text NC (at 134.62 88.265 90) (layer B.SilkS))
  (gr_text NO (at 134.62 92.964 90) (layer F.SilkS))
  (gr_text NC (at 134.62 88.265 90) (layer F.SilkS))
  (gr_text "C\n" (at 134.62 83.1215 90) (layer B.SilkS))
  (gr_text "C\n" (at 134.62 83.312 90) (layer F.SilkS))
  (zone (net 4) (net_name "Net-(K1-Pad3)") (layer B.Cu) (hatch full 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.095 85.09) (xy 135.89 85.09) (xy 135.89 71.12) (xy 108.458 71.12) (xy 108.458 81.28)
        (xy 121.285 81.28)
      )
    )
  )
  (zone (net 3) (net_name "Net-(K1-Pad5)") (layer F.Cu) (hatch full 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.89 91.44) (xy 135.89 102.235) (xy 110.49 102.235) (xy 110.49 88.9) (xy 117.475 88.9)
        (xy 117.475 88.9) (xy 117.475 98.425) (xy 127.635 98.425) (xy 127.635 91.44) (xy 127.635 91.44)
      )
    )
  )
  (zone (net 3) (net_name "Net-(K1-Pad5)") (layer B.Cu) (hatch full 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.635 91.44) (xy 135.89 91.44) (xy 135.89 102.235) (xy 110.49 102.235) (xy 110.49 88.9)
        (xy 117.475 88.9) (xy 117.475 98.425) (xy 127.635 98.425)
      )
    )
  )
  (zone (net 2) (net_name "Net-(K1-Pad4)") (layer F.Cu) (hatch full 0.508)
    (priority 1)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.635 97.155) (xy 127.635 90.805) (xy 135.89 90.805) (xy 135.89 85.725) (xy 118.11 85.725)
        (xy 118.11 88.9) (xy 118.11 97.155)
      )
    )
  )
  (zone (net 2) (net_name "Net-(K1-Pad4)") (layer B.Cu) (hatch full 0.508)
    (priority 1)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.11 85.725) (xy 135.89 85.725) (xy 135.89 90.805) (xy 127.635 90.805) (xy 127.635 97.155)
        (xy 118.11 97.155)
      )
    )
  )
  (zone (net 4) (net_name "Net-(K1-Pad3)") (layer F.Cu) (hatch full 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.89 85.09) (xy 125.095 85.09) (xy 121.285 81.28) (xy 108.458 81.28) (xy 108.458 71.12)
        (xy 126.746 71.12) (xy 135.89 71.12)
      )
    )
  )
)
