(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 214)
    (zones 0)
    (modules 20)
    (nets 46)
  )
  (page A4)
  (title_block
    (title "ESP to RS232 Software Serial Bridge")
    (date 2019-02-12)
    (rev "v1.1 Rev 3")
    (company NetwiZe.be)
    (comment 3 "License: CC BY-SA 4.0")
    (comment 4 "Author: Francis Van Roie")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.55)
    (trace_clearance 0.35)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.2)
    (via_size 0.6858)
    (via_drill 0.35)
    (via_min_size 0.25)
    (via_min_drill 0.3)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 1.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 129.794 79.502)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(J1-Pad4)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(J2-Pad1)")
  (net 11 "Net-(J2-Pad4)")
  (net 12 "Net-(J2-Pad6)")
  (net 13 "Net-(J2-Pad7)")
  (net 14 "Net-(J2-Pad8)")
  (net 15 "Net-(J2-Pad9)")
  (net 16 "Net-(R1-Pad2)")
  (net 17 "Net-(R2-Pad2)")
  (net 18 RXD)
  (net 19 TXD)
  (net 20 "Net-(U2-Pad7)")
  (net 21 "Net-(U2-Pad9)")
  (net 22 "Net-(U2-Pad10)")
  (net 23 GPIO16)
  (net 24 GPIO14)
  (net 25 RIN)
  (net 26 TOUT)
  (net 27 GPIO4)
  (net 28 GPIO5)
  (net 29 "Net-(SW1-Pad2)")
  (net 30 "Net-(C2-Pad2)")
  (net 31 "Net-(U2-Pad8)")
  (net 32 "Net-(U3-Pad1)")
  (net 33 "Net-(U3-Pad2)")
  (net 34 "Net-(U3-Pad6)")
  (net 35 "Net-(U3-Pad7)")
  (net 36 "Net-(U3-Pad9)")
  (net 37 "Net-(U3-Pad10)")
  (net 38 "Net-(U3-Pad11)")
  (net 39 "Net-(U3-Pad12)")
  (net 40 "Net-(U3-Pad13)")
  (net 41 "Net-(U3-Pad14)")
  (net 42 "Net-(U3-Pad17)")
  (net 43 "Net-(C1-Pad2)")
  (net 44 "Net-(C2-Pad1)")
  (net 45 "Net-(SW1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.35)
    (trace_width 0.55)
    (via_dia 0.6858)
    (via_drill 0.35)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GPIO14)
    (add_net GPIO16)
    (add_net GPIO4)
    (add_net GPIO5)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW1-Pad4)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad9)")
    (add_net RIN)
    (add_net RXD)
    (add_net TOUT)
    (add_net TXD)
  )
  (net_class Ground ""
    (clearance 0.25)
    (trace_width 0.75)
    (via_dia 0.6858)
    (via_drill 0.35)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
  )
  (net_class Power ""
    (clearance 0.25)
    (trace_width 0.75)
    (via_dia 0.6858)
    (via_drill 0.35)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net +5V)
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO14580 (layer F.Cu) (tedit 56D1B4CB)
    (at 149.7744 82.8924)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO14580")
    (tags "mounting hole 2.2mm no annular m2 iso14580")
    (attr virtual)
    (fp_text reference H1 (at 0 -5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 -6.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO14580 (layer F.Cu) (tedit 56D1B4CB)
    (at 149.7744 107.8924)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO14580")
    (tags "mounting hole 2.2mm no annular m2 iso14580")
    (attr virtual)
    (fp_text reference H2 (at 0 8) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 9.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module "AliExpress:AliExpress 5 pin Micro USB SMT B" (layer F.Cu) (tedit 5C5EB457)
    (at 131.953 95.0976 270)
    (attr smd)
    (fp_text reference J1 (at 0 -4.2 90) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 3.194 270) (layer F.Fab))
    (pad 1 smd rect (at -1.4 -2.77 270) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V) (clearance 0.2) (zone_connect 2) (thermal_gap 0.2))
    (pad 2 smd rect (at -0.65 -2.77 270) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad2)") (clearance 0.2))
    (pad 3 smd rect (at 0 -2.77 270) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad3)") (clearance 0.2))
    (pad 4 smd rect (at 0.65 -2.77 270) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad4)") (clearance 0.2))
    (pad 5 smd rect (at 1.4 -2.77 270) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (clearance 0.2) (zone_connect 2))
    (pad "" np_thru_hole circle (at -2 -2.15 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1) (zone_connect 0))
    (pad 6 smd rect (at -3.95 0 270) (size 1.4 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad "" np_thru_hole circle (at 2 -2.15 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1) (zone_connect 0))
    (pad 6 smd rect (at 3.95 0 270) (size 1.4 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (model "${KIPRJMOD}/Hirose Micro USB Digikey PN H11635CT-ND.step"
      (offset (xyz 0 -2.7 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 5C44D661)
    (at 133.2484 106.68)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 9.2964 180) (layer F.Fab) hide)
  )
  (module "AliExpress:SKSCPCE010 ALPS" (layer F.Cu) (tedit 5C5EB335)
    (at 131.4696 87.0204 270)
    (attr smd)
    (fp_text reference SW1 (at 0 -0.0508 180) (layer F.SilkS))
    (fp_text value PRG (at 0 2.6416 270) (layer F.Fab))
    (pad 3 smd rect (at -1.8 0.65 270) (size 1.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 1.8 -0.65 270) (size 1.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(SW1-Pad2)"))
    (pad 4 smd rect (at -1.8 -0.65 270) (size 1.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(SW1-Pad4)"))
    (pad 1 smd rect (at 1.8 0.65 270) (size 1.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (model U:/Projects/KiCad/Models/ALPS/SKSCPCE010/untitled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5C5968F3)
    (at 143.9164 97.3074)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6.1722 90) (layer F.SilkS))
    (fp_text value MAX3232 (at 1.27 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 TOUT))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 RIN))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 GPIO14))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 GPIO16))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad10)"))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad9)"))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad8)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad7)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C1-Pad2)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C2-Pad2)"))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C3644FA)
    (at 150.7744 89.0524)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (zone_connect 2)
    (fp_text reference J3 (at -0.4572 -2.3368 90) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 1.6256 6.35 270) (layer F.Fab))
    (fp_text user %R (at 0 15.1384 180) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 TXD) (zone_connect 2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 RXD) (zone_connect 2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 GPIO5) (zone_connect 2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 GPIO4) (zone_connect 2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5C62957D)
    (at 133.1468 81.9924 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.921 -0.0508 90) (layer F.SilkS))
    (fp_text value 10k (at 4.5 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Module:ESP-12E (layer B.Cu) (tedit 5C3B5733)
    (at 139.7 98.552)
    (descr "Wi-Fi Module, http://wiki.ai-thinker.com/_media/esp8266/docs/aithinker_esp_12f_datasheet_en.pdf")
    (tags "Wi-Fi Module")
    (attr smd)
    (fp_text reference U3 (at 0 0.0675 180 unlocked) (layer B.SilkS))
    (fp_text value ESP-12F (at 0.254 13.7795) (layer B.Fab))
    (fp_text user Antenna (at -0.06 7 -180) (layer Cmts.User))
    (fp_text user "KEEP-OUT ZONE" (at 0.03 9.55 -180) (layer Cmts.User))
    (fp_text user %R (at 0.49 0.8) (layer B.Fab))
    (pad 1 smd rect (at -7.6 3.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -7.6 1.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -7.6 -0.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(R1-Pad2)"))
    (pad 4 smd rect (at -7.6 -2.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 23 GPIO16))
    (pad 5 smd rect (at -7.6 -4.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 24 GPIO14))
    (pad 6 smd rect (at -7.6 -6.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -7.6 -8.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -7.6 -10.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 9 smd rect (at -5 -12) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at -3 -12) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(U3-Pad10)"))
    (pad 11 smd rect (at -1 -12) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U3-Pad11)"))
    (pad 12 smd rect (at 1 -12) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U3-Pad12)"))
    (pad 13 smd rect (at 3 -12) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U3-Pad13)"))
    (pad 14 smd rect (at 5 -12) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U3-Pad14)"))
    (pad 15 smd rect (at 7.6 -10.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 16 smd rect (at 7.6 -8.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (pad 17 smd rect (at 7.6 -6.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U3-Pad17)"))
    (pad 18 smd rect (at 7.6 -4.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(SW1-Pad2)"))
    (pad 19 smd rect (at 7.6 -2.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 27 GPIO4))
    (pad 20 smd rect (at 7.6 -0.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 28 GPIO5))
    (pad 21 smd rect (at 7.6 1.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 18 RXD))
    (pad 22 smd rect (at 7.6 3.5) (size 2.5 1) (layers B.Cu B.Paste B.Mask)
      (net 19 TXD))
    (model ${KIPRJMOD}/ESP-12F.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm (layer F.Cu) (tedit 5C366EBA)
    (at 153.9748 89.8524 90)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (fp_text reference J2 (at 8.674 -2.1336 90) (layer F.SilkS))
    (fp_text value DB9_Female (at -5.296 6.7564 270) (layer F.Fab))
    (fp_text user %R (at -12.2048 2.7432 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -2.77 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 26 TOUT))
    (pad 3 thru_hole circle (at -5.54 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 RIN))
    (pad 4 thru_hole circle (at -8.31 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at -11.08 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 thru_hole circle (at -1.385 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at -4.155 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at -6.925 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at -9.695 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad9)"))
    (pad 0 thru_hole circle (at -18.04 1.42 90) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at 6.96 1.42 90) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/DB9 - 203-09SCKKBE.STEP"
      (offset (xyz -5.5 -10.5 6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C3B79F7)
    (at 137.9982 81.9924 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (zone_connect 2)
    (attr smd)
    (fp_text reference C8 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 -15.24 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V) (zone_connect 2))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5C391ED1)
    (at 135.7 83.3882)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.06948 -1.7018 180 unlocked) (layer B.SilkS))
    (fp_text value 0.1uF (at -12.6624 -0.0254) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C3B79A6)
    (at 137.9982 93.75696 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.651 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 15.24) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C3B79B4)
    (at 137.9982 97.67848 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.651 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 15.24) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C3B814A)
    (at 137.9982 89.83544 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.651 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 15.24) (layer F.Fab))
    (fp_text user %R (at 0 -0.095001 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C3B79C7)
    (at 137.9982 101.6 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.651 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 -15.24 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5C629575)
    (at 133.1468 101.6 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.9718 -0.0508 90 unlocked) (layer F.SilkS))
    (fp_text value 10k (at 4.5 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5C392080)
    (at 143.7 83.3882)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0.0508 -1.8368 180 unlocked) (layer B.SilkS))
    (fp_text value 10uF (at -16.3444 0.0254 unlocked) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C5C9549)
    (at 137.9982 85.91392 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.651 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 15.24) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5C3CF19F)
    (at 144.0688 85.6996 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at -0.254 -4.2672 270) (layer F.SilkS))
    (fp_text value AMS1117-3.3 (at 1.27 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 270) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.15 2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PRG (at 133.8 87.0204 90) (layer F.SilkS))
  (gr_text "Software Serial Bridge" (at 137.2108 105.918) (layer F.SilkS))
  (gr_text "PCB design by NetwiZe.be\nCC-BY-SA 2019-01-20" (at 137.2108 108.966) (layer F.SilkS))
  (gr_text USB (at 131.896 95.0976 90) (layer F.SilkS))
  (gr_text 5 (at 148.6408 96.6724 90) (layer F.SilkS))
  (gr_text TX (at 148.6408 101.7524 90) (layer F.SilkS))
  (gr_text 3V3 (at 148.6408 88.5952 90) (layer F.SilkS))
  (gr_text GND (at 148.6408 91.5924 90) (layer F.SilkS))
  (gr_text RX (at 148.6408 99.2124 90) (layer F.SilkS))
  (gr_text 4 (at 148.6393 94.1324 90) (layer F.SilkS))
  (gr_arc (start 157.762 108.7628) (end 157.762016 110.7948) (angle -89.99954885) (layer Edge.Cuts) (width 0.01))
  (gr_text TX (at 142.452915 105.150035 180) (layer B.SilkS))
  (gr_text RX (at 142.452915 106.368335 180) (layer B.SilkS))
  (gr_text SW.Serial (at 142.452915 107.689135 180) (layer B.SilkS))
  (gr_text 16 (at 137.068115 105.149135 180) (layer B.SilkS))
  (gr_text 14 (at 137.068115 106.368335 180) (layer B.SilkS))
  (gr_text GPIO (at 137.068115 107.689135 180) (layer B.SilkS))
  (gr_arc (start 131.834 108.7755) (end 129.794 108.7628) (angle -90.1) (layer Edge.Cuts) (width 0.005))
  (gr_arc (start 157.754 82.024606) (end 159.794 82.016622) (angle -89.6) (layer Edge.Cuts) (width 0.005))
  (dimension 30.83561 (width 0.15) (layer Eco1.User)
    (gr_text "30.83 mm" (at 126.741402 95.398138 89.95280415) (layer Eco1.User))
    (feature1 (pts (xy 131.9022 110.8202) (xy 127.442282 110.816526)))
    (feature2 (pts (xy 131.9276 79.9846) (xy 127.467682 79.980926)))
    (crossbar (pts (xy 128.054102 79.981409) (xy 128.028702 110.817009)))
    (arrow1a (pts (xy 128.028702 110.817009) (xy 127.443209 109.690023)))
    (arrow1b (pts (xy 128.028702 110.817009) (xy 128.61605 109.690989)))
    (arrow2a (pts (xy 128.054102 79.981409) (xy 127.466754 81.107429)))
    (arrow2b (pts (xy 128.054102 79.981409) (xy 128.639595 81.108395)))
  )
  (dimension 29.9974 (width 0.15) (layer Eco1.User)
    (gr_text "30 mm" (at 144.7927 113.834699) (layer Eco1.User))
    (feature1 (pts (xy 159.7914 109.3724) (xy 159.7914 113.12112)))
    (feature2 (pts (xy 129.794 109.3724) (xy 129.794 113.12112)))
    (crossbar (pts (xy 129.794 112.534699) (xy 159.7914 112.534699)))
    (arrow1a (pts (xy 159.7914 112.534699) (xy 158.664896 113.12112)))
    (arrow1b (pts (xy 159.7914 112.534699) (xy 158.664896 111.948278)))
    (arrow2a (pts (xy 129.794 112.534699) (xy 130.920504 113.12112)))
    (arrow2b (pts (xy 129.794 112.534699) (xy 130.920504 111.948278)))
  )
  (gr_text ESP-12 (at 139.700001 95.8342 180) (layer B.SilkS))
  (gr_arc (start 131.826 82.0166) (end 131.825984 79.9846) (angle -89.99954885) (layer Edge.Cuts) (width 0.01))
  (gr_text "ESP to RS232 v1.1" (at 137.2108 104.648) (layer F.SilkS))
  (gr_line (start 159.7914 82.0166) (end 159.794 108.7628) (layer Edge.Cuts) (width 0.005))
  (gr_line (start 131.826 79.9846) (end 157.7594 79.9846) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 129.794 108.7628) (end 129.794 82.0166) (layer Edge.Cuts) (width 0.005))
  (gr_line (start 157.7594 110.7948) (end 131.826 110.815524) (layer Edge.Cuts) (width 0.01))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.29845 103.2637) (xy 127.3556 77.7748) (xy 162.8267 77.7494) (xy 162.76955 103.2383)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.2908 98.9076) (xy 135.3312 99.0092) (xy 135.3312 93.3196) (xy 142.2908 93.218)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.720725 79.085282) (xy 127.655638 83.20286) (xy 146.054763 83.217941) (xy 146.2024 103.251) (xy 162.306 103.2764)
        (xy 161.98215 79.25435)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.6604 83.7692) (xy 127.587057 103.178745) (xy 145.3388 103.2002) (xy 145.3388 83.7692)
      )
    )
  )
)
