(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 43)
    (no_connects 0)
    (area 117.692238 60.264 153.173 96.215)
    (thickness 1.6)
    (drawings 15)
    (tracks 189)
    (zones 0)
    (modules 22)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 117.856 92.964)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (gerberprecision 5)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D1-Pad1)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(F1-Pad1)")
  (net 11 "Net-(R1-Pad1)")
  (net 12 "Net-(R4-Pad2)")
  (net 13 "Net-(JP1-Pad1)")
  (net 14 "Net-(JP1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net VCC)
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 0)
    (at 138.43 84.074)
    (attr smd)
    (fp_text reference C1 (at -2.032 -2.54) (layer F.SilkS))
    (fp_text value 1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 131.318 85.852)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 2.286 1.778) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 0)
    (at 130.556 77.978)
    (attr smd)
    (fp_text reference C3 (at 3.556 2.032) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 0)
    (at 144.018 80.518 270)
    (attr smd)
    (fp_text reference C4 (at -2.286 -2.54 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 149.606 75.184 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -2.032 2.286 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 147.066 89.916)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -2.286 -2.3) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 134.112 73.66)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -2) (layer F.SilkS))
    (fp_text value LED (at 0 2) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 138.43 90.17 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at -3.556 -1.524 180) (layer F.SilkS))
    (fp_text value LED (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module NR_Footprints:Polyfuse_Littelfuse_1206L025 (layer F.Cu) (tedit 577E419C)
    (at 120.904 73.406 270)
    (fp_text reference F1 (at 1.27 2.032 360) (layer F.SilkS))
    (fp_text value 1206L025 (at 1.8 -2 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 2.8 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 130.048 68.072)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -1.016 -2.54) (layer F.SilkS))
    (fp_text value "Batt Pwr" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 131.064 82.042)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 2.54 2.032) (layer F.SilkS))
    (fp_text value 470K (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 141.732 73.152)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -2.794 -2.032) (layer F.SilkS))
    (fp_text value 3K3 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 138.43 76.962)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 2.286 2.54) (layer F.SilkS))
    (fp_text value 0.25R (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 123.698 85.598)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 131.318 90.17 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -2.54 -2.032 180) (layer F.SilkS))
    (fp_text value 3K3 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NR_Footprints:SOT23_5pins_LTC (layer F.Cu) (tedit 577E22BA)
    (at 119.634 79.502 270)
    (fp_text reference U1 (at 3.81 0.254 360) (layer F.SilkS))
    (fp_text value LTC4411 (at 0.889 -4.445 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.9 0 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.9 -2.62 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad1)"))
    (pad 5 smd rect (at 0 -2.62 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
  )
  (module NR_Footprints:SOT23_5pins_LTC (layer F.Cu) (tedit 577E22BA)
    (at 125.984 72.898 270)
    (fp_text reference U2 (at 3.556 0.508 360) (layer F.SilkS))
    (fp_text value LTC4054-4.2 (at 0.889 -4.445 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.9 0 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(JP1-Pad2)"))
    (pad 4 smd rect (at 1.9 -2.62 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at 0 -2.62 270) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R4-Pad2)"))
  )
  (module NR_Footprints:TSOT-23_8_pins_LT (layer F.Cu) (tedit 577E3EF7)
    (at 121.92 89.916 270)
    (fp_text reference U3 (at 1.778 2.286 360) (layer F.SilkS))
    (fp_text value LT3060-3.3 (at 1.524 -4.318 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 0.4 1.22) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.65 0 270) (size 0.4 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.3 0 270) (size 0.4 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.95 0 270) (size 0.4 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.95 -2.62 270) (size 0.4 1.22) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 6 smd rect (at 1.3 -2.62 270) (size 0.4 1.22) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 7 smd rect (at 0.65 -2.62 270) (size 0.4 1.22) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 8 smd rect (at 0 -2.62 270) (size 0.4 1.22) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
  )
  (module Oddities:NetTie-I_SMD (layer F.Cu) (tedit 0)
    (at 140.716 68.072)
    (descr "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC. Make connection between 1 and 2 by yourself.")
    (tags "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC. Make connection between 1 and 2 by yourself.")
    (fp_text reference JP1 (at -0.04064 -1.778) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.048) (layer F.Fab))
    (pad 1 smd rect (at -2.54 0) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 2.54 0) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(JP1-Pad2)"))
  )
  (module NR_Footprints:JST_2pin_Male_LiPo (layer F.Cu) (tedit 577E6CB3)
    (at 147.574 68.072)
    (fp_text reference P2 (at 2.667 2.413) (layer F.SilkS))
    (fp_text value "Batt Chg" (at 1.397 -2.032) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(JP1-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Connect:USB_Micro-B_10103594-0001LF (layer F.Cu) (tedit 560290CC)
    (at 122.428 67.564 180)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P3 (at -1.5 -4.625 180) (layer F.SilkS))
    (fp_text value USB_A (at 0 6.175 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at -0.65 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.0009 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.3 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.425 -1.625 270) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 2.425 -1.625 270) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at -2.725 1.375 270) (size 1.7 1.2) (drill oval 1.2 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 2.725 1.375 270) (size 1.7 1.2) (drill oval 1.2 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 6 smd rect (at -0.9625 1.625 270) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.9625 1.625 270) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 149.098 82.042 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 5.08 -1.016 540) (layer F.SilkS))
    (fp_text value "PWR OUT" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text ON (at 138.43 87.884) (layer F.SilkS))
  (gr_text "OSHW\nOpen Source Hardware" (at 133.858 73.152) (layer B.SilkS))
  (gr_text "RupTek\nLiPo Manager\nJuly 2016." (at 134.112 88.138) (layer B.SilkS))
  (gr_text "Power Out" (at 146.558 83.312 90) (layer F.SilkS))
  (gr_text "Batt Pwr Out" (at 133.858 65.532) (layer F.SilkS))
  (gr_text "Batt Chg" (at 148.844 65.786) (layer F.SilkS))
  (gr_text Charging (at 134.62 70.358) (layer F.SilkS))
  (gr_text LTC4054 (at 129.286 71.12) (layer F.SilkS))
  (gr_text LTC4411 (at 124.206 80.01 90) (layer F.SilkS))
  (gr_text LT3060 (at 120.142 88.138) (layer F.SilkS))
  (gr_line (start 117.856 64.262) (end 151.892 64.262) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.856 64.516) (end 117.856 64.262) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.892 92.964) (end 151.892 64.262) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.856 92.964) (end 151.892 92.964) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.856 64.262) (end 117.856 92.964) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.638 92.71) (xy 118.11 92.71) (xy 118.11 64.516) (xy 151.638 64.516) (xy 151.638 92.71)
      )
    )
  )
)
