(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 5)
    (no_connects 0)
    (area 129.150001 100.3 263.85 147.700001)
    (thickness 1.6)
    (drawings 32)
    (tracks 0)
    (zones 0)
    (modules 12)
    (nets 2)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory PDF/))
  )
  (net 0 "")
  (net 1 shield)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net shield)
  )
  (module Mounting_Holes:MountingHole_5.3mm_M5 (layer F.Cu) (tedit 5B432B3E)
    (at 215 122)
    (descr "Mounting Hole 5.3mm, no annular, M5")
    (tags "mounting hole 5.3mm no annular m5")
    (attr virtual)
    (fp_text reference REF** (at 0 -8) (layer F.SilkS) hide)
    (fp_text value MountingHole_5.3mm_M5 (at 0 6.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 5.3 5.3) (drill 5.3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B432677)
    (at 152 135)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 3) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B43267E)
    (at 152 117)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B432686)
    (at 248 117)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B43268D)
    (at 248 135)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 3) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_5.3mm_M5 (layer F.Cu) (tedit 5B432B32)
    (at 185 122)
    (descr "Mounting Hole 5.3mm, no annular, M5")
    (tags "mounting hole 5.3mm no annular m5")
    (attr virtual)
    (fp_text reference REF** (at 0 -8) (layer F.SilkS) hide)
    (fp_text value MountingHole_5.3mm_M5 (at 0 6.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 5.3 5.3) (drill 5.3) (layers *.Cu *.Mask))
  )
  (module coverfootprint:MountingHole_11mm_Pad (layer F.Cu) (tedit 5B434C0D)
    (at 236 126)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference J1 (at 0 -9.4) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 9.4) (layer F.Fab) hide)
    (fp_text user %R (at 0 -10.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 13 13) (drill 11) (layers *.Cu *.Mask)
      (net 1 shield))
  )
  (module coverfootprint:MountingHole_11mm_Pad (layer F.Cu) (tedit 5B434C0D)
    (at 224 126)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference J2 (at 0 -9.4) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 9.4) (layer F.Fab) hide)
    (fp_text user %R (at 0 -10.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 13 13) (drill 11) (layers *.Cu *.Mask)
      (net 1 shield))
  )
  (module coverfootprint:MountingHole_11mm_Pad (layer F.Cu) (tedit 5B434C0D)
    (at 206 126)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference J3 (at 0 -9.4) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 9.4) (layer F.Fab) hide)
    (fp_text user %R (at 0 -10.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 13 13) (drill 11) (layers *.Cu *.Mask)
      (net 1 shield))
  )
  (module coverfootprint:MountingHole_11mm_Pad (layer F.Cu) (tedit 5B434C0D)
    (at 194 126)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference J4 (at 0 -9.4) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 9.4) (layer F.Fab) hide)
    (fp_text user %R (at 0 -10.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 13 13) (drill 11) (layers *.Cu *.Mask)
      (net 1 shield))
  )
  (module coverfootprint:MountingHole_11mm_Pad (layer F.Cu) (tedit 5B434C0D)
    (at 176 126)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference J5 (at 0 -9.4) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 9.4) (layer F.Fab) hide)
    (fp_text user %R (at 0 -10.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 13 13) (drill 11) (layers *.Cu *.Mask)
      (net 1 shield))
  )
  (module coverfootprint:MountingHole_11mm_Pad (layer F.Cu) (tedit 5B434C0D)
    (at 164 126)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference J6 (at 0 -9.4) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 9.4) (layer F.Fab) hide)
    (fp_text user %R (at 0 -10.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 13 13) (drill 11) (layers *.Cu *.Mask)
      (net 1 shield))
  )
  (gr_text pierremuth.wordpress.com (at 237 135) (layer B.Mask))
  (gr_text mini-nixie (at 158.5 135) (layer B.Mask))
  (gr_text mini-nixie (at 158.5 135) (layer F.Mask))
  (gr_text pierremuth.wordpress.com (at 237 135) (layer F.Mask))
  (dimension 7 (width 0.3) (layer Cmts.User)
    (gr_text "7,000 mm" (at 257.35 118.5 270) (layer Cmts.User))
    (feature1 (pts (xy 250 122) (xy 258.7 122)))
    (feature2 (pts (xy 250 115) (xy 258.7 115)))
    (crossbar (pts (xy 256 115) (xy 256 122)))
    (arrow1a (pts (xy 256 122) (xy 255.413579 120.873496)))
    (arrow1b (pts (xy 256 122) (xy 256.586421 120.873496)))
    (arrow2a (pts (xy 256 115) (xy 255.413579 116.126504)))
    (arrow2b (pts (xy 256 115) (xy 256.586421 116.126504)))
  )
  (dimension 7 (width 0.3) (layer Cmts.User)
    (gr_text "7,000 mm" (at 143.65 118.5 270) (layer Cmts.User))
    (feature1 (pts (xy 150 122) (xy 142.3 122)))
    (feature2 (pts (xy 150 115) (xy 142.3 115)))
    (crossbar (pts (xy 145 115) (xy 145 122)))
    (arrow1a (pts (xy 145 122) (xy 144.413579 120.873496)))
    (arrow1b (pts (xy 145 122) (xy 145.586421 120.873496)))
    (arrow2a (pts (xy 145 115) (xy 144.413579 116.126504)))
    (arrow2b (pts (xy 145 115) (xy 145.586421 116.126504)))
  )
  (dimension 35 (width 0.3) (layer Cmts.User)
    (gr_text "35.000 mm" (at 232.5 108.65) (layer Cmts.User))
    (feature1 (pts (xy 215 115) (xy 215 107.3)))
    (feature2 (pts (xy 250 115) (xy 250 107.3)))
    (crossbar (pts (xy 250 110) (xy 215 110)))
    (arrow1a (pts (xy 215 110) (xy 216.126504 109.413579)))
    (arrow1b (pts (xy 215 110) (xy 216.126504 110.586421)))
    (arrow2a (pts (xy 250 110) (xy 248.873496 109.413579)))
    (arrow2b (pts (xy 250 110) (xy 248.873496 110.586421)))
  )
  (dimension 35 (width 0.3) (layer Cmts.User)
    (gr_text "35.000 mm" (at 167.5 108.65) (layer Cmts.User))
    (feature1 (pts (xy 185 115) (xy 185 107.3)))
    (feature2 (pts (xy 150 115) (xy 150 107.3)))
    (crossbar (pts (xy 150 110) (xy 185 110)))
    (arrow1a (pts (xy 185 110) (xy 183.873496 110.586421)))
    (arrow1b (pts (xy 185 110) (xy 183.873496 109.413579)))
    (arrow2a (pts (xy 150 110) (xy 151.126504 110.586421)))
    (arrow2b (pts (xy 150 110) (xy 151.126504 109.413579)))
  )
  (dimension 11 (width 0.3) (layer Cmts.User)
    (gr_text "11.000 mm" (at 257.35 131.5 90) (layer Cmts.User))
    (feature1 (pts (xy 250 126) (xy 258.7 126)))
    (feature2 (pts (xy 250 137) (xy 258.7 137)))
    (crossbar (pts (xy 256 137) (xy 256 126)))
    (arrow1a (pts (xy 256 126) (xy 256.586421 127.126504)))
    (arrow1b (pts (xy 256 126) (xy 255.413579 127.126504)))
    (arrow2a (pts (xy 256 137) (xy 256.586421 135.873496)))
    (arrow2b (pts (xy 256 137) (xy 255.413579 135.873496)))
  )
  (dimension 14 (width 0.3) (layer Cmts.User)
    (gr_text "14.000 mm" (at 243 146.35) (layer Cmts.User))
    (feature1 (pts (xy 250 137) (xy 250 147.7)))
    (feature2 (pts (xy 236 137) (xy 236 147.7)))
    (crossbar (pts (xy 236 145) (xy 250 145)))
    (arrow1a (pts (xy 250 145) (xy 248.873496 145.586421)))
    (arrow1b (pts (xy 250 145) (xy 248.873496 144.413579)))
    (arrow2a (pts (xy 236 145) (xy 237.126504 145.586421)))
    (arrow2b (pts (xy 236 145) (xy 237.126504 144.413579)))
  )
  (dimension 12 (width 0.3) (layer Cmts.User)
    (gr_text "12.000 mm" (at 230 142.35) (layer Cmts.User))
    (feature1 (pts (xy 236 137) (xy 236 143.7)))
    (feature2 (pts (xy 224 137) (xy 224 143.7)))
    (crossbar (pts (xy 224 141) (xy 236 141)))
    (arrow1a (pts (xy 236 141) (xy 234.873496 141.586421)))
    (arrow1b (pts (xy 236 141) (xy 234.873496 140.413579)))
    (arrow2a (pts (xy 224 141) (xy 225.126504 141.586421)))
    (arrow2b (pts (xy 224 141) (xy 225.126504 140.413579)))
  )
  (dimension 18 (width 0.3) (layer Cmts.User)
    (gr_text "18.000 mm" (at 215 146.35) (layer Cmts.User))
    (feature1 (pts (xy 224 137) (xy 224 147.7)))
    (feature2 (pts (xy 206 137) (xy 206 147.7)))
    (crossbar (pts (xy 206 145) (xy 224 145)))
    (arrow1a (pts (xy 224 145) (xy 222.873496 145.586421)))
    (arrow1b (pts (xy 224 145) (xy 222.873496 144.413579)))
    (arrow2a (pts (xy 206 145) (xy 207.126504 145.586421)))
    (arrow2b (pts (xy 206 145) (xy 207.126504 144.413579)))
  )
  (dimension 12 (width 0.3) (layer Cmts.User)
    (gr_text "12.000 mm" (at 200 142.35) (layer Cmts.User))
    (feature1 (pts (xy 206 137) (xy 206 143.7)))
    (feature2 (pts (xy 194 137) (xy 194 143.7)))
    (crossbar (pts (xy 194 141) (xy 206 141)))
    (arrow1a (pts (xy 206 141) (xy 204.873496 141.586421)))
    (arrow1b (pts (xy 206 141) (xy 204.873496 140.413579)))
    (arrow2a (pts (xy 194 141) (xy 195.126504 141.586421)))
    (arrow2b (pts (xy 194 141) (xy 195.126504 140.413579)))
  )
  (dimension 18 (width 0.3) (layer Cmts.User)
    (gr_text "18.000 mm" (at 185 146.35) (layer Cmts.User))
    (feature1 (pts (xy 194 137) (xy 194 147.7)))
    (feature2 (pts (xy 176 137) (xy 176 147.7)))
    (crossbar (pts (xy 176 145) (xy 194 145)))
    (arrow1a (pts (xy 194 145) (xy 192.873496 145.586421)))
    (arrow1b (pts (xy 194 145) (xy 192.873496 144.413579)))
    (arrow2a (pts (xy 176 145) (xy 177.126504 145.586421)))
    (arrow2b (pts (xy 176 145) (xy 177.126504 144.413579)))
  )
  (dimension 12 (width 0.3) (layer Cmts.User)
    (gr_text "12.000 mm" (at 170 142.35) (layer Cmts.User))
    (feature1 (pts (xy 176 137) (xy 176 143.7)))
    (feature2 (pts (xy 164 137) (xy 164 143.7)))
    (crossbar (pts (xy 164 141) (xy 176 141)))
    (arrow1a (pts (xy 176 141) (xy 174.873496 141.586421)))
    (arrow1b (pts (xy 176 141) (xy 174.873496 140.413579)))
    (arrow2a (pts (xy 164 141) (xy 165.126504 141.586421)))
    (arrow2b (pts (xy 164 141) (xy 165.126504 140.413579)))
  )
  (dimension 14 (width 0.3) (layer Cmts.User)
    (gr_text "14.000 mm" (at 157 146.35) (layer Cmts.User))
    (feature1 (pts (xy 164 137) (xy 164 147.7)))
    (feature2 (pts (xy 150 137) (xy 150 147.7)))
    (crossbar (pts (xy 150 145) (xy 164 145)))
    (arrow1a (pts (xy 164 145) (xy 162.873496 145.586421)))
    (arrow1b (pts (xy 164 145) (xy 162.873496 144.413579)))
    (arrow2a (pts (xy 150 145) (xy 151.126504 145.586421)))
    (arrow2b (pts (xy 150 145) (xy 151.126504 144.413579)))
  )
  (dimension 22 (width 0.3) (layer Cmts.User)
    (gr_text "22.000 mm" (at 135.65 126 270) (layer Cmts.User))
    (feature1 (pts (xy 150 137) (xy 134.3 137)))
    (feature2 (pts (xy 150 115) (xy 134.3 115)))
    (crossbar (pts (xy 137 115) (xy 137 137)))
    (arrow1a (pts (xy 137 137) (xy 136.413579 135.873496)))
    (arrow1b (pts (xy 137 137) (xy 137.586421 135.873496)))
    (arrow2a (pts (xy 137 115) (xy 136.413579 116.126504)))
    (arrow2b (pts (xy 137 115) (xy 137.586421 116.126504)))
  )
  (dimension 100 (width 0.3) (layer Cmts.User)
    (gr_text "100.000 mm" (at 200 101.65) (layer Cmts.User))
    (feature1 (pts (xy 250 115) (xy 250 100.3)))
    (feature2 (pts (xy 150 115) (xy 150 100.3)))
    (crossbar (pts (xy 150 103) (xy 250 103)))
    (arrow1a (pts (xy 250 103) (xy 248.873496 103.586421)))
    (arrow1b (pts (xy 250 103) (xy 248.873496 102.413579)))
    (arrow2a (pts (xy 150 103) (xy 151.126504 103.586421)))
    (arrow2b (pts (xy 150 103) (xy 151.126504 102.413579)))
  )
  (gr_line (start 150 137) (end 150 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 250 137) (end 150 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 250 115) (end 150 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 250 137) (end 250 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name shield) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.6) (smoothing chamfer))
    (polygon
      (pts
        (xy 250 115) (xy 150 115) (xy 150 137) (xy 250 137) (xy 250 127)
      )
    )
  )
  (zone (net 1) (net_name shield) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.6) (smoothing chamfer))
    (polygon
      (pts
        (xy 250 115) (xy 150 115) (xy 150 137) (xy 250 137)
      )
    )
  )
)
