(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/VREGIN")
  (net 2 "/RST#")
  (net 3 "/AC9")
  (net 4 "/AC8")
  (net 5 "/AC7")
  (net 6 "/AC6")
  (net 7 "/AC5")
  (net 8 "/AC4")
  (net 9 "/AC3")
  (net 10 "/AC2")
  (net 11 "/AC1")
  (net 12 "/AC0")
  (net 13 "/SHLD")
  (net 14 "/VCCIO")
  (net 15 "/3V3-U")
  (net 16 "/PU2")
  (net 17 "/PU1")
  (net 18 "/AD0")
  (net 19 "/AD1")
  (net 20 "/AD2")
  (net 21 "/AD3")
  (net 22 "/AD4")
  (net 23 "/AD5")
  (net 24 "/AD6")
  (net 25 "/AD7")
  (net 26 "/3V3-F")
  (net 27 "/SPI-MISO")
  (net 28 "/CDONE")
  (net 29 "/CRESET")
  (net 30 "/SPI-CS")
  (net 31 "/SPI-MOSI")
  (net 32 "/USR03")
  (net 33 "/G3-USR04")
  (net 34 "/USR05")
  (net 35 "/USR06")
  (net 36 "/USR07")
  (net 37 "/USR08")
  (net 38 "/5V0-F")
  (net 39 "/SPI-CLK")
  (net 40 "/USR30")
  (net 41 "/RGB2")
  (net 42 "/RGB0")
  (net 43 "/USR27")
  (net 44 "/USR26")
  (net 45 "/USR25")
  (net 46 "/USR24")
  (net 47 "/USR23")
  (net 48 "/USR22")
  (net 49 "/USR21")
  (net 50 "/USR20")
  (net 51 "GND")
  (net 52 "/VBUS")
  (net 53 "/USR09")
  (net 54 "/USR10")
  (net 55 "/USR11")
  (net 56 "/USR12")
  (net 57 "/G0_USR13")
  (net 58 "/USR14")
  (net 59 "/USR19")
  (net 60 "/USR18")
  (net 61 "/G6_USR17")
  (net 62 "/G1_USR15")
  (net 63 "/NEO_OUT")
  (net 64 "/RGB1")
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 43.815 53.34 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 3.81 -0.073) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 34 "/USR05") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 22 "/AD4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 43.815 45.72 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 40 "/USR30") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "/AD1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_DCW_Library:Conn_2x7_hole40mil_pad60-75mil_pitch100mil" (layer "F.Cu")
    (at 40.64 74.93 90)
    (property "DigiKey#" "")
    (property "JLCPCB-LCSC" "")
    (property "Manufacturer" "")
    (property "Mfr_Part#" "")
    (property "Mouser#" "")
    (property "Newark#" "")
    (property "Package" "")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "")
    (property "Value3" "")
    (property "ki_description" "14-pin header")
    (property "ki_keywords" "header")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -11.43 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2x7 100mil" (at -1.27 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.27 -7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 59 "/USR19") (pinfunction "1") (pintype "passive"))
    (pad "1" smd circle (at -1.27 -7.62 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 59 "/USR19") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 -7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 26 "/3V3-F") (pinfunction "2") (pintype "power_in"))
    (pad "2" smd circle (at 1.27 -7.62 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 26 "/3V3-F") (pinfunction "2") (pintype "power_in"))
    (pad "3" thru_hole circle (at -1.27 -5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 51 "GND") (pinfunction "3") (pintype "power_in"))
    (pad "3" smd circle (at -1.27 -5.08 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 51 "GND") (pinfunction "3") (pintype "power_in"))
    (pad "4" thru_hole circle (at 1.27 -5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 53 "/USR09") (pinfunction "4") (pintype "passive"))
    (pad "4" smd circle (at 1.27 -5.08 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 53 "/USR09") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -1.27 -2.54 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 38 "/5V0-F") (pinfunction "5") (pintype "power_in"))
    (pad "5" smd circle (at -1.27 -2.54 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 38 "/5V0-F") (pinfunction "5") (pintype "power_in"))
    (pad "6" thru_hole circle (at 1.27 -2.54 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 60 "/USR18") (pinfunction "6") (pintype "passive"))
    (pad "6" smd circle (at 1.27 -2.54 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 60 "/USR18") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 61 "/G6_USR17") (pinfunction "7") (pintype "passive"))
    (pad "7" smd circle (at -1.27 0 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 61 "/G6_USR17") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 54 "/USR10") (pinfunction "8") (pintype "passive"))
    (pad "8" smd circle (at 1.27 0 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 54 "/USR10") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -1.27 2.54 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 64 "/RGB1") (pinfunction "9") (pintype "passive"))
    (pad "9" smd circle (at -1.27 2.54 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 64 "/RGB1") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at 1.27 2.54 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 55 "/USR11") (pinfunction "10") (pintype "passive"))
    (pad "10" smd circle (at 1.27 2.54 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 55 "/USR11") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at -1.27 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 62 "/G1_USR15") (pinfunction "11") (pintype "passive"))
    (pad "11" smd circle (at -1.27 5.08 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 62 "/G1_USR15") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at 1.27 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 56 "/USR12") (pinfunction "12") (pintype "passive"))
    (pad "12" smd circle (at 1.27 5.08 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 56 "/USR12") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at -1.27 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 58 "/USR14") (pinfunction "13") (pintype "passive"))
    (pad "13" smd circle (at -1.27 7.62 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 58 "/USR14") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at 1.27 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 57 "/G0_USR13") (pinfunction "14") (pintype "passive"))
    (pad "14" smd circle (at 1.27 7.62 90) (size 1.905 1.905) (layers "B.Cu" "B.Mask")
      (net 57 "/G0_USR13") (pinfunction "14") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x07_P2.54mm_Horizontal.step"
      (offset (xyz 1.27 7.62 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 43.815 48.26 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 44 "/USR26") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 20 "/AD2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 57.15 60.96)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R15" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 12 "/AC0") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 50 "/USR20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 57.15 48.26)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 3.81 0.027) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 33 "/G3-USR04") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 7 "/AC5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 57.15 53.34)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R12" (at 3.81 0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "/AC3") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 47 "/USR23") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 64.77 45.72 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "/AC6") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 32 "/USR03") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 43.815 58.42 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 36 "/USR07") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 24 "/AD6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 43.815 50.8 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 45 "/USR25") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 21 "/AD3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_DCW_Library:CON_1x20_hole40mil_pad60mil_pitch100mil" (layer "F.Cu")
    (at 68.58 52.07)
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x20, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J12" (at -2.286 -12.4968 90 unlocked) (layer "F.SilkS"))
    (fp_text value "1x20 100mil" (at 0 26.67 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -24.13) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 38 "/5V0-F") (pinfunction "Pin_1") (pintype "power_out"))
    (pad "1" smd oval (at 0 -24.13 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 38 "/5V0-F") (pinfunction "Pin_1") (pintype "power_out"))
    (pad "2" thru_hole circle (at 0 -21.59) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 39 "/SPI-CLK") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "2" smd oval (at 0 -21.59 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 39 "/SPI-CLK") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 0 -19.05) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 40 "/USR30") (pinfunction "Pin_3") (pintype "passive"))
    (pad "3" smd oval (at 0 -19.05 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 40 "/USR30") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 0 -16.51) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 41 "/RGB2") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "4" smd oval (at 0 -16.51 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 41 "/RGB2") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 0 -13.97) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 42 "/RGB0") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "5" smd oval (at 0 -13.97 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 42 "/RGB0") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 0 -11.43) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 43 "/USR27") (pinfunction "Pin_6") (pintype "passive"))
    (pad "6" smd oval (at 0 -11.43 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 43 "/USR27") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -8.89) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 44 "/USR26") (pinfunction "Pin_7") (pintype "passive"))
    (pad "7" smd oval (at 0 -8.89 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 44 "/USR26") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 45 "/USR25") (pinfunction "Pin_8") (pintype "passive"))
    (pad "8" smd oval (at 0 -6.35 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 45 "/USR25") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 46 "/USR24") (pinfunction "Pin_9") (pintype "passive"))
    (pad "9" smd oval (at 0 -3.81 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 46 "/USR24") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 47 "/USR23") (pinfunction "Pin_10") (pintype "passive"))
    (pad "10" smd oval (at 0 -1.27 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 47 "/USR23") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 51 "GND") (pinfunction "Pin_11") (pintype "power_in"))
    (pad "11" smd oval (at 0 1.27 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 51 "GND") (pinfunction "Pin_11") (pintype "power_in"))
    (pad "12" thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 48 "/USR22") (pinfunction "Pin_12") (pintype "passive"))
    (pad "12" smd oval (at 0 3.81 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 48 "/USR22") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 49 "/USR21") (pinfunction "Pin_13") (pintype "passive"))
    (pad "13" smd oval (at 0 6.35 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 49 "/USR21") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 0 8.89) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 50 "/USR20") (pinfunction "Pin_14") (pintype "passive"))
    (pad "14" smd oval (at 0 8.89 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 50 "/USR20") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 11.43) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 59 "/USR19") (pinfunction "Pin_15") (pintype "passive"))
    (pad "15" smd oval (at 0 11.43 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 59 "/USR19") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 0 13.97) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 60 "/USR18") (pinfunction "Pin_16") (pintype "passive"))
    (pad "16" smd oval (at 0 13.97 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 60 "/USR18") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 16.51) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 61 "/G6_USR17") (pinfunction "Pin_17") (pintype "passive"))
    (pad "17" smd oval (at 0 16.51 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 61 "/G6_USR17") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 0 19.05) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 64 "/RGB1") (pinfunction "Pin_18") (pintype "passive"))
    (pad "18" smd oval (at 0 19.05 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 64 "/RGB1") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 21.59) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 62 "/G1_USR15") (pinfunction "Pin_19") (pintype "passive"))
    (pad "19" smd oval (at 0 21.59 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 62 "/G1_USR15") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 0 24.13) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 63 "/NEO_OUT") (pinfunction "Pin_20") (pintype "passive+no_connect"))
    (pad "20" smd oval (at 0 24.13 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 63 "/NEO_OUT") (pinfunction "Pin_20") (pintype "passive+no_connect"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.step"
      (offset (xyz 0 24.13 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_DCW_Library:MountingHole_hole93mil_pad190mil" (layer "F.Cu")
    (at 74.168 27.94)
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Enable" "0")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H3" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 4.826 4.826) (drill 2.3622) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 43.815 43.18 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 43 "/USR27") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 18 "/AD0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "F.Cu")
    (at 50.419 28.48)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "DigiKey#" "")
    (property "JLCPCB-LCSC" "")
    (property "Manufacturer" "")
    (property "Mfr_Part#" "")
    (property "Mouser#" "")
    (property "Newark#" "")
    (property "Package" "")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "")
    (property "Value3" "")
    (property "ki_description" "3-pin header")
    (property "ki_keywords" "header")
    (attr through_hole)
    (fp_text reference "J4" (at -0.0508 6.1402) (layer "F.SilkS"))
    (fp_text value "1x3 header" (at 0 6.06) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "/5V0-F") (pinfunction "1") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "/VREGIN") (pinfunction "2") (pintype "power_out"))
    (pad "3" thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "/VBUS") (pinfunction "3") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_DCW_Library:CON_1x14_hole40mil_pad60mil_pitch100mil" (layer "F.Cu")
    (at 32.385 44.45)
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x14, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 2.4638 -4.445 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "1x14 100mil" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -16.51) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 13 "/SHLD") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "1" smd oval (at 0 -16.51 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 13 "/SHLD") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle (at 0 -13.97) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 14 "/VCCIO") (pinfunction "Pin_2") (pintype "power_in"))
    (pad "2" smd oval (at 0 -13.97 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 14 "/VCCIO") (pinfunction "Pin_2") (pintype "power_in"))
    (pad "3" thru_hole circle (at 0 -11.43) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 15 "/3V3-U") (pinfunction "Pin_3") (pintype "power_out"))
    (pad "3" smd oval (at 0 -11.43 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 15 "/3V3-U") (pinfunction "Pin_3") (pintype "power_out"))
    (pad "4" thru_hole circle (at 0 -8.89) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 16 "/PU2") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "4" smd oval (at 0 -8.89 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 16 "/PU2") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 17 "/PU1") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "5" smd oval (at 0 -6.35 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 17 "/PU1") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 51 "GND") (pinfunction "Pin_6") (pintype "power_in"))
    (pad "6" smd oval (at 0 -3.81 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 51 "GND") (pinfunction "Pin_6") (pintype "power_in"))
    (pad "7" thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 18 "/AD0") (pinfunction "Pin_7") (pintype "passive"))
    (pad "7" smd oval (at 0 -1.27 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 18 "/AD0") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 19 "/AD1") (pinfunction "Pin_8") (pintype "passive"))
    (pad "8" smd oval (at 0 1.27 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 19 "/AD1") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 20 "/AD2") (pinfunction "Pin_9") (pintype "passive"))
    (pad "9" smd oval (at 0 3.81 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 20 "/AD2") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 21 "/AD3") (pinfunction "Pin_10") (pintype "passive"))
    (pad "10" smd oval (at 0 6.35 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 21 "/AD3") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 8.89) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 22 "/AD4") (pinfunction "Pin_11") (pintype "passive"))
    (pad "11" smd oval (at 0 8.89 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 22 "/AD4") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 0 11.43) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 23 "/AD5") (pinfunction "Pin_12") (pintype "passive"))
    (pad "12" smd oval (at 0 11.43 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 23 "/AD5") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 13.97) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 24 "/AD6") (pinfunction "Pin_13") (pintype "passive"))
    (pad "13" smd oval (at 0 13.97 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 24 "/AD6") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 0 16.51) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 25 "/AD7") (pinfunction "Pin_14") (pintype "passive"))
    (pad "14" smd oval (at 0 16.51 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 25 "/AD7") (pinfunction "Pin_14") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x14_P2.54mm_Vertical.step"
      (offset (xyz 0 16.51 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_DCW_Library:MountingHole_hole93mil_pad190mil" (layer "F.Cu")
    (at 27.94 76.835)
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Enable" "0")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H2" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 4.826 4.826) (drill 2.3622) (layers "*.Cu" "*.Mask"))
  )
  (footprint "0_DCW_Library:MOD_EasyWEB-ShastaPlus" (layer "F.Cu")
    (at 60.96 44.45)
    (fp_text reference "REF**" (at 0 -27.94 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MOD_EasyWEB-ShastaPlus" (at 0 -22.86 unlocked) (layer "F.Fab") hide)
    (fp_text user "J12-20" (at 11.43 31.75 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "J12-1" (at 11.43 -16.74 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "USB" (at -0.235 -16.51 unlocked) (layer "Dwgs.User"))
    (fp_text user "J11-1" (at -11.43 -16.74 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "J11-20" (at -11.43 31.75 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "ShastaPlus" (at 0 3.81 90 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 -25.4 unlocked) (layer "F.Fab") hide)
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 43.815 55.88 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 35 "/USR06") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 23 "/AD5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical" (layer "F.Cu")
    (at 35.56 28.48)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (property "DigiKey#" "")
    (property "JLCPCB-LCSC" "")
    (property "Manufacturer" "")
    (property "Mfr_Part#" "")
    (property "Mouser#" "")
    (property "Newark#" "")
    (property "Package" "")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "")
    (property "Value3" "")
    (property "ki_description" "3-pin header")
    (property "ki_keywords" "header")
    (attr through_hole)
    (fp_text reference "J3" (at -0.127 6.159) (layer "F.SilkS"))
    (fp_text value "1x3 header" (at 0 6.06) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2 270 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "/3V3-F") (pinfunction "1") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "/VCCIO") (pinfunction "2") (pintype "power_out"))
    (pad "3" thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/3V3-U") (pinfunction "3") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 43.815 60.96 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 37 "/USR08") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 25 "/AD7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_DCW_Library:MountingHole_hole93mil_pad190mil" (layer "F.Cu")
    (at 27.94 27.94)
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Enable" "0")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H1" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 4.826 4.826) (drill 2.3622) (layers "*.Cu" "*.Mask"))
  )
  (footprint "0_DCW_Library:MountingHole_hole93mil_pad190mil" (layer "F.Cu")
    (at 74.168 76.835)
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Enable" "0")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H4" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 4.826 4.826) (drill 2.3622) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 57.15 58.42)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R14" (at 3.7592 0.0508) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "/AC1") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 49 "/USR21") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 57.15 55.88)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R13" (at 3.81 0.077) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "/AC2") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 48 "/USR22") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_DCW_Library:CON_1x20_hole40mil_pad60mil_pitch100mil" (layer "F.Cu")
    (at 53.34 52.07)
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x20, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J11" (at 2.3876 -12.5476 90 unlocked) (layer "F.SilkS"))
    (fp_text value "1x20 100mil" (at 0 26.67 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -24.13) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 26 "/3V3-F") (pinfunction "Pin_1") (pintype "power_out"))
    (pad "1" smd oval (at 0 -24.13 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 26 "/3V3-F") (pinfunction "Pin_1") (pintype "power_out"))
    (pad "2" thru_hole circle (at 0 -21.59) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 51 "GND") (pinfunction "Pin_2") (pintype "power_out"))
    (pad "2" smd oval (at 0 -21.59 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 51 "GND") (pinfunction "Pin_2") (pintype "power_out"))
    (pad "3" thru_hole circle (at 0 -19.05) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 27 "/SPI-MISO") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "3" smd oval (at 0 -19.05 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 27 "/SPI-MISO") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 -16.51) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 28 "/CDONE") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "4" smd oval (at 0 -16.51 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 28 "/CDONE") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 0 -13.97) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 29 "/CRESET") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "5" smd oval (at 0 -13.97 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 29 "/CRESET") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 0 -11.43) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 30 "/SPI-CS") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "6" smd oval (at 0 -11.43 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 30 "/SPI-CS") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle (at 0 -8.89) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 31 "/SPI-MOSI") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "7" smd oval (at 0 -8.89 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 31 "/SPI-MOSI") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 32 "/USR03") (pinfunction "Pin_8") (pintype "passive"))
    (pad "8" smd oval (at 0 -6.35 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 32 "/USR03") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 33 "/G3-USR04") (pinfunction "Pin_9") (pintype "passive"))
    (pad "9" smd oval (at 0 -3.81 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 33 "/G3-USR04") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 34 "/USR05") (pinfunction "Pin_10") (pintype "passive"))
    (pad "10" smd oval (at 0 -1.27 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 34 "/USR05") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 51 "GND") (pinfunction "Pin_11") (pintype "power_in"))
    (pad "11" smd oval (at 0 1.27 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 51 "GND") (pinfunction "Pin_11") (pintype "power_in"))
    (pad "12" thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 35 "/USR06") (pinfunction "Pin_12") (pintype "passive"))
    (pad "12" smd oval (at 0 3.81 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 35 "/USR06") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 36 "/USR07") (pinfunction "Pin_13") (pintype "passive"))
    (pad "13" smd oval (at 0 6.35 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 36 "/USR07") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 0 8.89) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 37 "/USR08") (pinfunction "Pin_14") (pintype "passive"))
    (pad "14" smd oval (at 0 8.89 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 37 "/USR08") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 11.43) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 53 "/USR09") (pinfunction "Pin_15") (pintype "passive"))
    (pad "15" smd oval (at 0 11.43 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 53 "/USR09") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 0 13.97) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 54 "/USR10") (pinfunction "Pin_16") (pintype "passive"))
    (pad "16" smd oval (at 0 13.97 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 54 "/USR10") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 16.51) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 55 "/USR11") (pinfunction "Pin_17") (pintype "passive"))
    (pad "17" smd oval (at 0 16.51 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 55 "/USR11") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 0 19.05) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 56 "/USR12") (pinfunction "Pin_18") (pintype "passive"))
    (pad "18" smd oval (at 0 19.05 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 56 "/USR12") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 21.59) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 57 "/G0_USR13") (pinfunction "Pin_19") (pintype "passive"))
    (pad "19" smd oval (at 0 21.59 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 57 "/G0_USR13") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 0 24.13) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 58 "/USR14") (pinfunction "Pin_20") (pintype "passive"))
    (pad "20" smd oval (at 0 24.13 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 58 "/USR14") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.step"
      (offset (xyz 0 24.13 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_DCW_Library:MOD_FTDI-UM232H" (layer "F.Cu")
    (at 40.005 44.4482)
    (fp_text reference "REF**" (at 0 19.05 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MOD_FTDI-UM232H" (at 0 21.59 unlocked) (layer "F.Fab") hide)
    (fp_text user "USB" (at -0.0762 -23.163 unlocked) (layer "Dwgs.User"))
    (fp_text user "J1-1" (at 10.16 -16.51 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "FT232H" (at 0 0 -90 unlocked) (layer "Dwgs.User"))
    (fp_text user "J2-1" (at -10.16 -16.51 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "J2-14" (at -10.16 16.51 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "J1-14" (at 10.16 16.51 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "${REFERENCE}" (at 0 20.32 unlocked) (layer "F.Fab") hide)
  )
  (footprint "0_DCW_Library:CON_1x14_hole40mil_pad60mil_pitch100mil" (layer "F.Cu")
    (at 47.625 44.45)
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x14, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -2.6162 -4.445 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "1x14 100mil" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 -16.51) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 51 "GND") (pinfunction "Pin_1") (pintype "power_in"))
    (pad "1" smd oval (at 0 -16.51 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 51 "GND") (pinfunction "Pin_1") (pintype "power_in"))
    (pad "2" thru_hole circle (at 0 -13.97) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 1 "/VREGIN") (pinfunction "Pin_2") (pintype "power_in"))
    (pad "2" smd oval (at 0 -13.97 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 1 "/VREGIN") (pinfunction "Pin_2") (pintype "power_in"))
    (pad "3" thru_hole circle (at 0 -11.43) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 52 "/VBUS") (pinfunction "Pin_3") (pintype "power_out"))
    (pad "3" smd oval (at 0 -11.43 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 52 "/VBUS") (pinfunction "Pin_3") (pintype "power_out"))
    (pad "4" thru_hole circle (at 0 -8.89) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "/RST#") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "4" smd oval (at 0 -8.89 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 2 "/RST#") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 3 "/AC9") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "5" smd oval (at 0 -6.35 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 3 "/AC9") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "/AC8") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "6" smd oval (at 0 -3.81 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 4 "/AC8") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 5 "/AC7") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "7" smd oval (at 0 -1.27 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 5 "/AC7") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 6 "/AC6") (pinfunction "Pin_8") (pintype "passive"))
    (pad "8" smd oval (at 0 1.27 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 6 "/AC6") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 7 "/AC5") (pinfunction "Pin_9") (pintype "passive"))
    (pad "9" smd oval (at 0 3.81 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 7 "/AC5") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 8 "/AC4") (pinfunction "Pin_10") (pintype "passive"))
    (pad "10" smd oval (at 0 6.35 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 8 "/AC4") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 8.89) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 9 "/AC3") (pinfunction "Pin_11") (pintype "passive"))
    (pad "11" smd oval (at 0 8.89 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 9 "/AC3") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 0 11.43) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 10 "/AC2") (pinfunction "Pin_12") (pintype "passive"))
    (pad "12" smd oval (at 0 11.43 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 10 "/AC2") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 13.97) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 11 "/AC1") (pinfunction "Pin_13") (pintype "passive"))
    (pad "13" smd oval (at 0 13.97 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 11 "/AC1") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 0 16.51) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 12 "/AC0") (pinfunction "Pin_14") (pintype "passive"))
    (pad "14" smd oval (at 0 16.51 90) (size 1.778 2.286) (layers "B.Cu" "B.Mask")
      (net 12 "/AC0") (pinfunction "Pin_14") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x14_P2.54mm_Vertical.step"
      (offset (xyz 0 16.51 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 57.15 50.8)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "UM232H-ShastaPlus-Adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R11" (at 3.81 0.027) (layer "F.SilkS"))
    (fp_text value "2k2" (at 3.81 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "/AC4") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 46 "/USR24") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 74.168 79.629) (end 27.94 79.629)
    (layer "Edge.Cuts"))
  (gr_line (start 76.962 27.94) (end 76.962 76.835)
    (layer "Edge.Cuts"))
  (gr_arc (start 27.94 79.629) (mid 25.964344 78.810656) (end 25.146 76.835)
    (layer "Edge.Cuts"))
  (gr_arc (start 76.962 76.835) (mid 76.143657 78.810657) (end 74.168 79.629)
    (layer "Edge.Cuts"))
  (gr_arc (start 25.146 27.94) (mid 25.964344 25.964344) (end 27.94 25.146)
    (layer "Edge.Cuts"))
  (gr_arc (start 74.168 25.146) (mid 76.143657 25.964343) (end 76.962 27.94)
    (layer "Edge.Cuts"))
  (gr_line (start 25.146 76.835) (end 25.146 27.94)
    (layer "Edge.Cuts"))
  (gr_line (start 27.94 25.146) (end 74.168 25.146)
    (layer "Edge.Cuts"))
  (gr_text "2" (at 30.4292 73.66) (layer "F.SilkS"))
  (gr_text "2025-Apr-13" (at 73.66 51.943 90) (layer "F.SilkS"))
  (gr_text "UM232H" (at 40.4876 35.052 -90) (layer "F.SilkS"))
  (gr_text "ShastaPlus" (at 63.1952 35.56 90) (layer "F.SilkS"))
  (gr_text "14" (at 45.339 61.976 -90) (layer "F.SilkS"))
  (gr_text "USB" (at 59.69 27.305) (layer "F.SilkS"))
  (gr_text "20" (at 66.5226 75.2094 90) (layer "F.SilkS"))
  (gr_text "13" (at 49.7332 76.1492) (layer "F.SilkS"))
  (gr_text "1" (at 66.294 27.432 90) (layer "F.SilkS"))
  (gr_text "FTDI" (at 43.6626 35.052 -90) (layer "F.SilkS"))
  (gr_text "1" (at 55.753 28.448 90) (layer "F.SilkS"))
  (gr_text "14" (at 34.544 59.944 -90) (layer "F.SilkS"))
  (gr_text "1" (at 45.339 28.448 -90) (layer "F.SilkS"))
  (gr_text "WebFPGA" (at 60.0202 36.195 90) (layer "F.SilkS"))
  (gr_text "David C Wiens" (at 27.94 51.943 -90) (layer "F.SilkS"))
  (gr_text "USB" (at 40.767 27.305) (layer "F.SilkS"))
  (gr_text "20" (at 55.5498 77.2414 90) (layer "F.SilkS"))
  (gr_text "Expansion" (at 34.8488 71.9836) (layer "F.SilkS"))
  (gr_text "1" (at 34.544 26.1112 -90) (layer "F.SilkS"))
  (gr_text "14" (at 49.7332 73.66) (layer "F.SilkS"))
  (zone (net 38) (net_name "/5V0-F") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 52.07 29.6418)
        (xy 52.2986 29.718)
        (xy 54.6354 29.718)
        (xy 54.6354 28.702)
        (xy 52.7304 28.702)
        (xy 51.993883 27.9711)
        (xy 51.61344 27.972049)
        (xy 51.2572 27.9908)
      )
    )
  )
  (zone (net 26) (net_name "/3V3-F") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 40.894 29.718)
        (xy 40.894 28.702)
        (xy 39.878 28.702)
      )
    )
  )
  (zone (net 51) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.2794))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2794) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 25.654 25.654)
        (xy 76.454 25.654)
        (xy 76.454 79.121)
        (xy 25.654 79.121)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 38.1 76.2)
        (xy 33.02 76.2)
        (xy 33.02 73.66)
        (xy 38.1 73.66)
      )
    )
  )
)
