(kicad_pcb (version 20171130) (host pcbnew 5.1.12-84ad8e8a86~92~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 496)
    (zones 0)
    (modules 36)
    (nets 18)
  )
  (page USLetter)
  (title_block
    (title "4 Channel Clock Distribution Board, V1")
    (date 2021-03-14)
    (rev -)
    (company "Amateur Radio / Phased Arrays")
    (comment 1 "Coherent RTL-SDR Projects")
    (comment 2 creativecommons.org/licenses/by/4.0/)
    (comment 3 "License: CC BY 4.0")
    (comment 4 "Author: Zach Leffke, KJ4QLP")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(F1-Pad2)")
  (net 4 "Net-(F2-Pad2)")
  (net 5 "Net-(F3-Pad2)")
  (net 6 "Net-(F4-Pad2)")
  (net 7 "Net-(F5-Pad1)")
  (net 8 "Net-(F5-Pad2)")
  (net 9 "Net-(R1-Pad2)")
  (net 10 /Y0)
  (net 11 /Y1)
  (net 12 /Y2)
  (net 13 /Y3)
  (net 14 +12V)
  (net 15 "Net-(C4-Pad1)")
  (net 16 "Net-(C5-Pad1)")
  (net 17 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net +12V)
    (add_net +3V3)
    (add_net /Y0)
    (add_net /Y1)
    (add_net /Y2)
    (add_net /Y3)
    (add_net GND)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad2)")
    (add_net "Net-(F3-Pad2)")
    (add_net "Net-(F4-Pad2)")
    (add_net "Net-(F5-Pad1)")
    (add_net "Net-(F5-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 133.35 78.74 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 1.905 0 180) (layer F.SilkS))
    (fp_text value VREG (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 16 "Net-(C5-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 141.605 92.71)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP7 (at 0 4.445) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 17 "Net-(R2-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 134.366 71.501 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 1.397 0 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1 1) (layers F.Cu F.Mask)
      (net 8 "Net-(F5-Pad2)"))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 133.35 83.185 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 1.905 0 180) (layer F.SilkS))
    (fp_text value SPX3819M5-L-3-3 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C5-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C4-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 +12V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 138.43 92.71)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP5 (at 0 4.445) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 135.255 92.71)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP6 (at 0 4.445) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 14 +12V))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 133.35 86.36)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.413 -0.508) (layer F.SilkS))
    (fp_text value 100k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 17 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 14 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 130.175 83.185 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 128.27 83.185 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 135.89 84.455 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -0.127 -1.524 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 129.54 87.63 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 1.143 1.397) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 133.35 88.265)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 149.225 92.075)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H4 (at 0 5.08) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 130.175 92.075)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H3 (at 0 5.08) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 136.779 70.866 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -0.762 1.524 90) (layer F.SilkS))
    (fp_text value CLKIN_FILT_BYPASS (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 8 "Net-(F5-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 7 "Net-(F5-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 129.54 74.295)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_GND1 (at -6.35 0) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 129.54 77.47)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_3v3 (at -5.715 0) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 1 +3V3))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 149.225 66.675)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.445) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 130.175 66.675)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.445) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 144.653 79.883)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 1.27 0 270) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 8.89 -1.27) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 6 "Net-(F4-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 144.653 84.963)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 1.27 0 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 5 "Net-(F3-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 144.653 74.803)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at 1.27 0 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 9.017 -1.27) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 4 "Net-(F2-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 144.653 69.723)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP0 (at 1.27 0 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 9.017 -0.508) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 3 "Net-(F1-Pad2)"))
  )
  (module Package_SO:TSSOP-8_4.4x3mm_P0.65mm (layer F.Cu) (tedit 5E476F32)
    (at 139.065 77.47 270)
    (descr "TSSOP, 8 Pin (JEDEC MO-153 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (attr smd)
    (fp_text reference U1 (at 1.27 -2.45 90) (layer F.SilkS))
    (fp_text value 5PB1104PGxx (at 0 2.45 90) (layer F.Fab))
    (fp_text user %R (at -1.143 0.762 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /Y1))
    (pad 7 smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /Y3))
    (pad 6 smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 5 smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /Y2))
    (pad 4 smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 3 smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Y0))
    (pad 2 smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(F5-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-8_4.4x3mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 135.89 75.565 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.397 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.254 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 9 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Molex_734120114_UMC_RF_CONN_Vertical (layer F.Cu) (tedit 5D2892B1)
    (at 139.065 66.675)
    (attr smd)
    (fp_text reference J4 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value CLKIN (at 0.2 3.175) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.125) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.5 0) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(F5-Pad1)"))
    (pad 1 smd rect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module digikey-footprints:Molex_734120114_UMC_RF_CONN_Vertical (layer F.Cu) (tedit 5D2892B1)
    (at 147.955 81.915 270)
    (attr smd)
    (fp_text reference J3 (at 0 -3.175 90) (layer F.SilkS))
    (fp_text value Y3 (at 0.2 3.175 90) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.125 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.5 0 270) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 1.5 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(F4-Pad2)"))
    (pad 1 smd rect (at 0 -1.5 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module digikey-footprints:Molex_734120114_UMC_RF_CONN_Vertical (layer F.Cu) (tedit 5D2892B1)
    (at 147.955 86.995 270)
    (attr smd)
    (fp_text reference J2 (at 0 -3.175 90) (layer F.SilkS))
    (fp_text value Y2 (at 0.2 3.175 90) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.125 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.5 0 270) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 1.5 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(F3-Pad2)"))
    (pad 1 smd rect (at 0 -1.5 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module digikey-footprints:Molex_734120114_UMC_RF_CONN_Vertical (layer F.Cu) (tedit 5D2892B1)
    (at 147.955 76.835 270)
    (attr smd)
    (fp_text reference J1 (at 0 -3.175 90) (layer F.SilkS))
    (fp_text value Y1 (at 0.2 3.175 90) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.125 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.5 0 270) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 1.5 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(F2-Pad2)"))
    (pad 1 smd rect (at 0 -1.5 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module digikey-footprints:Molex_734120114_UMC_RF_CONN_Vertical (layer F.Cu) (tedit 5D2892B1)
    (at 147.955 71.755 270)
    (attr smd)
    (fp_text reference J0 (at 0 -3.175 90) (layer F.SilkS))
    (fp_text value Y0 (at 0.2 3.175 90) (layer F.Fab))
    (fp_text user %R (at -0.05 -0.125 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.5 0 270) (size 1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 1.5 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(F1-Pad2)"))
    (pad 1 smd rect (at 0 -1.5 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module kj4qlp:0805_3PC_Pad (layer F.Cu) (tedit 604DA283)
    (at 143.51 81.915)
    (attr smd)
    (fp_text reference F4 (at -1.143 -1.524) (layer F.SilkS))
    (fp_text value MEM2012S35R0T001 (at 0 1.95) (layer F.Fab))
    (pad 3 smd rect (at 0 0) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd trapezoid (at -1.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /Y3))
    (pad 2 smd rect (at 1.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(F4-Pad2)"))
  )
  (module kj4qlp:0805_3PC_Pad (layer F.Cu) (tedit 604DA283)
    (at 143.51 86.995)
    (attr smd)
    (fp_text reference F3 (at -1.143 -1.524) (layer F.SilkS))
    (fp_text value MEM2012S35R0T001 (at 0 1.95) (layer F.Fab))
    (pad 3 smd rect (at 0 0) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd trapezoid (at -1.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /Y2))
    (pad 2 smd rect (at 1.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(F3-Pad2)"))
  )
  (module kj4qlp:0805_3PC_Pad (layer F.Cu) (tedit 604DA283)
    (at 139.065 70.866 270)
    (attr smd)
    (fp_text reference F5 (at -1.016 -1.524 90) (layer F.SilkS))
    (fp_text value MEM2012S35R0T001 (at 0 1.95 90) (layer F.Fab))
    (pad 3 smd rect (at 0 0 270) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd trapezoid (at -1.15 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(F5-Pad1)"))
    (pad 2 smd rect (at 1.15 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(F5-Pad2)"))
  )
  (module kj4qlp:0805_3PC_Pad (layer F.Cu) (tedit 604DA283)
    (at 143.51 76.835)
    (attr smd)
    (fp_text reference F2 (at -1.143 -1.524) (layer F.SilkS))
    (fp_text value MEM2012S35R0T001 (at 0 1.95) (layer F.Fab))
    (pad 3 smd rect (at 0 0) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd trapezoid (at -1.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /Y1))
    (pad 2 smd rect (at 1.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(F2-Pad2)"))
  )
  (module kj4qlp:0805_3PC_Pad (layer F.Cu) (tedit 604DA283)
    (at 143.51 71.755)
    (attr smd)
    (fp_text reference F1 (at -1.143 -1.524) (layer F.SilkS))
    (fp_text value MEM2012S35R0T001 (at 0 1.95) (layer F.Fab))
    (pad 3 smd rect (at 0 0) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd trapezoid (at -1.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /Y0))
    (pad 2 smd rect (at 1.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(F1-Pad2)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 135.89 79.375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "#2" (at 128.27 88.9 90) (layer B.SilkS))
  (gr_text "#2" (at 128.27 69.85 90) (layer B.SilkS))
  (gr_text "#2" (at 151.13 69.85 90) (layer B.SilkS))
  (gr_text "#2" (at 151.13 88.9 90) (layer B.SilkS))
  (dimension 25.4 (width 0.15) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 118.08 79.375 270) (layer Dwgs.User))
    (feature1 (pts (xy 130.175 92.075) (xy 118.793579 92.075)))
    (feature2 (pts (xy 130.175 66.675) (xy 118.793579 66.675)))
    (crossbar (pts (xy 119.38 66.675) (xy 119.38 92.075)))
    (arrow1a (pts (xy 119.38 92.075) (xy 118.793579 90.948496)))
    (arrow1b (pts (xy 119.38 92.075) (xy 119.966421 90.948496)))
    (arrow2a (pts (xy 119.38 66.675) (xy 118.793579 67.801504)))
    (arrow2b (pts (xy 119.38 66.675) (xy 119.966421 67.801504)))
  )
  (gr_text SN: (at 149.225 74.295 90) (layer B.SilkS))
  (gr_text "CLK\nIN" (at 136.525 66.675) (layer F.SilkS))
  (gr_text "4 Channel Clock Distribution Board\nVersion 2, Revision -\n\nCoherent RTL-SDR Project\nZ. Leffke, VT-NSI, 20220209" (at 139.7 79.375 90) (layer B.SilkS))
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "0.7500 in" (at 139.7 55.596) (layer Dwgs.User))
    (feature1 (pts (xy 149.225 66.675) (xy 149.225 56.309579)))
    (feature2 (pts (xy 130.175 66.675) (xy 130.175 56.309579)))
    (crossbar (pts (xy 130.175 56.896) (xy 149.225 56.896)))
    (arrow1a (pts (xy 149.225 56.896) (xy 148.098496 57.482421)))
    (arrow1b (pts (xy 149.225 56.896) (xy 148.098496 56.309579)))
    (arrow2a (pts (xy 130.175 56.896) (xy 131.301504 57.482421)))
    (arrow2b (pts (xy 130.175 56.896) (xy 131.301504 56.309579)))
  )
  (gr_text ~DIS (at 141.605 90.805) (layer F.SilkS))
  (gr_text GND (at 131.445 74.295 -90) (layer F.SilkS))
  (gr_text +3V3 (at 131.445 77.47 270) (layer F.SilkS))
  (gr_text GND (at 138.43 90.805) (layer F.SilkS))
  (gr_text +12V (at 135.255 90.805) (layer F.SilkS))
  (gr_line (start 127 95.25) (end 127 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 95.25) (end 127 95.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 63.5) (end 152.4 95.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 63.5) (end 152.4 63.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 148.717 77.47) (xy 147.193 77.47) (xy 147.193 76.2) (xy 148.717 76.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 148.717 72.39) (xy 147.193 72.39) (xy 147.193 71.12) (xy 148.717 71.12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 148.717 82.55) (xy 147.193 82.55) (xy 147.193 81.28) (xy 148.717 81.28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 148.717 87.63) (xy 147.193 87.63) (xy 147.193 86.36) (xy 148.717 86.36)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 152.4 95.25) (xy 127 95.25) (xy 127 63.5) (xy 152.4 63.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 152.4 95.25) (xy 127 95.25) (xy 127 63.5) (xy 152.4 63.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 139.7 67.31) (xy 138.43 67.31) (xy 138.43 66.04) (xy 139.7 66.04)
      )
    )
  )
)
