(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 175)
    (zones 0)
    (modules 20)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.762)
    (user_trace_width 2.794)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /Shoe/Q_3V3)
  (net 2 /Shoe/Q_MAG~RST)
  (net 3 /Shoe/SDA)
  (net 4 /Shoe/SCL)
  (net 5 /Shoe/Q_TX_SDA)
  (net 6 /Shoe/Q_RX_SDA)
  (net 7 /Shoe/Q_TX_SCL)
  (net 8 /Shoe/Q_RX_SCL)
  (net 9 /Shoe/Q_INT)
  (net 10 /Shoe/Q_GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /Shoe/Q_3V3)
    (add_net /Shoe/Q_GND)
    (add_net /Shoe/Q_INT)
    (add_net /Shoe/Q_MAG~RST)
    (add_net /Shoe/Q_RX_SCL)
    (add_net /Shoe/Q_RX_SDA)
    (add_net /Shoe/Q_TX_SCL)
    (add_net /Shoe/Q_TX_SDA)
    (add_net /Shoe/SCL)
    (add_net /Shoe/SDA)
  )
  (net_class RF ""
    (clearance 0.254)
    (trace_width 2.794)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module KwanSystems:StKwansSoldermask (layer B.Cu) (tedit 5F40003C)
    (at 80.518 60.198 180)
    (fp_text reference G502 (at -3.683 2.7432) (layer B.Mask) hide)
    (fp_text value KwanSystems (at 4.2926 -3.7084) (layer B.Mask) hide)
    (fp_text user github.com/kwan3217/kicad (at 2.286 -5.842 unlocked) (layer B.SilkS))
    (fp_text user stkwans.blogspot.com (at -2.794 -2.54 unlocked) (layer B.SilkS))
    (fp_text user "a division of Kwan Systems" (at 1.524 11.176 180 unlocked) (layer B.SilkS) hide)
    (fp_text user "St Kwan's Home for" (at -3.81 2.286 unlocked) (layer B.SilkS))
    (fp_text user "the Terminally ADD" (at -4.318 1.016 unlocked) (layer B.SilkS))
  )
  (module KwanSystems:SolderJumper-2_Bridged (layer F.Cu) (tedit 5F4584FB)
    (at 88.9 66.294 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference J1207 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 4 /Shoe/SCL))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 7 /Shoe/Q_TX_SCL))
  )
  (module KwanSystems:SolderJumper-2_Bridged (layer F.Cu) (tedit 5F4584FB)
    (at 86.868 66.294 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference J1202 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 3 /Shoe/SDA))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 6 /Shoe/Q_RX_SDA))
  )
  (module Package_SO:TSSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5F458241)
    (at 87.884 66.294 270)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1202 (at 0 -2.55 270) (layer F.SilkS) hide)
    (fp_text value P82B96 (at 0 2.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 8 smd rect (at 2.15 -0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3))
    (pad 7 smd rect (at 2.15 -0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /Shoe/SCL))
    (pad 6 smd rect (at 2.15 0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /Shoe/Q_RX_SCL))
    (pad 5 smd rect (at 2.15 0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /Shoe/Q_TX_SCL))
    (pad 4 smd rect (at -2.15 0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND))
    (pad 3 smd rect (at -2.15 0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /Shoe/Q_TX_SDA))
    (pad 2 smd rect (at -2.15 -0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /Shoe/Q_RX_SDA))
    (pad 1 smd rect (at -2.15 -0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /Shoe/SDA))
  )
  (module KwanSystems:Axis (layer F.Cu) (tedit 590A7BBF)
    (at 94.996 77.216 90)
    (descr "Built for the MPU-9250 using guidelines found in http://cds.linear.com/docs/en/packaging/Carsem%20MLP%20users%20guide.pdf")
    (fp_text reference G904 (at -1.3 1.5 90) (layer F.Fab) hide)
    (fp_text value Axis (at -1.8 2.75 90) (layer F.SilkS) hide)
    (fp_text user Z (at 3.302 -3.302 180) (layer B.SilkS))
    (fp_text user Y (at 0 -3.302 180) (layer B.SilkS))
    (fp_text user X (at 3.2 0 180) (layer B.SilkS))
    (fp_text user Z (at 3.302 -3.302 180) (layer F.SilkS))
    (fp_text user X (at 3.2 0 180) (layer F.SilkS))
    (fp_text user Y (at 0 -3.302 180) (layer F.SilkS))
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 86.36 59.182)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference G503 (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW (at 0.75 0) (layer F.Fab) hide)
  )
  (module KwanSystems:Symbol_KiCAD-Logo_CopperAndSilkScreenTop_small (layer F.Cu) (tedit 0)
    (at 92.202 58.166)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference G501 (at 0 0) (layer F.SilkS) hide)
    (fp_text value DesignedWithKicad (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 90.424 67.818 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1207 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /Shoe/SCL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoe/Q_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 90.424 64.77 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1201 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /Shoe/SDA))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoe/Q_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 95.25 69.85 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Shoe/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoe/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 95.25 70.866 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1505 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Shoe/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoe/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.678 70.866 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1408 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoe/Q_3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Shoe/Q_GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 86.614 70.866 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1406 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Shoe/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoe/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 95.25 66.548 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1308 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Shoe/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoe/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 95.25 67.564 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1305 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Shoe/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoe/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Harwin:Harwin_M20-89009xx_1x09_P2.54mm_Horizontal (layer F.Cu) (tedit 5F3DBDB7)
    (at 76.2 67.31 180)
    (descr "Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89009xx, 9 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator")
    (tags "connector Harwin M20-890 horizontal")
    (attr smd)
    (fp_text reference J1201 (at -0.48 -12.63) (layer F.SilkS) hide)
    (fp_text value Conn_01x09_Male (at -0.48 12.63) (layer F.Fab))
    (pad 9 smd rect (at -5.525 10.16 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND))
    (pad 8 smd rect (at -5.525 7.62 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoe/Q_MAG~RST))
    (pad 7 smd rect (at -5.525 5.08 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /Shoe/Q_TX_SDA))
    (pad 6 smd rect (at -5.525 2.54 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /Shoe/Q_RX_SDA))
    (pad 5 smd rect (at -5.525 0 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /Shoe/Q_TX_SCL))
    (pad 4 smd rect (at -5.525 -2.54 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /Shoe/Q_RX_SCL))
    (pad 3 smd rect (at -5.525 -5.08 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /Shoe/Q_INT))
    (pad 2 smd rect (at -5.525 -7.62 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3))
    (pad 1 smd rect (at -5.525 -10.16 180) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND))
    (model ${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_M20-89009xx_1x09_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:BME280 (layer F.Cu) (tedit 5F3D9117)
    (at 88.646 70.866 90)
    (fp_text reference U1401 (at -3.556 -0.762 90) (layer F.Fab))
    (fp_text value BME280 (at 0.012 0.775 90) (layer F.Fab) hide)
    (pad 6 smd rect (at -1.025 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3))
    (pad 7 smd rect (at -1.025 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND))
    (pad 5 smd rect (at -1.025 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND))
    (pad 4 smd rect (at 1.025 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 /Shoe/SCL))
    (pad 1 smd rect (at 1.025 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND))
    (pad 3 smd rect (at 1.025 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 /Shoe/SDA))
    (pad 8 smd rect (at -1.025 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3))
    (pad 2 smd rect (at 1.025 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3))
    (model /home/jeppesen/workspace/kicad/KwanSystems.pretty/BME280--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module KwanSystems:LGA-14L (layer F.Cu) (tedit 5F3D6253)
    (at 92.964 67.31 90)
    (fp_text reference U1501 (at 3.048 0.405 270) (layer F.Fab))
    (fp_text value LSM6DSO (at 4.826 -0.762 90) (layer F.Fab) hide)
    (fp_text user >Name (at -2 -1.5 90) (layer F.Fab) hide)
    (fp_text user >Value (at -2 2.5 90) (layer F.Fab) hide)
    (fp_text user Z (at -0.45 0.25 90) (layer Dwgs.User))
    (fp_text user X (at 0.35 0.25 90) (layer Dwgs.User))
    (fp_text user Y (at -0.4 -0.5 90) (layer Dwgs.User))
    (pad 1 smd rect (at -1.1625 -0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.1625 -0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -1.1625 0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -1.1625 0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at 0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 1.1625 0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 1.1625 0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 1.1625 -0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 1.1625 -0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 0 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Shoe/SCL) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /Shoe/SDA) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:LGA-14L (layer F.Cu) (tedit 5F3D6253)
    (at 92.964 70.612 90)
    (fp_text reference U1301 (at 3.048 0.405 270) (layer F.Fab))
    (fp_text value LSM6DSO (at 4.826 -0.762 90) (layer F.Fab) hide)
    (fp_text user >Name (at -2 -1.5 90) (layer F.Fab) hide)
    (fp_text user >Value (at -2 2.5 90) (layer F.Fab) hide)
    (fp_text user Z (at -0.45 0.25 90) (layer Dwgs.User))
    (fp_text user X (at 0.35 0.25 90) (layer Dwgs.User))
    (fp_text user Y (at -0.4 -0.5 90) (layer Dwgs.User))
    (pad 1 smd rect (at -1.1625 -0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.1625 -0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -1.1625 0.25 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -1.1625 0.75 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /Shoe/Q_INT) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at 0.5 0.9125 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 1.1625 0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 1.1625 0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 1.1625 -0.25 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 1.1625 -0.75 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 0 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Shoe/SCL) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -0.5 -0.9125) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /Shoe/SDA) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:AK09970 (layer F.Cu) (tedit 5F3D3F3B)
    (at 92.964 63.5 90)
    (fp_text reference U1201 (at 0 0.3 90) (layer Dwgs.User))
    (fp_text value AK09970 (at 0.2 -0.3 90) (layer Dwgs.User))
    (fp_text user Z (at -0.6 0.7 90) (layer Dwgs.User))
    (fp_text user Y (at -0.7 -0.9 90) (layer Dwgs.User))
    (fp_text user X (at 0.8 0.7 90) (layer Dwgs.User))
    (pad 16 smd rect (at -1.5375 0.75) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoe/Q_MAG~RST))
    (pad 15 smd rect (at -1.5375 0.25) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3))
    (pad 14 smd rect (at -1.5375 -0.25) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -1.5375 -0.75) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND))
    (pad 12 smd rect (at -0.75 -1.5375 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoe/Q_GND))
    (pad 11 smd rect (at -0.25 -1.5375 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 0.25 -1.5375 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 0.75 -1.5375 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 1.5375 -0.75 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.5375 -0.25 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.5375 0.25 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.5375 0.75 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 3 /Shoe/SDA))
    (pad 4 smd rect (at 0.75 1.5375 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.25 1.5375 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 4 /Shoe/SCL))
    (pad 2 smd rect (at -0.25 1.5375 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 /Shoe/Q_3V3))
    (pad 1 smd rect (at -0.75 1.5375 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text ID (at 80.01 57.15) (layer F.SilkS))
  (gr_text M~RST (at 80.01 59.69) (layer F.SilkS))
  (gr_text TSDA (at 80.01 62.23) (layer F.SilkS))
  (gr_text RSDA (at 80.01 64.77) (layer F.SilkS))
  (gr_text TSCL (at 80.01 67.31) (layer F.SilkS))
  (gr_text RSCL (at 80.01 69.85) (layer F.SilkS))
  (gr_text INT (at 80.01 72.39) (layer F.SilkS))
  (gr_text 3V3 (at 80.01 74.93) (layer F.SilkS))
  (gr_text GND (at 80.01 77.47) (layer F.SilkS))
  (gr_text "Wearable Pocketometer\nShoe Board\nv1.0\n2020 Sep 01" (at 77.216 74.93) (layer B.SilkS))
  (gr_text "a division of\nKwan Systems" (at 95.758 60.96) (layer B.SilkS))
  (gr_line (start 96.52 58.42) (end 96.52 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.98 78.74) (end 78.74 78.74) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 78.74 76.2) (end 76.2 76.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 78.74 58.42) (end 78.74 55.88) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 93.98 58.42) (end 96.52 58.42) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 93.98 76.2) (end 93.98 78.74) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.2 58.42) (end 76.2 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.98 55.88) (end 78.74 55.88) (layer Edge.Cuts) (width 0.05))
  (zone (net 10) (net_name /Shoe/Q_GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.47 55.88) (xy 96.52 55.88) (xy 96.52 78.74) (xy 76.2 78.74) (xy 76.2 55.88)
      )
    )
  )
  (zone (net 10) (net_name /Shoe/Q_GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.09 55.88) (xy 96.52 55.88) (xy 96.52 78.74) (xy 76.2 78.74) (xy 76.2 64.77)
        (xy 85.09 64.77)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.582 64.262) (xy 76.2 64.262) (xy 76.2 55.88) (xy 84.582 55.88)
      )
    )
  )
)
