(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 41)
    (no_connects 0)
    (area 123.224999 118.424999 173.175001 136.175001)
    (thickness 1.6)
    (drawings 7)
    (tracks 200)
    (zones 0)
    (modules 18)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.3)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.9)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.5)
    (user_via 2.2 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 GND)
  (net 3 +12V)
  (net 4 /Temp)
  (net 5 "Net-(J4-Pad1)")
  (net 6 "Net-(J4-Pad17)")
  (net 7 "Net-(J4-Pad2)")
  (net 8 "Net-(J4-Pad18)")
  (net 9 "Net-(J4-Pad3)")
  (net 10 "Net-(J4-Pad20)")
  (net 11 "Net-(J4-Pad5)")
  (net 12 "Net-(J4-Pad21)")
  (net 13 "Net-(J4-Pad22)")
  (net 14 "Net-(J4-Pad23)")
  (net 15 "Net-(J4-Pad8)")
  (net 16 "Net-(J4-Pad24)")
  (net 17 /Heat)
  (net 18 "Net-(J4-Pad25)")
  (net 19 "Net-(J4-Pad10)")
  (net 20 "Net-(J4-Pad26)")
  (net 21 "Net-(J4-Pad11)")
  (net 22 VCC)
  (net 23 "Net-(J4-Pad12)")
  (net 24 "Net-(J4-Pad28)")
  (net 25 "Net-(J4-Pad13)")
  (net 26 "Net-(J4-Pad14)")
  (net 27 "Net-(J4-Pad16)")
  (net 28 "Net-(Q1-Pad1)")
  (net 29 "Net-(Q2-Pad1)")
  (net 30 "Net-(Q2-Pad3)")
  (net 31 "Net-(C2-Pad1)")
  (net 32 "Net-(C3-Pad1)")
  (net 33 "Net-(C1-Pad1)")
  (net 34 "Net-(HEAT1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.4)
    (via_dia 0.9)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Heat)
    (add_net /Temp)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(HEAT1-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad11)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad13)")
    (add_net "Net-(J4-Pad14)")
    (add_net "Net-(J4-Pad16)")
    (add_net "Net-(J4-Pad17)")
    (add_net "Net-(J4-Pad18)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad20)")
    (add_net "Net-(J4-Pad21)")
    (add_net "Net-(J4-Pad22)")
    (add_net "Net-(J4-Pad23)")
    (add_net "Net-(J4-Pad24)")
    (add_net "Net-(J4-Pad25)")
    (add_net "Net-(J4-Pad26)")
    (add_net "Net-(J4-Pad28)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad3)")
    (add_net VCC)
  )
  (net_class 12V ""
    (clearance 0.3)
    (trace_width 1.8)
    (via_dia 1.5)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
  )
  (net_class Thin ""
    (clearance 0.26)
    (trace_width 0.3)
    (via_dia 0.7)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
  )
  (module KiCadCustomLibs:DFN-8-1EP_6x5mm (layer F.Cu) (tedit 5A21536F)
    (at 162.1 127.4)
    (descr "DD Package; 8-Lead Plastic DFN (6mm x 5mm) (see http://www.everspin.com/file/236/download)")
    (tags "dfn ")
    (attr smd)
    (fp_text reference Q1 (at 0.2 3.6) (layer F.SilkS))
    (fp_text value AON6403 (at 0 3.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.46 0 270) (size 4.6 4.12) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(HEAT1-Pad1)") (solder_mask_margin 0.1) (solder_paste_margin -0.15) (clearance 0.1))
    (pad 3 smd rect (at -2.9 -1.905 270) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V) (solder_mask_margin 0.1) (clearance 0.1))
    (pad 3 smd rect (at -2.9 -0.635 270) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V) (solder_mask_margin 0.1) (clearance 0.1))
    (pad 3 smd rect (at -2.9 0.635 270) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V) (solder_mask_margin 0.1) (clearance 0.1))
    (pad 1 smd rect (at -2.9 1.905 270) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q1-Pad1)") (solder_mask_margin 0.1) (clearance 0.1))
    (pad 2 smd rect (at 2.9 1.905 270) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(HEAT1-Pad1)") (solder_mask_margin 0.1) (clearance 0.1))
    (pad 2 smd rect (at 2.9 0.635 270) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(HEAT1-Pad1)") (solder_mask_margin 0.1) (clearance 0.1))
    (pad 2 smd rect (at 2.9 -0.635 270) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(HEAT1-Pad1)") (solder_mask_margin 0.1) (clearance 0.1))
    (pad 2 smd rect (at 2.9 -1.905 270) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(HEAT1-Pad1)") (solder_mask_margin 0.1) (clearance 0.1))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-8-1EP_6x5mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A214CD4)
    (at 124.6 119.8)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference 12V (at 0.5 2.3) (layer B.SilkS))
    (fp_text value PWR (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module ROTARY-ENCODER (layer F.Cu) (tedit 5A2129B8)
    (at 130.8 127.4)
    (fp_text reference SW1 (at 0 1.7) (layer F.SilkS))
    (fp_text value Rotary_Encoder (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 7.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(C2-Pad1)"))
    (pad 3 thru_hole circle (at 2.5 7.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 0 7.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at -2.5 -7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole circle (at 2.5 -7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(C1-Pad1)"))
    (pad "" thru_hole circle (at 5.6 0) (size 3 3) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -5.6 0) (size 3 3) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (model AB2_ROT_ENC_W_SW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.015 0.015 0.015))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SOD-123F (layer F.Cu) (tedit 5A215310)
    (at 162.6 123.2 180)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at -0.03 1.57 180) (layer F.SilkS))
    (fp_text value D (at 0 2.1 180) (layer F.Fab) hide)
    (fp_text user %R (at -0.127 -1.905 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Modules:Arduino_Nano (layer B.Cu) (tedit 5A201141)
    (at 171.79 134.99 90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference J4 (at 7.62 5.08 90) (layer B.SilkS) hide)
    (fp_text value Arduino_Nano_Header (at 8.89 -19.05 360) (layer B.Fab))
    (fp_text user %R (at 6.35 -19.05 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J4-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 -33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad17)"))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (pad 18 thru_hole oval (at 15.24 -30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad18)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad3)"))
    (pad 19 thru_hole oval (at 15.24 -27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /Temp))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole oval (at 15.24 -25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad20)"))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad5)"))
    (pad 21 thru_hole oval (at 15.24 -22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad21)"))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C2-Pad1)"))
    (pad 22 thru_hole oval (at 15.24 -20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad22)"))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C3-Pad1)"))
    (pad 23 thru_hole oval (at 15.24 -17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad23)"))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad8)"))
    (pad 24 thru_hole oval (at 15.24 -15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad24)"))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /Heat))
    (pad 25 thru_hole oval (at 15.24 -12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad25)"))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad10)"))
    (pad 26 thru_hole oval (at 15.24 -10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J4-Pad26)"))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J4-Pad11)"))
    (pad 27 thru_hole oval (at 15.24 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 VCC))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J4-Pad12)"))
    (pad 28 thru_hole oval (at 15.24 -5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad28)"))
    (pad 13 thru_hole oval (at 0 -30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad13)"))
    (pad 29 thru_hole oval (at 15.24 -2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 0 -33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J4-Pad14)"))
    (pad 30 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 15 thru_hole oval (at 0 -35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (pad 16 thru_hole oval (at 15.24 -35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J4-Pad16)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5A215327)
    (at 141.2 124.3)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference LCD (at 0 -2.33) (layer F.SilkS))
    (fp_text value LCD (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad23)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad24)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A2152E9)
    (at 152.24 127.24)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -0.01 2.41) (layer F.SilkS))
    (fp_text value SI2308 (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A21558F)
    (at 155.62 126.19)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.91 -0.05) (layer F.SilkS))
    (fp_text value 100K (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A2152F3)
    (at 155.64 128.33 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.01 -1.4 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A215574)
    (at 149.36 128.44 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.81 0.14 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A215299)
    (at 145.74 128.46 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.1 1.52 360) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /Temp))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A21556F)
    (at 147.54 128.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.76 -0.07 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /Heat))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A202830)
    (at 171.27 122.94)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference TEMP (at -2.53 1.21 90) (layer F.SilkS))
    (fp_text value "Temp sensor" (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Temp))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A215341)
    (at 138.35 124.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.95 -0.04 180) (layer F.SilkS))
    (fp_text value 22n (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A215368)
    (at 154.45 132.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.3 0 180) (layer F.SilkS))
    (fp_text value 22n (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A21534A)
    (at 138.15 132.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2 -0.1 180) (layer F.SilkS))
    (fp_text value 22n (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A214C96)
    (at 124.6 134.8)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference GND (at 0.4 -2.4) (layer B.SilkS))
    (fp_text value PWR (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A214F2C)
    (at 171.3 131.8 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference HEAT (at 2.5 1.4 270) (layer F.SilkS))
    (fp_text value Heater (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(HEAT1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_text V1.0 (at 145.93 132.86) (layer F.SilkS))
  (gr_text nppc (at 145.87 124.45) (layer F.SilkS))
  (gr_text Reflow (at 149.66 122.6) (layer F.SilkS))
  (gr_line (start 173.1 118.5) (end 123.3 118.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.3 136.1) (end 173.1 136.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.1 136.1) (end 173.1 118.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.3 118.5) (end 123.3 136.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 173.4 136.6) (xy 121.9 136.6) (xy 121.8 118.2) (xy 173.4 118.1)
      )
    )
    (polygon
      (pts        (xy 159 131.01) (xy 159 131.18) (xy 159.000767 131.01)
      )
    )
    (polygon
      (pts        (xy 159.03 124.53) (xy 159.000767 131.01) (xy 166.67 131.01) (xy 166.67 124.53)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 121.6 117.9) (xy 121.7 136.7) (xy 173.6 136.7) (xy 173.2 117.8)
      )
    )
  )
  (zone (net 34) (net_name "Net-(HEAT1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 159.6 125) (xy 166.1 125) (xy 166.1 130.6) (xy 159.6 130.6) (xy 159.6 130.4)
      )
    )
  )
)
