(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 15)
    (no_connects 0)
    (area 142.84181 97.915666 162.330526 118.677)
    (thickness 1.6)
    (drawings 36)
    (tracks 21)
    (zones 0)
    (modules 10)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.16)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(P1-Pad2)")
  (net 5 "Net-(C1-Pad1)")
  (net 6 "Net-(C2-Pad2)")
  (net 7 "Net-(U1-Pad1)")
  (net 8 VCC)
  (net 9 "Net-(R1-Pad1)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net VCC)
  )
  (module multimeter:std_wirepads (layer F.Cu) (tedit 59838648)
    (at 154.686 114.046)
    (fp_text reference D1 (at 1.27 3.175) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.905) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at 2.286 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
  )
  (module multimeter:std_2wirepads_close (layer F.Cu) (tedit 5983842B)
    (at 152.146 114.046 180)
    (fp_text reference SW1 (at 4.318 -3.556 180) (layer F.SilkS) hide)
    (fp_text value SW_DIP_x01 (at 0.635 -1.905 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 2.286 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 VCC))
  )
  (module multimeter:std_cap (layer F.Cu) (tedit 59838763)
    (at 159.766 105.029 90)
    (fp_text reference C1 (at 2.159 0.508 90) (layer F.SilkS))
    (fp_text value 47uF (at 5.08 -3.175 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module multimeter:std_cap (layer F.Cu) (tedit 59838766)
    (at 159.766 111.125 90)
    (fp_text reference C2 (at 1.905 0.508 90) (layer F.SilkS))
    (fp_text value 47uF (at 5.08 -3.175 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
  )
  (module multimeter:std_2wirepads_close (layer F.Cu) (tedit 59838744)
    (at 147.32 102.87 90)
    (fp_text reference P1 (at 0.254 -3.302 180) (layer F.SilkS) hide)
    (fp_text value AUDIO_IN (at 0.635 -1.905 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.905 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad2)"))
  )
  (module multimeter:std_2wirepads_close (layer F.Cu) (tedit 5980DC14)
    (at 147.32 109.855 270)
    (fp_text reference P2 (at 0.635 1.905 270) (layer F.SilkS) hide)
    (fp_text value POWER (at 0.635 -1.905 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.905 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 VCC))
  )
  (module multimeter:std_2wirepads_close (layer F.Cu) (tedit 5983874E)
    (at 147.32 105.41 270)
    (fp_text reference P3 (at 0.635 1.905 270) (layer F.SilkS) hide)
    (fp_text value AUDIO_OUT (at 0.635 -1.905 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 1.905 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module multimeter:std_resistor (layer F.Cu) (tedit 598387B1)
    (at 149.86 111.76)
    (fp_text reference R1 (at 3.81 0) (layer F.SilkS))
    (fp_text value R_LED (at 3.81 -1.905) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 598387A0)
    (at 149.86 101.6)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value LM386 (at 3.81 10.01) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Desktop:logo (layer F.Cu) (tedit 0)
    (at 153.797 102.108)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "Smokey\nAmp" (at 153.67 110.871) (layer B.SilkS))
  (gr_text V1 (at 159.893 114.427) (layer F.SilkS))
  (gr_line (start 161.036 99.949) (end 161.036 115.316) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 99.949) (end 161.036 99.949) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 115.316) (end 146.05 99.949) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text + (at 159.004 109.474) (layer F.SilkS))
  (gr_text + (at 159.004 103.378) (layer F.SilkS))
  (gr_text POWER (at 153.797 107.95) (layer B.SilkS))
  (gr_text A-OUT (at 154.051 105.41) (layer B.SilkS))
  (gr_text A-IN (at 154.686 102.87) (layer B.SilkS))
  (gr_text SW (at 147.574 114.046) (layer B.SilkS))
  (gr_text LED (at 159.258 114.046) (layer B.SilkS))
  (gr_line (start 161.036 115.316) (end 146.05 115.316) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.036 115.316) (xy 146.05 115.316) (xy 146.05 99.949) (xy 161.036 99.949)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.036 115.316) (xy 146.05 115.316) (xy 146.05 99.949) (xy 161.036 99.949)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.463 103.886) (xy 146.05 103.886) (xy 146.05 99.949) (xy 148.463 99.949)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.463 108.331) (xy 146.05 108.331) (xy 146.05 104.394) (xy 148.463 104.394)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.463 112.776) (xy 146.05 112.776) (xy 146.05 108.839) (xy 148.463 108.839)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.861 115.316) (xy 153.67 115.316) (xy 153.67 113.03) (xy 157.861 113.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.162 115.316) (xy 148.844 115.316) (xy 148.844 113.03) (xy 153.162 113.03)
      )
    )
  )
)
