(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "SolarPanel+")
  (net 4 "Net-(J1-Pin_1)")
  (net 5 "Net-(J1-Pin_2)")
  (net 6 "Net-(J1-Pin_3)")
  (net 7 "GND1")
  (net 8 "Net-(Q1-G)")
  (net 9 "Net-(U1-PB0)")
  (net 10 "Net-(U1-PB1)")
  (net 11 "Net-(U1-PB2)")
  (net 12 "Net-(U2-MOSI)")
  (net 13 "Net-(R10-Pad1)")
  (net 14 "Net-(U3-+)")
  (net 15 "Net-(U1-~{RESET}{slash}PB3)")
  (net 16 "Net-(D2-K)")
  (net 17 "Net-(U4-BAT)")
  (net 18 "Net-(U4-~{CHRG})")
  (net 19 "Net-(U4-PROG)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 126.225 104.56)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 101.25 111.325)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "SLR+" (at 0.08 1.365) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 3 "SolarPanel+") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:TSOT-23-5" (layer "F.Cu")
    (at 114.1375 112.425)
    (descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSOT TO_SOT_SMD")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Constant-current/constant-voltage linear charger for single cell lithium-ion batteries with 2.9V Trickle Charge, 4.5V to 6.5V VDD, -40 to +85 degree Celsius, TSOT-23-5")
    (property "ki_keywords" "Constant-current constant-voltage linear charger single cell lithium-ion battery")
    (attr smd)
    (fp_text reference "U4" (at -0.025 -2.175) (layer "F.SilkS"))
    (fp_text value "LTC4054" (at 0.5725 2.105) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(U4-~{CHRG})") (pinfunction "~{CHRG}") (pintype "open_collector"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND1") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U4-BAT)") (pinfunction "BAT") (pintype "power_out"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "V_{CC}") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(U4-PROG)") (pinfunction "PROG") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 110.8 113.225 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -2.095 1.67 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "Net-(U4-BAT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 115.275 118.85 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0.04 -1.415 90) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.315 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 19 "Net-(U4-PROG)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 119.475 119.025)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -1.1 -1.55) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "++Sherms-Custom-Libs:SOT95P270X145-5N-7230" (layer "F.Cu")
    (at 107.125 112.25)
    (descr "(OT) [SOT-23]")
    (tags "Integrated Circuit")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (attr smd)
    (fp_text reference "U3" (at -0.285 -2.2) (layer "F.SilkS"))
    (fp_text value "BU7230-Comparator-5pin" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.25 -0.95 90) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "SolarPanel+") (pinfunction "-") (pintype "input"))
    (pad "2" smd rect (at -1.25 0 90) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND1") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd rect (at -1.25 0.95 90) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(U3-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd rect (at 1.25 0.95 90) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(R10-Pad1)") (pintype "open_collector"))
    (pad "5" smd rect (at 1.25 -0.95 90) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "V+") (pintype "power_in"))
    (model "MCP6546UT-E_OT.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 123.835 117.945)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (attr through_hole)
    (fp_text reference "U2" (at -0.135 -1.895) (layer "F.SilkS"))
    (fp_text value "ATtiny10-ISP" (at 1.27 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-PB0)") (pinfunction "MISO-PB0") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-PB1)") (pinfunction "SCK-PB1") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(U2-MOSI)") (pinfunction "MOSI") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(U1-~{RESET}{slash}PB3)") (pinfunction "~{RST-PB3}") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 125.675 113.4)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -0.9 -1.575) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.875 -1.6) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 9 "Net-(U1-PB0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 12 "Net-(U2-MOSI)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 121.9 104.875)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.73 -1.035) (layer "F.SilkS"))
    (fp_text value "150" (at 0.15 -1.675) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 9 "Net-(U1-PB0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 4 "Net-(J1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 112.125 105.475)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at -0.075 -2.125) (layer "F.SilkS"))
    (fp_text value "Conn_01x02-Battery" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND1") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 112.175 118.375 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -1.335 -1.475 90) (layer "F.SilkS"))
    (fp_text value "220" (at 0.455 -1.545 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 8 "Net-(Q1-G)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(R10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 102.025 116.3)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "SolarPanel+") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND1") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 108.525 117.575 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 1.25 1.575 90) (layer "F.SilkS"))
    (fp_text value "1m" (at -1.325 1.575 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(R10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 115.325 106.8625 90)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D2" (at 0.6825 -1.555 90) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 16 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 1 "VCC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 103.725 111.325 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 -0.91 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(D2-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 18 "Net-(U4-~{CHRG})") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 102.85 107.475 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 2 -1.3) (layer "F.SilkS"))
    (fp_text value "100k" (at -0.025 -1.225) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "SolarPanel+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 121.875 109.9)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -2.865 0.29) (layer "F.SilkS"))
    (fp_text value "150" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(U1-PB2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(J1-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 117.95 107.525 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "    (property \"Reference\" \"#PWR\" (at 0 -3.81 0)")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 2.765 -0.01 180) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (at 119.7125 114.9 180)
    (descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, ADC, SOT-23-6")
    (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "ATtiny10-TS" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(U1-PB0)") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -1.1375 0 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U1-PB1)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at 1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1-PB2)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at 1.1375 0 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" smd roundrect (at 1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U1-~{RESET}{slash}PB3)") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 121.9 107.375)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.58 -1.135) (layer "F.SilkS"))
    (fp_text value "150" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(U1-PB1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(J1-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 112.725 123.6)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "SolarPanel2" (at 0.675 -1.15) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 7 "GND1") (pinfunction "1") (pintype "passive"))
  )
  (footprint "digikey-footprints:SOT-23-3" (layer "F.Cu")
    (at 119.975 122.825)
    (property "Category" "Discrete Semiconductor Products")
    (property "Description" "MOSFET N-CH 20V 3A SOT-23")
    (property "Family" "Transistors - FETs, MOSFETs - Single")
    (property "MPN" "SLS2302")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (property "ki_description" "MOSFET N-CH 60V 115MA SOT-23")
    (property "ki_keywords" "2N7002NCT-ND")
    (attr smd)
    (fp_text reference "Q1" (at -2.405 0.055) (layer "F.SilkS"))
    (fp_text value "SLS2302-A2SHB-N-Mosfet" (at 0.025 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.125 0.15) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(Q1-G)") (pinfunction "G") (pintype "bidirectional") (solder_mask_margin 0.07))
    (pad "2" smd rect (at -1.05 0.95) (size 1.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND1") (pinfunction "S") (pintype "bidirectional") (solder_mask_margin 0.07))
    (pad "3" smd rect (at 1.05 0) (size 1.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "D") (pintype "bidirectional") (solder_mask_margin 0.07))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 108.05 105.75 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0.55 1.5 90) (layer "F.SilkS"))
    (fp_text value "2m" (at -1.05 1.475 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(U3-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 108.4 123.325 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 1.275 1.6) (layer "F.SilkS"))
    (fp_text value "1m" (at -0.625 1.5) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(U3-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 102.875 123.35)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at -1.825 -1.6) (layer "F.SilkS"))
    (fp_text value "1m" (at 0.475 -1.575) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(U3-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 102.825 103.975 180)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (property "Sheetfile" "ATtiny10-firefly-4-leds.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D1" (at 2.1 -1.55) (layer "F.SilkS"))
    (fp_text value "D_Schottky" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 1 "VCC") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 3 "SolarPanel+") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 100.05 102.55) (end 128.35 125)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "ATtiny10 Fire Fly's\nSherman Stebbins\nV1.1" (at 121.55 116.625) (layer "B.SilkS"))
  (gr_text "+" (at 126.405 116.615) (layer "F.SilkS"))
  (gr_text "Red led" (at 116.01 104.05) (layer "F.SilkS"))
  (gr_text "- Solar +" (at 104.175 119.625 90) (layer "F.SilkS"))
  (gr_text "-" (at 104.175 104.925 90) (layer "F.SilkS"))
  (gr_text "+" (at 113.92 104.3) (layer "F.SilkS"))
  (gr_text "Batt -" (at 108.375 109.5) (layer "F.SilkS"))
  (gr_text "7230" (at 106.3 114.53) (layer "F.SilkS"))
  (gr_text "+" (at 115.93 113.96) (layer "F.SilkS"))
  (gr_text "k" (at 105.275 104.4) (layer "F.SilkS"))
  (gr_text "." (at 121.5125 116.46) (layer "F.SilkS"))
  (gr_text "+" (at 112.6 103.58) (layer "F.SilkS"))
  (gr_text "100k" (at 110.7 110.42) (layer "F.SilkS"))
  (gr_text "-" (at 116.28 106.67 180) (layer "F.SilkS"))
  (gr_text "-" (at 126.8 125.01) (layer "F.SilkS"))
  (dimension (type aligned) (layer "F.Cu")
    (pts (xy 100.05 102.55) (xy 128.35 102.55))
    (height -8.85)
    (gr_text "28.3000 mm" (at 114.2 91.9) (layer "F.Cu"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
)
