(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "unconnected-(Connector1-Pad2)")
  (net 3 "unconnected-(Connector1-Pad4)")
  (net 4 "unconnected-(Connector1-Pad6)")
  (net 5 "unconnected-(Connector1-Pad8)")
  (net 6 "unconnected-(Connector1-Pad10)")
  (net 7 "unconnected-(Connector1-Pad20)")
  (net 8 "/HUB_DETECT")
  (net 9 "unconnected-(Connector1-Pad26)")
  (net 10 "/ALERT_PMIC")
  (net 11 "unconnected-(Connector1-Pad29)")
  (net 12 "/Pi_SD_SCK")
  (net 13 "unconnected-(Connector1-Pad32)")
  (net 14 "unconnected-(Connector1-Pad34)")
  (net 15 "unconnected-(Connector1-Pad35)")
  (net 16 "unconnected-(Connector1-Pad36)")
  (net 17 "unconnected-(Connector1-Pad38)")
  (net 18 "unconnected-(Connector1-Pad40)")
  (net 19 "unconnected-(Connector1-Pad41)")
  (net 20 "unconnected-(Connector1-Pad42)")
  (net 21 "/MUX_SEL")
  (net 22 "unconnected-(Connector1-Pad44)")
  (net 23 "/Pi_SD_RX_MISO")
  (net 24 "unconnected-(Connector1-Pad47)")
  (net 25 "unconnected-(Connector1-Pad48)")
  (net 26 "/SD_Detect")
  (net 27 "/Pi_SD_TX_MOSI")
  (net 28 "unconnected-(Connector1-Pad52)")
  (net 29 "unconnected-(Connector1-Pad53)")
  (net 30 "/Pi_SD_CS")
  (net 31 "+3.3V")
  (net 32 "unconnected-(Connector1-Pad56)")
  (net 33 "unconnected-(Connector1-Pad58)")
  (net 34 "unconnected-(Connector1-Pad59)")
  (net 35 "unconnected-(Connector1-Pad60)")
  (net 36 "unconnected-(Connector1-Pad61)")
  (net 37 "unconnected-(Connector1-Pad62)")
  (net 38 "unconnected-(Connector1-Pad63)")
  (net 39 "unconnected-(Connector1-Pad64)")
  (net 40 "unconnected-(Connector1-Pad65)")
  (net 41 "unconnected-(Connector1-Pad66)")
  (net 42 "unconnected-(Connector1-Pad67)")
  (net 43 "unconnected-(Connector1-Pad69)")
  (net 44 "unconnected-(Connector1-Pad70)")
  (net 45 "unconnected-(Connector1-Pad71)")
  (net 46 "/VBUS")
  (net 47 "unconnected-(Connector1-Pad73)")
  (net 48 "unconnected-(Connector1-Pad75)")
  (net 49 "unconnected-(Connector1-PadP2)")
  (net 50 "unconnected-(Connector1-PadP5)")
  (net 51 "unconnected-(Connector1-PadP3)")
  (net 52 "unconnected-(Connector1-PadP1)")
  (net 53 "unconnected-(Connector1-PadP6)")
  (net 54 "unconnected-(Connector1-PadP4)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical_HUB" (layer "F.Cu")
    (at 150.452 82.773)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (property "Sheetfile" "test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x06, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x06_Counter_Clockwise" (at 1.27 15.03) (layer "F.Fab") hide)
    (fp_line (start -12.82 -16.33) (end 12.7 -16.33)
      (layer "Edge.Cuts"))
    (fp_line (start -12.82 1.24) (end -12.82 -16.33)
      (layer "Edge.Cuts"))
    (fp_line (start -12.82 1.24) (end -12.717698 29)
      (layer "Edge.Cuts"))
    (fp_line (start -12.717698 29) (end 12.802302 29)
      (layer "Edge.Cuts"))
    (fp_line (start 12.7 -16.33) (end 12.802302 29)
      (layer "Edge.Cuts"))
    (pad "1" thru_hole custom (at -12.82 0) (size 1.7 1.7) (drill oval 1.5 1 (offset 0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "1" thru_hole rect (at -9.5 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole custom (at -12.82 2.54) (size 1.7 1.7) (drill oval 1.5 1 (offset 0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 46 "/VBUS") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "2" thru_hole oval (at -9.5 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "/VBUS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole custom (at -12.82 5.08) (size 1.7 1.7) (drill oval 1.5 1 (offset 0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 31 "+3.3V") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "3" thru_hole oval (at -9.5 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "+3.3V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole custom (at -12.82 7.62) (size 1.7 1.7) (drill oval 1.5 1 (offset 0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 26 "/SD_Detect") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "4" thru_hole oval (at -9.5 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "/SD_Detect") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole custom (at -12.82 10.16) (size 1.7 1.7) (drill oval 1.5 1 (offset 0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 21 "/MUX_SEL") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "5" thru_hole oval (at -9.5 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/MUX_SEL") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole custom (at -12.82 12.7) (size 1.7 1.7) (drill oval 1.5 1 (offset 0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 12 "/Pi_SD_SCK") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "6" thru_hole oval (at -9.5 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/Pi_SD_SCK") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 9.22 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "7" thru_hole custom (at 12.802302 12.7) (size 1.7 1.7) (drill oval 1.5 1 (offset -0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "8" thru_hole oval (at 9.22 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/HUB_DETECT") (pinfunction "Pin_8") (pintype "passive"))
    (pad "8" thru_hole custom (at 12.802302 10.16) (size 1.7 1.7) (drill oval 1.5 1 (offset -0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 8 "/HUB_DETECT") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "9" thru_hole oval (at 9.22 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/ALERT_PMIC") (pinfunction "Pin_9") (pintype "passive"))
    (pad "9" thru_hole custom (at 12.802302 7.62) (size 1.7 1.7) (drill oval 1.5 1 (offset -0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 10 "/ALERT_PMIC") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "10" thru_hole oval (at 9.22 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/Pi_SD_RX_MISO") (pinfunction "Pin_10") (pintype "passive"))
    (pad "10" thru_hole custom (at 12.802302 5.08) (size 1.7 1.7) (drill oval 1.5 1 (offset -0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 23 "/Pi_SD_RX_MISO") (pinfunction "Pin_10") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "11" thru_hole oval (at 9.22 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/Pi_SD_TX_MOSI") (pinfunction "Pin_11") (pintype "passive"))
    (pad "11" thru_hole custom (at 12.802302 2.54) (size 1.7 1.7) (drill oval 1.5 1 (offset -0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 27 "/Pi_SD_TX_MOSI") (pinfunction "Pin_11") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad "12" thru_hole oval (at 9.22 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/Pi_SD_CS") (pinfunction "Pin_12") (pintype "passive"))
    (pad "12" thru_hole custom (at 12.802302 0) (size 1.7 1.7) (drill oval 1.5 1 (offset -0.4 0)) (property pad_prop_castellated) (layers "*.Cu" "*.Mask")
      (net 30 "/Pi_SD_CS") (pinfunction "Pin_12") (pintype "passive") (thermal_bridge_angle 90)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CNU027S-067-2001-VE:YEU_CNU027S-067-2001-VE" (layer "F.Cu")
    (at 151.432 91.328 90)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/CNU027S-067-2001-VE/ICH/view-part/?ref=eda")
    (property "Description" "\n73 (67 + 6 Power) Position Female Connector M.2 (NGFF) Mini Card Gold-Nickel Black\n")
    (property "MANUFACTURER" "Yamaichi Electronics")
    (property "MF" "Yamaichi Electronics")
    (property "MP" "CNU027S-067-2001-VE")
    (property "PARTREV" "N/A")
    (property "Package" "None")
    (property "Price" "None")
    (property "Purchase-URL" "https://testing.snapeda.com/api/url_track_click_mouser/?unipart_id=6300299&manufacturer=Yamaichi Electronics&part_name=CNU027S-067-2001-VE&search_term=None")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "test.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/CNU027S-067-2001-VE/ICH/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "Hub_Conn" (at -2.462 -0.092 90) (layer "F.SilkS"))
    (fp_text value "CNU027S-067-2001-VE" (at 0.155 -5.745 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -10 -0.575 90) (size 1.4 1.4) (drill 1.4) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 10 -0.575 90) (size 1.4 1.4) (drill 1.4) (layers "*.Cu" "*.Mask"))
    (pad "1" smd rect (at -9.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -9 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "unconnected-(Connector1-Pad2)") (pinfunction "2") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "3" smd rect (at -8.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" smd rect (at -8.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "unconnected-(Connector1-Pad4)") (pinfunction "4") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "5" smd rect (at -8.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" smd rect (at -8 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "unconnected-(Connector1-Pad6)") (pinfunction "6") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "7" smd rect (at -7.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.102))
    (pad "8" smd rect (at -7.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(Connector1-Pad8)") (pinfunction "8") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "9" smd rect (at -7.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "9") (pintype "passive") (solder_mask_margin 0.102))
    (pad "10" smd rect (at -7 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(Connector1-Pad10)") (pinfunction "10") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "11" smd rect (at -6.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "11") (pintype "passive") (solder_mask_margin 0.102))
    (pad "20" smd rect (at -4.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(Connector1-Pad20)") (pinfunction "20") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "21" smd rect (at -4.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "21") (pintype "passive") (solder_mask_margin 0.102))
    (pad "22" smd rect (at -4 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/HUB_DETECT") (pinfunction "22") (pintype "passive") (solder_mask_margin 0.102))
    (pad "23" smd rect (at -3.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "23") (pintype "passive") (solder_mask_margin 0.102))
    (pad "24" smd rect (at -3.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/HUB_DETECT") (pinfunction "24") (pintype "passive") (solder_mask_margin 0.102))
    (pad "25" smd rect (at -3.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "25") (pintype "passive") (solder_mask_margin 0.102))
    (pad "26" smd rect (at -3 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(Connector1-Pad26)") (pinfunction "26") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "27" smd rect (at -2.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "27") (pintype "passive") (solder_mask_margin 0.102))
    (pad "28" smd rect (at -2.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/ALERT_PMIC") (pinfunction "28") (pintype "passive") (solder_mask_margin 0.102))
    (pad "29" smd rect (at -2.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "unconnected-(Connector1-Pad29)") (pinfunction "29") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "30" smd rect (at -2 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/ALERT_PMIC") (pinfunction "30") (pintype "passive") (solder_mask_margin 0.102))
    (pad "31" smd rect (at -1.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/Pi_SD_SCK") (pinfunction "31") (pintype "passive") (solder_mask_margin 0.102))
    (pad "32" smd rect (at -1.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "unconnected-(Connector1-Pad32)") (pinfunction "32") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "33" smd rect (at -1.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/Pi_SD_SCK") (pinfunction "33") (pintype "passive") (solder_mask_margin 0.102))
    (pad "34" smd rect (at -1 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "unconnected-(Connector1-Pad34)") (pinfunction "34") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "35" smd rect (at -0.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "unconnected-(Connector1-Pad35)") (pinfunction "35") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "36" smd rect (at -0.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "unconnected-(Connector1-Pad36)") (pinfunction "36") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "37" smd rect (at -0.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "37") (pintype "passive") (solder_mask_margin 0.102))
    (pad "38" smd rect (at 0 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(Connector1-Pad38)") (pinfunction "38") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "39" smd rect (at 0.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "39") (pintype "passive") (solder_mask_margin 0.102))
    (pad "40" smd rect (at 0.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(Connector1-Pad40)") (pinfunction "40") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "41" smd rect (at 0.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(Connector1-Pad41)") (pinfunction "41") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "42" smd rect (at 1 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(Connector1-Pad42)") (pinfunction "42") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "43" smd rect (at 1.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/MUX_SEL") (pinfunction "43") (pintype "passive") (solder_mask_margin 0.102))
    (pad "44" smd rect (at 1.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(Connector1-Pad44)") (pinfunction "44") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "45" smd rect (at 1.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/MUX_SEL") (pinfunction "45") (pintype "passive") (solder_mask_margin 0.102))
    (pad "46" smd rect (at 2 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/Pi_SD_RX_MISO") (pinfunction "46") (pintype "passive") (solder_mask_margin 0.102))
    (pad "47" smd rect (at 2.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "unconnected-(Connector1-Pad47)") (pinfunction "47") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "48" smd rect (at 2.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(Connector1-Pad48)") (pinfunction "48") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "49" smd rect (at 2.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/SD_Detect") (pinfunction "49") (pintype "passive") (solder_mask_margin 0.102))
    (pad "50" smd rect (at 3 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/Pi_SD_TX_MOSI") (pinfunction "50") (pintype "passive") (solder_mask_margin 0.102))
    (pad "51" smd rect (at 3.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/SD_Detect") (pinfunction "51") (pintype "passive") (solder_mask_margin 0.102))
    (pad "52" smd rect (at 3.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "unconnected-(Connector1-Pad52)") (pinfunction "52") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "53" smd rect (at 3.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(Connector1-Pad53)") (pinfunction "53") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "54" smd rect (at 4 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/Pi_SD_CS") (pinfunction "54") (pintype "passive") (solder_mask_margin 0.102))
    (pad "55" smd rect (at 4.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V") (pinfunction "55") (pintype "passive") (solder_mask_margin 0.102))
    (pad "56" smd rect (at 4.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "unconnected-(Connector1-Pad56)") (pinfunction "56") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "57" smd rect (at 4.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "+3.3V") (pinfunction "57") (pintype "passive") (solder_mask_margin 0.102))
    (pad "58" smd rect (at 5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(Connector1-Pad58)") (pinfunction "58") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "59" smd rect (at 5.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "unconnected-(Connector1-Pad59)") (pinfunction "59") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "60" smd rect (at 5.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(Connector1-Pad60)") (pinfunction "60") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "61" smd rect (at 5.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "unconnected-(Connector1-Pad61)") (pinfunction "61") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "62" smd rect (at 6 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(Connector1-Pad62)") (pinfunction "62") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "63" smd rect (at 6.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "unconnected-(Connector1-Pad63)") (pinfunction "63") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "64" smd rect (at 6.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(Connector1-Pad64)") (pinfunction "64") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "65" smd rect (at 6.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(Connector1-Pad65)") (pinfunction "65") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "66" smd rect (at 7 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "unconnected-(Connector1-Pad66)") (pinfunction "66") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "67" smd rect (at 7.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "unconnected-(Connector1-Pad67)") (pinfunction "67") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "68" smd rect (at 7.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "68") (pintype "passive") (solder_mask_margin 0.102))
    (pad "69" smd rect (at 7.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(Connector1-Pad69)") (pinfunction "69") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "70" smd rect (at 8 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "unconnected-(Connector1-Pad70)") (pinfunction "70") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "71" smd rect (at 8.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "unconnected-(Connector1-Pad71)") (pinfunction "71") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "72" smd rect (at 8.5 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/VBUS") (pinfunction "72") (pintype "passive") (solder_mask_margin 0.102))
    (pad "73" smd rect (at 8.75 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "unconnected-(Connector1-Pad73)") (pinfunction "73") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "74" smd rect (at 9 3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/VBUS") (pinfunction "74") (pintype "passive") (solder_mask_margin 0.102))
    (pad "75" smd rect (at 9.25 -3 90) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "unconnected-(Connector1-Pad75)") (pinfunction "75") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "P1" smd rect (at -11.55 -2.775 90) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "unconnected-(Connector1-PadP1)") (pinfunction "P1") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "P2" smd rect (at -10.9 -2.775 90) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "unconnected-(Connector1-PadP2)") (pinfunction "P2") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "P3" smd rect (at -10.25 -2.775 90) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "unconnected-(Connector1-PadP3)") (pinfunction "P3") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "P4" smd rect (at 10.25 -2.775 90) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "unconnected-(Connector1-PadP4)") (pinfunction "P4") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "P5" smd rect (at 10.9 -2.775 90) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "unconnected-(Connector1-PadP5)") (pinfunction "P5") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "P6" smd rect (at 11.55 -2.775 90) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "unconnected-(Connector1-PadP6)") (pinfunction "P6") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "SH1" thru_hole oval (at -13.4 0 90) (size 0.9 2.9) (drill oval 0.5 2.5) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.102))
    (pad "SH2" thru_hole oval (at 13.4 0 90) (size 0.9 2.9) (drill oval 0.5 2.5) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.102))
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 151.42 69.79)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (gr_arc (start 138.55 111.73) (mid 137.915219 111.60042) (end 137.709983 110.985915)
    (layer "Edge.Cuts"))
  (gr_arc (start 163.23 110.85) (mid 163.098607 111.548096) (end 162.42236 111.765566)
    (layer "Edge.Cuts"))
  (gr_arc (start 137.640001 67.27) (mid 137.816046 66.593236) (end 138.503625 66.46581)
    (layer "Edge.Cuts"))
  (gr_arc (start 162.549318 66.430239) (mid 163.021175 66.735225) (end 163.109999 67.29)
    (layer "Edge.Cuts"))
  (gr_text "SD_MOSI" (at 155.82 84.97) (layer "F.SilkS"))
  (gr_text "SD_CS" (at 156.16 82.95) (layer "F.SilkS"))
  (gr_text "GND" (at 142.18 83.16) (layer "F.SilkS"))
  (gr_text "SD_SCK" (at 142.18 95.74) (layer "F.SilkS"))
  (gr_text "SD_MISO" (at 155.75 87.33) (layer "F.SilkS"))
  (gr_text "HUB_Det" (at 155.89 92.32) (layer "F.SilkS"))
  (gr_text "3.3V" (at 142.25 88.05) (layer "F.SilkS"))
  (gr_text "GND" (at 156.59 95.6) (layer "F.SilkS"))
  (gr_text "ALERT" (at 155.93 89.77) (layer "F.SilkS"))
  (gr_text "SD_Det" (at 142.27 90.8) (layer "F.SilkS"))
  (gr_text "MUX_Sel" (at 142.32 93.15) (layer "F.SilkS"))
  (gr_text "VBUS" (at 142.27 85.59) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 163.322 111.76)
        (xy 137.668 111.76)
        (xy 137.668 66.294)
        (xy 163.068 66.294)
        (xy 163.068 66.548)
        (xy 163.322 66.548)
      )
    )
  )
  (zone (net 31) (net_name "+3.3V") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 163.068 77.978)
        (xy 163.322 103.886)
        (xy 163.322 111.76)
        (xy 137.668 111.76)
        (xy 137.668 66.294)
        (xy 163.068 66.548)
        (xy 163.068 78.74)
      )
    )
  )
)
