<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="38.1" y2="0" width="0.1524" layer="20"/>
<wire x1="74.93" y1="11.0998" x2="74.93" y2="43.18" width="0.1524" layer="20"/>
<wire x1="74.93" y1="43.18" x2="5.08" y2="43.18" width="0.1524" layer="20"/>
<wire x1="5.08" y1="43.18" x2="0" y2="40.64" width="0.1524" layer="20"/>
<wire x1="0" y1="40.64" x2="0" y2="0" width="0.1524" layer="20"/>
<text>RV-Project.Com</text>
<text>LED Remote Driver Dimmer 
Ver 2.23     2/13/2019</text>
<circle x="8.9154" y="19.05" radius="6.35" width="0.1524" layer="20"/>
<wire x1="38.1" y1="0" x2="38.1" y2="11.0998" width="0.1524" layer="20"/>
<wire x1="38.1" y1="11.0998" x2="74.93" y2="11.0998" width="0.1524" layer="20"/>
<text>LED 1</text>
<text>LED 2</text>
<text>2A</text>
<text>GND</text>
<text>GND</text>
<text>12V</text>
<text>ON-OFF-ON</text>
<text>350mA Max</text>
<text>Negative</text>
<text>Cut Out</text>
<text>Status</text>
<text>B:CW=Max
A:CCW=Max</text>
<text>12V</text>
<text>Dim Adjust</text>
<wire x1="10.4394" y1="30.4546" x2="7.3152" y2="30.48" width="0.1524" layer="20" curve="-175.381874"/>
<wire x1="7.3152" y1="31.7754" x2="10.4394" y2="31.7754" width="0.1524" layer="20" curve="-175.381874"/>
<wire x1="10.4394" y1="6.3246" x2="7.3152" y2="6.3246" width="0.1524" layer="20" curve="-175.381874"/>
<wire x1="7.3152" y1="7.6454" x2="10.4394" y2="7.6454" width="0.1524" layer="20" curve="-175.381874"/>
<wire x1="7.3406" y1="30.3784" x2="7.3152" y2="30.48" width="0.1524" layer="20"/>
<wire x1="7.3152" y1="30.48" x2="7.3152" y2="31.7754" width="0.1524" layer="20"/>
<wire x1="10.4394" y1="30.4546" x2="10.4394" y2="31.7754" width="0.1524" layer="20"/>
<wire x1="10.4394" y1="6.3246" x2="10.4394" y2="7.6454" width="0.1524" layer="20"/>
<wire x1="7.3152" y1="7.6454" x2="7.3152" y2="6.3246" width="0.1524" layer="20"/>
<text>Jumper
Option</text>
<text>Jumper R1 when
using 12V LED</text>
<text>Alternate 
Halo</text>
<text>12V</text>
<text>GND</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="MO1-18AWG">
</package>
<package name="ALPHARD901F">
</package>
<package name="MICRO_RECEIVER_1">
</package>
<package name="WAFER2PIN">
</package>
<package name="251SMALL">
</package>
<package name="D041-3.5MIL">
</package>
<package name="1X01_HEADER">
</package>
<package name="LUXDRIVE350">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="BIGFOOT_MEDIUM">
</package>
<package name="RADIAL_ELECTROLYTIC_200MIL(10MM)">
</package>
<package name="SMD-JUMPER_3">
</package>
<package name="ALPHA1/2WPOTENTIOMETER">
</package>
<package name="1/4W_AXIAL_RESISTOR_3.5MIL(V2)">
<description>Axial 1/4Watt Resistor&lt;p&gt;0.35" (tiny) footprint</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP3" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP6" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP7" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP8" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP9" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="R2" library="a-lib" package="ALPHARD901F" value="">
<attribute name="NAME"/>
</element>
<element name="RX1" library="a-lib" package="MICRO_RECEIVER_1" value="MICRO_RECEIVER_1"/>
<element name="JP2" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="J1" library="a-lib" package="WAFER2PIN" value="WAFER2PHORIZONTAL"/>
<element name="F1" library="a-lib" package="251SMALL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="JP4" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="M1" library="a-lib" package="LUXDRIVE350" value="3021DE"/>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="$1_15_$_2019-01-26_03-19-16" library="a-lib" package="BIGFOOT_MEDIUM" value="Bigfoot Medium"/>
<element name="C1" library="a-lib" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="220UF">
<attribute name="MARKING" value="227"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="LOGO1" library="a-lib" package="BIGFOOT_MEDIUM" value="Bigfoot Medium"/>
<element name="J2" library="a-lib" package="SMD-JUMPER_3" value="SMD-JUMPER"/>
<element name="R3" library="a-lib" package="ALPHA1/2WPOTENTIOMETER" value=""/>
<element name="R1" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
</element>
<element name="JP10" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="RX1" pad="NO1"/>
<contactref element="JP3" pad="P$1"/>
<contactref element="JP4" pad="1"/>
<contactref element="M1" pad="VCC"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP8" pad="P$1"/>
<contactref element="JP7" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="JP6" pad="P$1"/>
<contactref element="M1" pad="LED+"/>
</signal>
<signal name="N$7">
<contactref element="JP9" pad="P$1"/>
<contactref element="M1" pad="LED-"/>
</signal>
<signal name="N$8">
<contactref element="RX1" pad="12V1"/>
<contactref element="RX1" pad="COM1"/>
<contactref element="JP1" pad="P$1"/>
<contactref element="LED1" pad="A"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="P$1"/>
<contactref element="F1" pad="P$1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="GND">
<contactref element="RX1" pad="GND1"/>
<contactref element="D1" pad="A"/>
<contactref element="JP5" pad="1"/>
<contactref element="M1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="P$2"/>
<contactref element="R1" pad="1"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="M1" pad="REF"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="M1" pad="CTRL"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R2" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="3"/>
<contactref element="R2" pad="3"/>
<contactref element="R3" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="P$1"/>
<contactref element="F1" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="K"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
