(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 13)
    (no_connects 5)
    (area 158.924999 99.724999 203.075001 129.075001)
    (thickness 1.6)
    (drawings 7)
    (tracks 97)
    (zones 0)
    (modules 3)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad9)")
  (net 2 "Net-(J1-Pad5)")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J1-Pad6)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module rj45mid:rj45mid (layer F.Cu) (tedit 593474EC)
    (at 181 129 180)
    (fp_text reference J1 (at -5.2 15.25 180) (layer F.SilkS))
    (fp_text value RJ45 (at 0.1 15.45 180) (layer F.Fab))
    (fp_arc (start -6.5 9.45) (end -6.5 9.95) (angle 90) (layer Edge.Cuts) (width 0.15))
    (fp_arc (start 6.5 9.45) (end 7 9.45) (angle 90) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 9.45) (end 7 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 2.55) (end -7 9.45) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 6.5 9.95) (end -6.5 9.95) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7.2 2.55) (end -7 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7.2 0) (end 7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7.2 0) (end -7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 2.55) (end 7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (pad "" np_thru_hole circle (at -6 12.45 180) (size 1.524 1.524) (drill 1.05) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 12.45 180) (size 1.524 1.524) (drill 1.05) (layers *.Cu *.Mask))
    (pad 9 thru_hole rect (at -8.5 5.65 180) (size 2.5 6) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 9 thru_hole rect (at 8.5 5.65 180) (size 2.5 6) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 5 smd rect (at -0.51 12.75 180) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad5)"))
    (pad 4 smd rect (at 0.51 12.75 180) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at -1.53 12.75 180) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 3 smd rect (at 1.53 12.75 180) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 2.55 12.75 180) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 7 smd rect (at -2.55 12.75 180) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at -3.57 12.75 180) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 1 smd rect (at 3.57 12.75 180) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad1)"))
  )
  (module rj45mid:rj45mid (layer F.Cu) (tedit 593474EC)
    (at 191.5 99.8)
    (fp_text reference J3 (at -5.2 15.25) (layer F.SilkS))
    (fp_text value RJ45 (at 0.1 15.45) (layer F.Fab))
    (fp_arc (start -6.5 9.45) (end -6.5 9.95) (angle 90) (layer Edge.Cuts) (width 0.15))
    (fp_arc (start 6.5 9.45) (end 7 9.45) (angle 90) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 9.45) (end 7 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 2.55) (end -7 9.45) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 6.5 9.95) (end -6.5 9.95) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7.2 2.55) (end -7 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7.2 0) (end 7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7.2 0) (end -7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 2.55) (end 7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (pad "" np_thru_hole circle (at -6 12.45) (size 1.524 1.524) (drill 1.05) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 12.45) (size 1.524 1.524) (drill 1.05) (layers *.Cu *.Mask))
    (pad 9 thru_hole rect (at -8.5 5.65) (size 2.5 6) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 9 thru_hole rect (at 8.5 5.65) (size 2.5 6) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 5 smd rect (at -0.51 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.51 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.53 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 3 smd rect (at 1.53 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 2 smd rect (at 2.55 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad5)"))
    (pad 7 smd rect (at -2.55 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -3.57 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 3.57 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad4)"))
  )
  (module rj45mid:rj45mid (layer F.Cu) (tedit 593474EC)
    (at 170.5 99.8)
    (fp_text reference J2 (at -5.2 15.25) (layer F.SilkS))
    (fp_text value RJ45 (at 0.1 15.45) (layer F.Fab))
    (fp_arc (start -6.5 9.45) (end -6.5 9.95) (angle 90) (layer Edge.Cuts) (width 0.15))
    (fp_arc (start 6.5 9.45) (end 7 9.45) (angle 90) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 9.45) (end 7 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 2.55) (end -7 9.45) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 6.5 9.95) (end -6.5 9.95) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7.2 2.55) (end -7 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7.2 0) (end 7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7.2 0) (end -7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 2.55) (end 7.2 2.55) (layer Edge.Cuts) (width 0.15))
    (pad "" np_thru_hole circle (at -6 12.45) (size 1.524 1.524) (drill 1.05) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 12.45) (size 1.524 1.524) (drill 1.05) (layers *.Cu *.Mask))
    (pad 9 thru_hole rect (at -8.5 5.65) (size 2.5 6) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 9 thru_hole rect (at 8.5 5.65) (size 2.5 6) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 5 smd rect (at -0.51 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.51 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.53 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 3 smd rect (at 1.53 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 2.55 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 7 smd rect (at -2.55 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -3.57 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 3.57 12.75) (size 0.45 2.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad1)"))
  )
  (gr_line (start 177.7 99.8) (end 184.3 99.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203 99.8) (end 203 129) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.7 99.8) (end 203 99.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 129) (end 173.8 129) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 99.8) (end 159 129) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.3 99.8) (end 159 99.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 188.2 129) (end 203 129) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name "Net-(J1-Pad9)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203 99.8) (xy 159 99.8) (xy 159 129) (xy 203 129)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pad9)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203 99.8) (xy 159 99.8) (xy 159 129) (xy 203 129)
      )
    )
  )
)
