(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "LOGO" (layer "F.Cu")
    (at 150.1 72.2 -10)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0 170) (layer "F.SilkS"))
    (fp_text value "LOGO" (at 0.75 0 170) (layer "F.SilkS") hide)
  )
  (gr_curve (pts (xy 134.6 72.4) (xy 134.6 69.747835) (xy 136.180353 67.204296) (xy 138.993398 65.328932))
    (layer "Edge.Cuts"))
  (gr_curve (pts (xy 149.6 82.4) (xy 145.621753 82.4) (xy 141.806444 81.346432) (xy 138.993398 79.471068))
    (layer "Edge.Cuts"))
  (gr_curve (pts (xy 160.206602 79.471068) (xy 157.393556 81.346432) (xy 153.578247 82.4) (xy 149.6 82.4))
    (layer "Edge.Cuts"))
  (gr_curve (pts (xy 138.993398 65.328932) (xy 141.806444 63.453568) (xy 145.621753 62.4) (xy 149.6 62.4))
    (layer "Edge.Cuts"))
  (gr_curve (pts (xy 149.6 62.4) (xy 153.578247 62.4) (xy 157.393556 63.453568) (xy 160.206602 65.328932))
    (layer "Edge.Cuts"))
  (gr_curve (pts (xy 164.6 72.4) (xy 164.6 75.052165) (xy 163.019647 77.595704) (xy 160.206602 79.471068))
    (layer "Edge.Cuts"))
  (gr_curve (pts (xy 138.993398 79.471068) (xy 136.180353 77.595704) (xy 134.6 75.052165) (xy 134.6 72.4))
    (layer "Edge.Cuts"))
  (gr_curve (pts (xy 160.206602 65.328932) (xy 163.019647 67.204296) (xy 164.6 69.747835) (xy 164.6 72.4))
    (layer "Edge.Cuts"))
)
