(kicad_pcb (version 20171130) (host pcbnew 5.0.2-5.fc29)
  (general
    (thickness 1.6002)
    (drawings 44)
    (tracks 153)
    (zones 0)
    (modules 3)
    (nets 40)
  )
  (page USLetter)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 1.905 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.43 1.27)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad39)")
  (net 2 "Net-(J1-Pad37)")
  (net 3 "Net-(J1-Pad35)")
  (net 4 "Net-(J1-Pad33)")
  (net 5 "Net-(J1-Pad31)")
  (net 6 "Net-(J1-Pad29)")
  (net 7 "Net-(J1-Pad27)")
  (net 8 "Net-(J1-Pad25)")
  (net 9 "Net-(J1-Pad23)")
  (net 10 "Net-(J1-Pad21)")
  (net 11 "Net-(J1-Pad19)")
  (net 12 "Net-(J1-Pad17)")
  (net 13 "Net-(J1-Pad15)")
  (net 14 "Net-(J1-Pad13)")
  (net 15 "Net-(J1-Pad11)")
  (net 16 "Net-(J1-Pad9)")
  (net 17 "Net-(J1-Pad7)")
  (net 18 "Net-(J1-Pad5)")
  (net 19 "Net-(J1-Pad3)")
  (net 20 "Net-(J1-Pad1)")
  (net 21 "Net-(J2-Pad2)")
  (net 22 "Net-(J2-Pad4)")
  (net 23 "Net-(J2-Pad6)")
  (net 24 "Net-(J2-Pad8)")
  (net 25 "Net-(J2-Pad10)")
  (net 26 "Net-(J2-Pad12)")
  (net 27 "Net-(J2-Pad14)")
  (net 28 "Net-(J2-Pad16)")
  (net 29 "Net-(J2-Pad18)")
  (net 30 "Net-(J2-Pad20)")
  (net 31 "Net-(J2-Pad22)")
  (net 32 "Net-(J2-Pad24)")
  (net 33 "Net-(J2-Pad26)")
  (net 34 "Net-(J2-Pad28)")
  (net 35 "Net-(J2-Pad30)")
  (net 36 "Net-(J2-Pad32)")
  (net 37 "Net-(J2-Pad34)")
  (net 38 "Net-(J2-Pad36)")
  (net 39 "Net-(J2-Pad38)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J1-Pad29)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad31)")
    (add_net "Net-(J1-Pad33)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad39)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad8)")
  )
  (module harman:PinHeader_2x10_P2.54mm_Vertical_Odd (layer Bottom) (tedit 5C959D3E)
    (at 150.790001 74.930001 180)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at 1.27 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_02x10_Odd (at 1.27 -25.19 180) (layer B.Fab))
    (fp_text user %R (at 1.27 -11.43 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad3)"))
    (pad 5 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad5)"))
    (pad 7 thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad7)"))
    (pad 9 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad9)"))
    (pad 11 thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad11)"))
    (pad 13 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad13)"))
    (pad 15 thru_hole oval (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad15)"))
    (pad 17 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad17)"))
    (pad 19 thru_hole oval (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad19)"))
    (pad 21 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad21)"))
    (pad 23 thru_hole oval (at 2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad23)"))
    (pad 25 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad25)"))
    (pad 27 thru_hole oval (at 2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad27)"))
    (pad 29 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad29)"))
    (pad 31 thru_hole oval (at 2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad31)"))
    (pad 33 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad33)"))
    (pad 35 thru_hole oval (at 2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad35)"))
    (pad 37 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad37)"))
    (pad 39 thru_hole oval (at 2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad39)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 5767007-8:TE_5767007-8 (layer Top) (tedit 5C95AF22)
    (at 132.690001 86.355001 90)
    (attr smd)
    (fp_text reference J2 (at -3.71127 -5.63694 90) (layer F.SilkS) hide)
    (fp_text value 5767007-8 (at -3.07904 5.37203 90) (layer F.SilkS) hide)
    (pad 1 smd oval (at 5.715 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 20 "Net-(J1-Pad1)"))
    (pad 2 smd oval (at 5.715 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 3 smd oval (at 5.075 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 19 "Net-(J1-Pad3)"))
    (pad 4 smd oval (at 5.075 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 22 "Net-(J2-Pad4)"))
    (pad 5 smd oval (at 4.435 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 18 "Net-(J1-Pad5)"))
    (pad 6 smd oval (at 4.435 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 23 "Net-(J2-Pad6)"))
    (pad 7 smd oval (at 3.795 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 17 "Net-(J1-Pad7)"))
    (pad 8 smd oval (at 3.795 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 24 "Net-(J2-Pad8)"))
    (pad 9 smd oval (at 3.155 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 16 "Net-(J1-Pad9)"))
    (pad 10 smd oval (at 3.155 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 25 "Net-(J2-Pad10)"))
    (pad 11 smd oval (at 2.515 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 15 "Net-(J1-Pad11)"))
    (pad 12 smd oval (at 2.515 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 26 "Net-(J2-Pad12)"))
    (pad 13 smd oval (at 1.875 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 14 "Net-(J1-Pad13)"))
    (pad 14 smd oval (at 1.875 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 27 "Net-(J2-Pad14)"))
    (pad 15 smd oval (at 1.235 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 13 "Net-(J1-Pad15)"))
    (pad 16 smd oval (at 1.235 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 28 "Net-(J2-Pad16)"))
    (pad 17 smd oval (at 0.595 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 12 "Net-(J1-Pad17)"))
    (pad 18 smd oval (at 0.595 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 29 "Net-(J2-Pad18)"))
    (pad 19 smd oval (at -0.045 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 11 "Net-(J1-Pad19)"))
    (pad 20 smd oval (at -0.045 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 30 "Net-(J2-Pad20)"))
    (pad 21 smd oval (at -0.685 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 10 "Net-(J1-Pad21)"))
    (pad 22 smd oval (at -0.685 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 31 "Net-(J2-Pad22)"))
    (pad 23 smd oval (at -1.325 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 9 "Net-(J1-Pad23)"))
    (pad 24 smd oval (at -1.325 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 32 "Net-(J2-Pad24)"))
    (pad 25 smd oval (at -1.965 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 8 "Net-(J1-Pad25)"))
    (pad 26 smd oval (at -1.965 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 33 "Net-(J2-Pad26)"))
    (pad 27 smd oval (at -2.605 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 7 "Net-(J1-Pad27)"))
    (pad 28 smd oval (at -2.605 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 34 "Net-(J2-Pad28)"))
    (pad 29 smd oval (at -3.245 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 6 "Net-(J1-Pad29)"))
    (pad 30 smd oval (at -3.245 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 35 "Net-(J2-Pad30)"))
    (pad 31 smd oval (at -3.885 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 5 "Net-(J1-Pad31)"))
    (pad 32 smd oval (at -3.885 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 36 "Net-(J2-Pad32)"))
    (pad 33 smd oval (at -4.525 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 4 "Net-(J1-Pad33)"))
    (pad 34 smd oval (at -4.525 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 37 "Net-(J2-Pad34)"))
    (pad 35 smd oval (at -5.165 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 3 "Net-(J1-Pad35)"))
    (pad 36 smd oval (at -5.165 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 38 "Net-(J2-Pad36)"))
    (pad 37 smd oval (at -5.805 3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 2 "Net-(J1-Pad37)"))
    (pad 38 smd oval (at -5.805 -3.53 90) (size 0.43 1.27) (layers Top F.Paste F.Mask)
      (net 39 "Net-(J2-Pad38)"))
    (pad Hole np_thru_hole circle (at 11.425 0 90) (size 2.39 2.39) (drill 2.39) (layers *.Cu *.Mask F.SilkS))
    (pad S1 thru_hole circle (at 5.075 0 90) (size 1.318 1.318) (drill 0.81) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad39)"))
    (pad S2 thru_hole circle (at 2.535 0 90) (size 1.318 1.318) (drill 0.81) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad39)"))
    (pad S3 thru_hole circle (at -0.005 0 90) (size 1.318 1.318) (drill 0.81) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad39)"))
    (pad S4 thru_hole circle (at -2.545 0 90) (size 1.318 1.318) (drill 0.81) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad39)"))
    (pad S5 thru_hole circle (at -5.085 0 90) (size 1.318 1.318) (drill 0.81) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad39)"))
  )
  (module harman:PinHeader_2x10_P2.54mm_Vertical_Even (layer Bottom) (tedit 5C959D3A)
    (at 117.775001 74.930001 180)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J3 (at 1.27 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_02x10_Even (at 1.27 -25.19 180) (layer B.Fab))
    (fp_text user %R (at 1.27 -11.43 90) (layer B.Fab))
    (pad 40 thru_hole oval (at 2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad39)"))
    (pad 38 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad38)"))
    (pad 36 thru_hole oval (at 2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad36)"))
    (pad 34 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad34)"))
    (pad 32 thru_hole oval (at 2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad32)"))
    (pad 30 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad30)"))
    (pad 28 thru_hole oval (at 2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad28)"))
    (pad 26 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad26)"))
    (pad 24 thru_hole oval (at 2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad24)"))
    (pad 22 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad22)"))
    (pad 20 thru_hole oval (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad20)"))
    (pad 18 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad18)"))
    (pad 16 thru_hole oval (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad16)"))
    (pad 14 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad14)"))
    (pad 12 thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad12)"))
    (pad 10 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad10)"))
    (pad 8 thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad8)"))
    (pad 6 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad6)"))
    (pad 4 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad4)"))
    (pad 2 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 113.284 97.79) (layer B.SilkS))
  (gr_text GND (at 145.542 97.79) (layer B.SilkS))
  (gr_text 35 (at 145.415 95.25) (layer B.SilkS))
  (gr_text 31 (at 145.415 92.71) (layer B.SilkS))
  (gr_text 27 (at 145.415 90.17) (layer B.SilkS))
  (gr_text 23 (at 145.415 87.63) (layer B.SilkS))
  (gr_text 07 (at 145.415 77.47) (layer B.SilkS))
  (gr_text 33 (at 153.035 95.25) (layer B.SilkS))
  (gr_text 29 (at 153.035 92.71) (layer B.SilkS))
  (gr_text 25 (at 153.035 90.17) (layer B.SilkS))
  (gr_text GND (at 153.035 77.47) (layer B.SilkS))
  (gr_text 36 (at 113.03 95.25) (layer B.SilkS))
  (gr_text 32 (at 113.03 92.71) (layer B.SilkS))
  (gr_text 34 (at 120.015 95.25) (layer B.SilkS))
  (gr_text 30 (at 120.015 92.71) (layer B.SilkS))
  (gr_text 26 (at 120.015 90.17) (layer B.SilkS))
  (gr_text 28 (at 113.03 90.17) (layer B.SilkS))
  (gr_text 24 (at 113.03 87.63) (layer B.SilkS))
  (gr_text 22 (at 120.015 87.63) (layer B.SilkS))
  (gr_text 20 (at 113.03 85.09) (layer B.SilkS))
  (gr_text 18 (at 120.015 85.09) (layer B.SilkS))
  (gr_text 16 (at 113.03 82.55) (layer B.SilkS))
  (gr_text 10 (at 120.015 80.01) (layer B.SilkS))
  (gr_text 08 (at 113.03 77.47) (layer B.SilkS))
  (gr_text 06 (at 120.015 77.47) (layer B.SilkS))
  (gr_text Vsup (at 120.015 82.55) (layer B.SilkS))
  (gr_text Vtref (at 113.03 80.01) (layer B.SilkS))
  (gr_line (start 160.02 71.12) (end 106.68 71.12) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.02 101.6) (end 160.02 71.12) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 106.68 101.6) (end 160.02 101.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 106.68 71.12) (end 106.68 101.6) (layer Edge.Cuts) (width 0.1))
  (gr_text TRST (at 153.035 87.63) (layer B.SilkS))
  (gr_text TDI (at 145.415 85.09) (layer B.SilkS))
  (gr_text TMS (at 153.035 85.09) (layer B.SilkS))
  (gr_text TCK (at 145.415 82.55) (layer B.SilkS))
  (gr_text RTCK (at 153.035 82.55) (layer B.SilkS))
  (gr_text TDO (at 145.415 80.01) (layer B.SilkS))
  (gr_text SRST (at 153.035 80.01) (layer B.SilkS))
  (gr_text 38 (at 120.015 97.79) (layer B.SilkS))
  (gr_text 04 (at 113.03 74.93) (layer B.SilkS))
  (gr_text 02 (at 120.015 74.93) (layer B.SilkS))
  (gr_text 37 (at 154.94 97.79) (layer B.SilkS))
  (gr_text 03 (at 145.415 74.93) (layer B.SilkS))
  (gr_text 01 (at 153.035 74.93) (layer B.SilkS))
)
