(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 23)
    (no_connects 0)
    (area 124.862599 93.47206 170.025001 106.228123)
    (thickness 1.6)
    (drawings 8)
    (tracks 35)
    (zones 0)
    (modules 11)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (trace_clearance 0.1524)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.05)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 1.3716 0.6604)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.3 0.3)
    (mod_text_width 0.05)
    (pad_size 1.25 1.25)
    (pad_drill 0.85)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 /RUN_PD)
  (net 6 /LDO_VIN)
  (net 7 /V_OUT_CONN)
  (net 8 /LDO_VFB)
  (net 9 /LDO_SW)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /LDO_SW)
    (add_net /LDO_VFB)
    (add_net /LDO_VIN)
    (add_net /RUN_PD)
    (add_net /V_OUT_CONN)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5951D7AD)
    (at 139.6 102.3 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.3 0.3 180) (layer F.SilkS))
    (fp_text value 330kΩ (at -2.7 -0.4 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 9 /LDO_SW))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 8 /LDO_VFB))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 594EF745)
    (at 137.2 96.5)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -1.2 -1.1) (layer F.SilkS))
    (fp_text value 4.7µF (at 1 -1.1) (layer F.Fab))
    (fp_text user %R (at -1.2 -1.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 6 /LDO_VIN))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5951D7B5)
    (at 139.6 104.3 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.2 0.3 180) (layer F.SilkS))
    (fp_text value 22pF (at -2.4 -0.3 180) (layer F.Fab))
    (fp_text user %R (at 0.02 0.06 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 7 /V_OUT_CONN))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 8 /LDO_VFB))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 594EF755)
    (at 142.2 96.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 1.14 1.12 180) (layer F.SilkS))
    (fp_text value 4.7µF (at -0.96 1.12 180) (layer F.Fab))
    (fp_text user %R (at 1.14 1.12 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 7 /V_OUT_CONN))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:USB_Micro-B (layer F.Cu) (tedit 5959A843)
    (at 129.3 99.9 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 0 -2.8 270) (layer F.SilkS))
    (fp_text value USB_OTG (at -0.1 2.2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask)
      (net 6 /LDO_VIN))
    (pad 2 smd rect (at -0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -2.5 -1.35) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.5 -1.35) (size 1.25 1.25) (drill oval 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.5 1.35) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.5 1.35) (size 1.55 1.55) (drill oval 1.15) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5959A76D)
    (at 155.8 100.8 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J2 (at -8.45 5.75 360) (layer F.SilkS))
    (fp_text value BARREL_JACK (at -6.1 -4 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 7 /V_OUT_CONN))
    (pad 2 thru_hole rect (at -6 0 180) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole rect (at -3 4.7 180) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 5 /RUN_PD))
  )
  (module popsu_footprints:5KT (layer F.Cu) (tedit 593F75DF)
    (at 148 101.2 90)
    (fp_text reference L1 (at 0 -4.625 90) (layer F.SilkS))
    (fp_text value 10µH (at 0 4.625 90) (layer F.Fab))
    (pad 1 smd rect (at 2.8 0 90) (size 1.55 1.7) (layers F.Cu F.Mask)
      (net 9 /LDO_SW))
    (pad 2 smd rect (at -2.8 0 90) (size 1.55 1.7) (layers F.Cu F.Mask)
      (net 7 /V_OUT_CONN))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5951D7D9)
    (at 135.1 103.3 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.1 -1.1 180) (layer F.SilkS))
    (fp_text value 10kΩ (at -0.8 -1.1 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 5 /RUN_PD))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 6 /LDO_VIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5951D7E4)
    (at 135.2 99.9)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -1.2 -1.1) (layer F.SilkS))
    (fp_text value 120kΩ (at 0.9 -1.1) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 8 /LDO_VFB))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module popsu_footprints:S6-TSOT-23 (layer F.Cu) (tedit 593F7973)
    (at 139.6 99.5 90)
    (fp_text reference U1 (at -1.74 0 180) (layer F.SilkS))
    (fp_text value LTC3405 (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at -0.95 -1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 5 /RUN_PD))
    (pad 5 smd rect (at 0 -1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 8 /LDO_VFB))
    (pad 2 smd rect (at 0 1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.95 -1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 6 /LDO_VIN))
    (pad 3 smd rect (at 0.95 1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 9 /LDO_SW))
  )
  (module popsu_footprints:comp-logo-stacked (layer B.Cu) (tedit 0)
    (at 143.4 101.8 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 127 93.5) (end 168.4 93.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.2 104.4) (end 125.2 95.1) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.3 106.2) (end 127 106.2) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170 95.1) (end 170 104.7) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 168.4 104.6) (end 170 104.7) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 168.4 95.1) (end 168.4 93.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127 104.4) (end 127 106.2) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 126.9 95.2) (end 125.2 95.1) (angle 90) (layer Edge.Cuts) (width 0.05))
  (zone (net 6) (net_name /LDO_VIN) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.9 97) (xy 137.9 98) (xy 139 98) (xy 139 98.9) (xy 132.8 98.9)
        (xy 132.8 102.7) (xy 134.7 102.7) (xy 134.7 103.9) (xy 131.7 103.9) (xy 131.8 98.9)
        (xy 129.8 98.9) (xy 129.8 98.2) (xy 131.8 98.2) (xy 131.8 95.8) (xy 136.9 95.8)
      )
    )
  )
  (zone (net 9) (net_name /LDO_SW) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149 99.3) (xy 145.2 99.3) (xy 145.3 102.9) (xy 140 102.9) (xy 140 101.7)
        (xy 143.7 101.7) (xy 143.7 98.9) (xy 140.2 98.9) (xy 140.2 98.1) (xy 140.6 98.1)
        (xy 141.4 97.5) (xy 149 97.5)
      )
    )
  )
  (zone (net 7) (net_name /V_OUT_CONN) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.5 95.8) (xy 142.5 97.2) (xy 149.4 97.2) (xy 149.4 99.8) (xy 146.6 99.8)
        (xy 146.7 103.7) (xy 139.9 103.7) (xy 139.9 104.9) (xy 145 104.9) (xy 155.8 104.9)
        (xy 155.5 95.9)
      )
    )
  )
  (zone (net 8) (net_name /LDO_VFB) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.9 99.8) (xy 137 99.8) (xy 137 101.2) (xy 139.3 101.2) (xy 139.3 104.8)
        (xy 137.4 104.8) (xy 137.4 102.2) (xy 135.6 102.2) (xy 135.6 99.2) (xy 138.9 99.2)
      )
    )
  )
  (zone (net 5) (net_name /RUN_PD) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.9 104.8) (xy 135.5 104.8) (xy 135.5 102.8) (xy 136.9 102.8)
      )
    )
  )
  (zone (net 5) (net_name /RUN_PD) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.3 100.2) (xy 140.3 100.8) (xy 141.6 101.3) (xy 143.1 101.3) (xy 143.1 100.1)
        (xy 140.3 100.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.8 101.7) (xy 133.4 101.7) (xy 133.4 99.3) (xy 134.8 99.3)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.3 93.9) (xy 169.3 105.8) (xy 125.6 105.8) (xy 125.6 93.9)
      )
    )
  )
  (zone (net 5) (net_name /RUN_PD) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.9 100.1) (xy 141.1 100.1) (xy 141.1 101.1) (xy 138.5 103.7) (xy 135.5 103.7)
        (xy 135.5 104.8) (xy 139.1 104.8) (xy 142.6 101.4) (xy 143.1 101.4) (xy 143.1 100.1)
        (xy 146.3 97.8) (xy 155.9 97.8) (xy 156.9 98.4) (xy 161.4 98.4) (xy 161.4 94.3)
        (xy 160.6 94.3) (xy 157.1 94.3) (xy 155.5 96.7) (xy 146.3 96.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142 97) (xy 141.4 97) (xy 140 97.9) (xy 140 99.2) (xy 141.6 99.2)
        (xy 141.6 99.9) (xy 140 99.9) (xy 140 100.9) (xy 137.6 100.9) (xy 137.6 100.1)
        (xy 139.3 100.1) (xy 139.3 97.9) (xy 138 97) (xy 137.4 97) (xy 137.4 95.9)
        (xy 142 95.9)
      )
    )
  )
)
