(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 214)
    (zones 0)
    (modules 11)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.7 2.7)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad7)")
  (net 2 "Net-(J2-Pad7)")
  (net 3 GND)
  (net 4 +5V)
  (net 5 "Net-(J2-Pad2)")
  (net 6 "Net-(J2-Pad3)")
  (net 7 "Net-(J2-Pad4)")
  (net 8 "Net-(J2-Pad5)")
  (net 9 "Net-(U2-Pad9)")
  (net 10 "Net-(J1-Pad1)")
  (net 11 "Net-(U2-Pad5)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 "Net-(J1-Pad3)")
  (net 14 "Net-(J1-Pad9)")
  (net 15 "Net-(J1-Pad2)")
  (net 16 "Net-(J1-Pad6)")
  (net 17 "Net-(U1-Pad2)")
  (net 18 "Net-(U1-Pad4)")
  (net 19 "Net-(U2-Pad8)")
  (net 20 "Net-(U2-Pad6)")
  (net 21 "Net-(U1-Pad10)")
  (net 22 "Net-(U1-Pad6)")
  (net 23 "Net-(U1-Pad12)")
  (net 24 "Net-(J2-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
  )
  (module digikey-footprints:DSUB-9_Jack_5747840-3 (layer F.Cu) (tedit 5B971EEC)
    (at 101.6 87.63 90)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=5747840&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference J1 (at 8.128 -0.127 90) (layer F.SilkS))
    (fp_text value "DB9 (M)" (at 0 4.75 90) (layer F.SilkS))
    (fp_text user %R (at 0 -7.5 90) (layer F.Fab))
    (pad 10 thru_hole circle (at -12.495 0 90) (size 3.5 3.5) (drill 3.17) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 12.495 0 90) (size 3.5 3.5) (drill 3.17) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 5.48 1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (pad 6 thru_hole circle (at 4.11 -1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad6)"))
    (pad 2 thru_hole circle (at 2.74 1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 7 thru_hole circle (at 1.37 -1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad7)"))
    (pad 3 thru_hole circle (at 0 1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad3)"))
    (pad 8 thru_hole circle (at -1.37 -1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at -2.74 1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad 9 thru_hole circle (at -4.11 -1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad9)"))
    (pad 5 thru_hole circle (at -5.48 1.42 90) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 4 +5V))
  )
  (module w_conn_av:minidin-8 (layer F.Cu) (tedit 5B971EF2)
    (at 162.687 87.63 90)
    (descr "MiniDin 8 (S-Video), Tyco P/N 1734096-1")
    (fp_text reference J2 (at 0 8.128 90) (layer F.SilkS))
    (fp_text value "M-DIN-8 (F)" (at 0 -7.366 90) (layer F.SilkS))
    (pad SH thru_hole circle (at -6.75 1.8 90) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask)
      (net 3 GND))
    (pad SH thru_hole circle (at 6.75 1.8 90) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask)
      (net 3 GND))
    (pad 5 thru_hole circle (at -3.4 -1.2 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 2 thru_hole circle (at -1.3 -1.2 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 3.4 -1.2 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at 1.3 -3.8 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 6 thru_hole circle (at 3.4 -3.8 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 24 "Net-(J2-Pad6)"))
    (pad 8 thru_hole circle (at -3.4 -3.8 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 3 GND))
    (pad 7 thru_hole circle (at -0.9 -3.8 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(J2-Pad7)"))
    (pad 1 thru_hole circle (at 1.3 -1.2 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 4 +5V))
    (pad SH thru_hole circle (at 0 2.6 90) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask)
      (net 3 GND))
    (model walter/conn_av/minidin-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 5B93FA32)
    (at 142.24 80.01)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HC74 (at 3.81 8.255 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(U2-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad6)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U2-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad9)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 5B93FA15)
    (at 111.76 78.74)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HC157 (at 3.81 8.89 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad6)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U2-Pad9)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad9)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad5)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 5B93F9E2)
    (at 127 80.01)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HC04 (at 3.81 8.255 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad6)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad6)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad6)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad12)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5B970947)
    (at 108.204 100.33)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0.254 6.096) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5 (at -0.0635 4.572) (layer F.Fab))
    (fp_text user %R (at 0.254 6.096) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 -0.127) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5B97091E)
    (at 108.2675 74.803)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at -0.0635 -4.2545) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at -0.0635 0.3175) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5B97093D)
    (at 164.211 75.1205)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.318) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0 -4.318) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0.0635 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 164.2745 100.203)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0.3175 5.7785) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 4.318) (layer F.Fab))
    (fp_text user %R (at 0.3 5.7785) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 143.1925 100.203)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbol:KiCad-Logo2_6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 131.318 100.0125)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text "rev 1" (at 158.369 101.346) (layer F.SilkS))
  (gr_text github.com/rattboi/gen-to-pce-controller-adapter (at 136.271 74.6125) (layer F.SilkS))
  (gr_line (start 167.5765 103.505) (end 97.79 103.505) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.5765 71.755) (end 97.79 71.755) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.5765 103.505) (end 167.5765 71.755) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 71.755) (end 97.79 103.505) (layer Edge.Cuts) (width 0.15))
  (dimension 17.78 (width 0.3) (layer Dwgs.User)
    (gr_text "0.7000 in" (at 167.2 95.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 165.1 86.36) (xy 165.686421 86.36)))
    (feature2 (pts (xy 165.1 104.14) (xy 165.686421 104.14)))
    (crossbar (pts (xy 165.1 104.14) (xy 165.1 86.36)))
    (arrow1a (pts (xy 165.1 86.36) (xy 165.686421 87.486504)))
    (arrow1b (pts (xy 165.1 86.36) (xy 164.513579 87.486504)))
    (arrow2a (pts (xy 165.1 104.14) (xy 165.686421 103.013496)))
    (arrow2b (pts (xy 165.1 104.14) (xy 164.513579 103.013496)))
  )
  (dimension 8.89 (width 0.3) (layer Dwgs.User)
    (gr_text "0.3500 in" (at 167.2 75.565 90) (layer Dwgs.User))
    (feature1 (pts (xy 163.83 71.12) (xy 165.686421 71.12)))
    (feature2 (pts (xy 163.83 80.01) (xy 165.686421 80.01)))
    (crossbar (pts (xy 165.1 80.01) (xy 165.1 71.12)))
    (arrow1a (pts (xy 165.1 71.12) (xy 165.686421 72.246504)))
    (arrow1b (pts (xy 165.1 71.12) (xy 164.513579 72.246504)))
    (arrow2a (pts (xy 165.1 80.01) (xy 165.686421 78.883496)))
    (arrow2b (pts (xy 165.1 80.01) (xy 164.513579 78.883496)))
  )
  (dimension 11.43 (width 0.3) (layer Dwgs.User)
    (gr_text "0.4500 in" (at 161.73 98.425 270) (layer Dwgs.User))
    (feature1 (pts (xy 163.83 104.14) (xy 163.243579 104.14)))
    (feature2 (pts (xy 163.83 92.71) (xy 163.243579 92.71)))
    (crossbar (pts (xy 163.83 92.71) (xy 163.83 104.14)))
    (arrow1a (pts (xy 163.83 104.14) (xy 163.243579 103.013496)))
    (arrow1b (pts (xy 163.83 104.14) (xy 164.416421 103.013496)))
    (arrow2a (pts (xy 163.83 92.71) (xy 163.243579 93.836504)))
    (arrow2b (pts (xy 163.83 92.71) (xy 164.416421 93.836504)))
  )
  (dimension 11.43 (width 0.3) (layer Dwgs.User)
    (gr_text "0.4500 in" (at 165.93 98.425 90) (layer Dwgs.User))
    (feature1 (pts (xy 163.83 92.71) (xy 164.416421 92.71)))
    (feature2 (pts (xy 163.83 104.14) (xy 164.416421 104.14)))
    (crossbar (pts (xy 163.83 104.14) (xy 163.83 92.71)))
    (arrow1a (pts (xy 163.83 92.71) (xy 164.416421 93.836504)))
    (arrow1b (pts (xy 163.83 92.71) (xy 163.243579 93.836504)))
    (arrow2a (pts (xy 163.83 104.14) (xy 164.416421 103.013496)))
    (arrow2b (pts (xy 163.83 104.14) (xy 163.243579 103.013496)))
  )
  (dimension 33.02 (width 0.3) (layer Dwgs.User)
    (gr_text "33.020 mm" (at 166.81 87.63 270) (layer Dwgs.User))
    (feature1 (pts (xy 168.91 104.14) (xy 168.323579 104.14)))
    (feature2 (pts (xy 168.91 71.12) (xy 168.323579 71.12)))
    (crossbar (pts (xy 168.91 71.12) (xy 168.91 104.14)))
    (arrow1a (pts (xy 168.91 104.14) (xy 168.323579 103.013496)))
    (arrow1b (pts (xy 168.91 104.14) (xy 169.496421 103.013496)))
    (arrow2a (pts (xy 168.91 71.12) (xy 168.323579 72.246504)))
    (arrow2b (pts (xy 168.91 71.12) (xy 169.496421 72.246504)))
  )
  (dimension 74.93 (width 0.3) (layer Dwgs.User)
    (gr_text "74.930 mm" (at 131.445 73.22) (layer Dwgs.User))
    (feature1 (pts (xy 168.91 71.12) (xy 168.91 71.706421)))
    (feature2 (pts (xy 93.98 71.12) (xy 93.98 71.706421)))
    (crossbar (pts (xy 93.98 71.12) (xy 168.91 71.12)))
    (arrow1a (pts (xy 168.91 71.12) (xy 167.783496 71.706421)))
    (arrow1b (pts (xy 168.91 71.12) (xy 167.783496 70.533579)))
    (arrow2a (pts (xy 93.98 71.12) (xy 95.106504 71.706421)))
    (arrow2b (pts (xy 93.98 71.12) (xy 95.106504 70.533579)))
  )
  (dimension 74.93 (width 0.3) (layer Dwgs.User)
    (gr_text "74.930 mm" (at 131.445 73.22) (layer Dwgs.User))
    (feature1 (pts (xy 168.91 71.12) (xy 168.91 71.706421)))
    (feature2 (pts (xy 93.98 71.12) (xy 93.98 71.706421)))
    (crossbar (pts (xy 93.98 71.12) (xy 168.91 71.12)))
    (arrow1a (pts (xy 168.91 71.12) (xy 167.783496 71.706421)))
    (arrow1b (pts (xy 168.91 71.12) (xy 167.783496 70.533579)))
    (arrow2a (pts (xy 93.98 71.12) (xy 95.106504 71.706421)))
    (arrow2b (pts (xy 93.98 71.12) (xy 95.106504 70.533579)))
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.5995 71.5645) (xy 168.148 71.5645) (xy 168.148 103.6955) (xy 97.5995 103.6955)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.5995 71.5645) (xy 168.148 71.5645) (xy 168.148 103.6955) (xy 97.5995 103.6955)
      )
    )
  )
)
