(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 93.98 84.074)
    (grid_origin 93.98 84.074)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "Net-(J3-Pad2)")
  (net 3 "Net-(J3-Pad3)")
  (net 4 "Net-(J3-Pad4)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "GND")
  (net 7 "Net-(Q1-Pad2)")
  (net 8 "Net-(Q1-Pad3)")
  (net 9 "Net-(R4-Pad2)")
  (net 10 "unconnected-(U1-Pad1)")
  (net 11 "unconnected-(U1-Pad2)")
  (net 12 "unconnected-(U1-Pad3)")
  (net 13 "unconnected-(U1-Pad7)")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 123.698 72.644 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 4.043 1.92) (layer "F.SilkS"))
    (fp_text value "39" (at 2.54 -0.254) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 123.7575 75.692 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 5.1395 -0.254 180) (layer "F.SilkS"))
    (fp_text value "39" (at 2.3455 -0.254 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad4)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 110.485 79.248 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.899 1.045) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 127.5675 81.6375 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 9.7555 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Male" (at 0 9.95 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 270) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:TO-92-3" (layer "F.Cu")
    (tedit 5AF9CDD1)
    (at 110.4225 73.1275)
    (descr "http://www.ti.com/lit/ds/symlink/tl431a.pdf")
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=PN2221-2222A.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/PN2222A/PN2222ACS-ND/4806937")
    (property "Description" "TRANS NPN 40V 0.8A TO-92")
    (property "Digi-Key_PN" "PN2222ACS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "PN2222A")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q1" (at -1.7105 -1.7535) (layer "F.SilkS"))
    (fp_text value "PN2222A" (at 1.3375 2.5645) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 -1.25 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 6 "GND") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 1.27 0 180) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval locked (at 2.54 0 180) (size 1 1.5) (drill 0.55) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 123.7575 81.788 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.1395 0 180) (layer "F.SilkS"))
    (fp_text value "39" (at 2.3455 -0.254 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 123.7575 78.74 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 5.1395 0 180) (layer "F.SilkS"))
    (fp_text value "39" (at 2.3455 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad3)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 96.48 73.074)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.83 -1.925) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 96.52 81.924 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 1.25 -1.524 90) (layer "F.SilkS"))
    (fp_text value ".01uf" (at 1.25 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5B86B3A2)
    (at 107.2475 81.6375 180)
    (descr "http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/6N137%20Series.pdf")
    (property "Category" "Integrated Circuits (ICs)")
    (property "DK_Datasheet_Link" "http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en589894")
    (property "DK_Detail_Page" "/product-detail/en/microchip-technology/ATTINY85-20PU/ATTINY85-20PU-ND/735469")
    (property "Description" "IC MCU 8BIT 8KB FLASH 8DIP")
    (property "Digi-Key_PN" "ATTINY85-20PU-ND")
    (property "Family" "Embedded - Microcontrollers")
    (property "MPN" "ATTINY85-20PU")
    (property "Manufacturer" "Microchip Technology")
    (property "Sheetfile" "IRProbeXmtr.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "U1" (at 4.1235 7.7235) (layer "F.SilkS"))
    (fp_text value "ATTINY85" (at 3.94 10.0095) (layer "F.SilkS"))
    (fp_text user "REF**" (at 3.94 3.49) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(U1-Pad1)") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "2" thru_hole circle locked (at 0 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(U1-Pad2)") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "3" thru_hole circle locked (at 0 5.08 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(U1-Pad3)") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "4" thru_hole circle locked (at 0 7.62 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 7.62 7.62 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(R4-Pad2)") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "6" thru_hole circle locked (at 7.62 5.08 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "7" thru_hole circle locked (at 7.62 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(U1-Pad7)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "8" thru_hole circle locked (at 7.62 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbols:OSHW-Logo2_7.3x6mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 119.888 77.216 -90)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF***" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text value "OSHW-Logo2_7.3x6mm_SilkScreen" (at 0.75 0 90) (layer "B.Fab") hide)
  )
  (gr_rect (start 93.98 70.104) (end 129.794 84.074) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Wireless CNC Probe \nIR Xmtr\nDavid Wolfenbarger\nRev -" (at 103.886 77.216 90) (layer "B.SilkS"))
  (gr_text "IR LEDs" (at 125.73 76.962 90) (layer "F.SilkS"))
  (gr_text "GND" (at 96.505 71.299) (layer "F.SilkS"))
  (gr_text "VCC" (at 125.98 81.674 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 96.455 77.299) (layer "F.SilkS"))
  (gr_text "Pwr In: 1S LiPo" (at 94.625 74.955 90) (layer "F.SilkS"))
  (gr_text "NC Probe" (at 111.68 81.424) (layer "F.SilkS"))
  (zone (net 1) (net_name "VCC") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.805 84.099)
        (xy 94.005 84.074)
        (xy 93.955 70.074)
        (xy 129.805 70.049)
      )
    )
  )
  (zone (net 6) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.794 84.074)
        (xy 93.98 84.074)
        (xy 93.98 70.104)
        (xy 129.794 70.104)
      )
    )
  )
)
