(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-rc2-dev-664-g5a90858)")
  (general
    (thickness 1.6)
    (drawings 37)
    (tracks 410)
    (zones 0)
    (modules 23)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.050000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 /AREF)
  (net 4 /RESET)
  (net 5 /RTS)
  (net 6 /X_P)
  (net 7 /X_N)
  (net 8 VCC)
  (net 9 +3V3)
  (net 10 /D3)
  (net 11 /D4)
  (net 12 /D5)
  (net 13 /D6)
  (net 14 /D7)
  (net 15 /D8)
  (net 16 /D9)
  (net 17 /SS)
  (net 18 /MOSI)
  (net 19 /MISO)
  (net 20 /SCK)
  (net 21 /A0)
  (net 22 /A1)
  (net 23 /A2)
  (net 24 /A3)
  (net 25 /A4)
  (net 26 /A5)
  (net 27 /328-RX)
  (net 28 /328-TX)
  (net 29 /D2)
  (net 30 "Net-(D1-Pad2)")
  (net 31 "Net-(U1-Pad4)")
  (net 32 /CTS)
  (net 33 "Net-(IC1-Pad19)")
  (net 34 "Net-(IC1-Pad22)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /328-RX)
    (add_net /328-TX)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /AREF)
    (add_net /CTS)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /RTS)
    (add_net /SCK)
    (add_net /SS)
    (add_net /X_N)
    (add_net /X_P)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(U1-Pad4)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net VCC)
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A7FD51E)
    (at 132.4356 116.1796 45)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9 45) (layer F.SilkS) hide)
    (fp_text value 3v3 (at 0 2.9 45) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 45) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at -1.099999 0 45) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 45) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 4 smd rect (at 1.1 0.95 45) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 45) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 5A7FD438)
    (at 126.317 92.739 30)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 30) (layer F.SilkS) hide)
    (fp_text value CONN_01X16 (at 0 40.43 30) (layer F.Fab))
    (fp_text user %R (at 0 19.05 120) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /A5))
    (pad 3 thru_hole oval (at 0 5.08 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A4))
    (pad 4 thru_hole oval (at 0 7.62 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A3))
    (pad 6 thru_hole oval (at 0 12.7 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A2))
    (pad 7 thru_hole oval (at 0 15.24 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 17.78 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A1))
    (pad 9 thru_hole oval (at 0 20.32 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /A0))
    (pad 10 thru_hole oval (at 0 22.86 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /AREF))
    (pad 11 thru_hole oval (at 0 25.4 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 0 27.94 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SCK))
    (pad 13 thru_hole oval (at 0 30.48 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /MISO))
    (pad 14 thru_hole oval (at 0 33.02 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /MOSI))
    (pad 15 thru_hole oval (at 0 35.56 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SS))
    (pad 16 thru_hole oval (at 0 38.1 30) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 131.707107 111.892893 225)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.439518 0.060811 315) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 225) (layer F.Fab))
    (pad 1 smd rect (at -1 0 225) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 225) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 129.8956 108.3564 135)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.071842 1.508683 135) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.75 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 135) (layer F.Fab))
    (pad 1 smd rect (at -1 0 135) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /AREF))
    (pad 2 smd rect (at 1 0 135) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 124.0536 107.7468 45)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.304734 0.933947 45) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 45) (layer F.Fab))
    (pad 1 smd rect (at -1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (pad 2 smd rect (at 1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /RTS))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 121.5136 114.5032 45)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 2.155261 0 315) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 45) (layer F.Fab))
    (pad 1 smd rect (at -1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /X_P))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 121.412 119.3292 315)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -0.071842 1.652367 315) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 315) (layer F.Fab))
    (pad 1 smd rect (at -1 0 315) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 315) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /X_N))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 130.302 118.364 135)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.44263 0.143684 225) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 135) (layer F.Fab))
    (pad 1 smd rect (at -1 0 135) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 135) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 134.4676 118.2624 45)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 2.188354 1.675843 45) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 45) (layer F.Fab))
    (pad 1 smd rect (at -1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A7FD4E7)
    (at 118.7196 115.8748 315)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0.035921 1.616446 315) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 315) (layer F.Fab))
    (pad 1 smd rect (at -1 0 315) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1 0 315) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 120.0912 113.0808 225)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0.071842 1.508683 225) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 225) (layer F.Fab))
    (pad 1 smd rect (at -1 0 225) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1 0 225) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 134.9756 113.9952 135)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L1 (at -2.530877 -0.304339 225) (layer F.SilkS))
    (fp_text value 10uH (at 0 1.75 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 135) (layer F.Fab))
    (pad 1 smd rect (at -1 0 135) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 135) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm (layer F.Cu) (tedit 5A7FD453)
    (at 125.061 94.939 330)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 330) (layer F.SilkS) hide)
    (fp_text value CONN_01X14 (at 0 37.89 330) (layer F.Fab))
    (fp_text user %R (at 0 17.78 60) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RESET))
    (pad 5 thru_hole oval (at 0 10.16 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RTS))
    (pad 7 thru_hole oval (at 0 15.24 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /328-TX))
    (pad 8 thru_hole oval (at 0 17.78 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /328-RX))
    (pad 9 thru_hole oval (at 0 20.32 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 10 thru_hole oval (at 0 22.86 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /CTS))
    (pad 11 thru_hole oval (at 0 25.4 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 0 27.94 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 0 30.48 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 14 thru_hole oval (at 0 33.02 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 15 thru_hole oval (at 0 35.56 330) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer F.Cu) (tedit 5A7FD44D)
    (at 109.776 125.735 90)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X14 (at 0 35.35 90) (layer F.Fab))
    (fp_text user %R (at 0 16.51 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /D3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D5))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D6))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /D7))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /D8))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /D9))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 5A7FD43D)
    (at 115.005 121.127)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference P4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 5A7FD43F)
    (at 137.578 121.127)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference P5 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 5A7FD441)
    (at 126.317 101.621)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference P6 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 122.682 106.3752 45)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.658156 -0.502894 45) (layer F.SilkS))
    (fp_text value 100K (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 45) (layer F.Fab))
    (pad 1 smd rect (at -1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:FA238-4pin_3.2x2.5mm_Offset" (layer F.Cu) (tedit 5A775CF5)
    (at 123.7996 116.8908 225)
    (descr "crystal Epson Toyocom FA-238 series http://www.mouser.com/ds/2/137/1721499-465440.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at -3.125129 -1.688288 225) (layer F.SilkS))
    (fp_text value 16M (at 0 2.45 225) (layer F.Fab))
    (fp_text user %R (at -0.043 -2.4256 225) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.8 225) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /X_P))
    (pad 2 smd rect (at 1.1 0.8 225) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.1 -0.8 225) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /X_N))
    (pad 4 smd rect (at -1.1 -0.8 225) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_SeikoEpson_FA238-4pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:SW_SPST_PTS830" (layer F.Cu) (tedit 5A774781)
    (at 127.4572 121.0056 135)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.6 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 2.6 135) (layer F.Fab))
    (fp_text user %R (at -1.05 -2.22 135) (layer F.Fab))
    (pad 1 smd rect (at -1.6 -0.825 135) (size 0.7 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.6 -0.825 135) (size 0.7 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.6 0.825 135) (size 0.7 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (pad 2 smd rect (at 1.6 0.825 135) (size 0.7 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5A867E31)
    (at 131.85 122.15098 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 1.69902 -4) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A890E8A)
    (at 134 122.05 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R2 (at 1.75 -1.75) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:QFN-32-1EP_5x5mm_Pitch0.5mm-GND" (layer F.Cu) (tedit 5A7FA315)
    (at 126.3 111.4 45)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference IC1 (at 0 -3.75 45) (layer F.SilkS))
    (fp_text value ATMEGA328-A (at 0 3.75 45) (layer F.Fab))
    (pad 1 smd rect (at -2.4 -1.75 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /D3))
    (pad 2 smd rect (at -2.4 -1.25 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /D4))
    (pad 3 smd rect (at -2.4 -0.75 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.4 -0.25 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 5 smd rect (at -2.4 0.25 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.4 0.75 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 7 smd rect (at -2.4 1.25 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /X_P))
    (pad 8 smd rect (at -2.4 1.75 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /X_N))
    (pad 9 smd rect (at -1.75 2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /D5))
    (pad 10 smd rect (at -1.25 2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /D6))
    (pad 11 smd rect (at -0.75 2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /D7))
    (pad 12 smd rect (at -0.25 2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /D8))
    (pad 13 smd rect (at 0.25 2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /D9))
    (pad 14 smd rect (at 0.75 2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /SS))
    (pad 15 smd rect (at 1.25 2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /MOSI))
    (pad 16 smd rect (at 1.75 2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /MISO))
    (pad 17 smd rect (at 2.4 1.75 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /SCK))
    (pad 18 smd rect (at 2.4 1.25 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 19 smd rect (at 2.4 0.75 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 2.4 0.25 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /AREF))
    (pad 21 smd rect (at 2.4 -0.25 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 2.4 -0.75 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 2.4 -1.25 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /A0))
    (pad 24 smd rect (at 2.4 -1.75 45) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /A1))
    (pad 25 smd rect (at 1.75 -2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /A2))
    (pad 26 smd rect (at 1.25 -2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /A3))
    (pad 27 smd rect (at 0.75 -2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /A4))
    (pad 28 smd rect (at 0.25 -2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /A5))
    (pad 29 smd rect (at -0.25 -2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (pad 30 smd rect (at -0.75 -2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /328-RX))
    (pad 31 smd rect (at -1.25 -2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /328-TX))
    (pad 32 smd rect (at -1.75 -2.4 135) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /D2))
    (pad 5 smd rect (at 0.8625 0.8625 45) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 5 smd rect (at 0.8625 -0.8625 45) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 5 smd rect (at -0.8625 0.8625 45) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 5 smd rect (at -0.8625 -0.8625 45) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Pyramiduino (at 121.2596 123.3424) (layer B.SilkS))
  (gr_text R5 (at 118.7196 122.2756) (layer B.SilkS))
  (gr_text R5 (at 118.7196 122.2756) (layer F.SilkS))
  (gr_text Pyramiduino (at 121.2596 123.3424) (layer F.SilkS))
  (gr_text NC (at 111.3536 113.3856 240) (layer F.SilkS))
  (gr_text www.addohms.com (at 126.0856 109.7788) (layer B.SilkS))
  (gr_text MI (at 143.764 117.7036 120) (layer F.SilkS))
  (gr_text SCK (at 142.6972 115.6716 120) (layer F.SilkS))
  (gr_text A3 (at 133.604 100.1268 120) (layer F.SilkS))
  (gr_text RESET (at 118.9736 100.33 240) (layer F.SilkS))
  (gr_text RTS (at 116.332 104.648 240) (layer F.SilkS))
  (gr_text TX (at 115.1128 106.8324 240) (layer F.SilkS))
  (gr_text RX (at 113.8428 109.0168 240) (layer F.SilkS))
  (gr_text 5V (at 112.6236 111.3028 240) (layer F.SilkS))
  (gr_text 5V (at 107.5944 119.9896 240) (layer F.SilkS))
  (gr_text 5V (at 106.3244 122.1232 240) (layer F.SilkS))
  (gr_text D2 (at 112.2172 128.27) (layer F.SilkS))
  (gr_text D3 (at 114.808 128.3716) (layer F.SilkS))
  (gr_text D4 (at 119.8372 128.27) (layer F.SilkS))
  (gr_text D5 (at 122.3772 128.27) (layer F.SilkS))
  (gr_text D6 (at 124.968 128.27) (layer F.SilkS))
  (gr_text D7 (at 127.508 128.27) (layer F.SilkS))
  (gr_text D8 (at 132.7404 128.27) (layer F.SilkS))
  (gr_text D9 (at 135.2296 128.3208) (layer F.SilkS))
  (gr_text 3V3 (at 140.3604 128.0668) (layer F.SilkS))
  (gr_text 3V3 (at 142.8496 128.0668) (layer F.SilkS))
  (gr_text AREF (at 140.0556 111.252 120) (layer F.SilkS))
  (gr_text SS (at 146.4056 122.2756 120) (layer F.SilkS))
  (gr_text MO (at 145.034 119.888 120) (layer F.SilkS))
  (gr_text A0 (at 138.5824 108.7628 120) (layer F.SilkS))
  (gr_text A1 (at 137.2108 106.4768 120) (layer F.SilkS))
  (gr_text A2 (at 134.874 102.362 120) (layer F.SilkS))
  (gr_text A4 (at 131.064 95.8596 120) (layer F.SilkS))
  (gr_text A5 (at 129.7432 93.5228 120) (layer F.SilkS))
  (gr_line (start 126.316 84.419) (end 100 130) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.633 130) (end 126.316 84.419) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 130) (end 152.633 130) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.16)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.9744 129.9464) (xy 126.3904 84.582) (xy 152.6032 129.8956) (xy 100.0252 130.048)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.16)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.0252 130.048) (xy 126.3396 84.4804) (xy 152.654 130.048) (xy 99.9744 130.048)
      )
    )
  )
)
