<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="7.622896875" y1="8.252709375" x2="24.566578125" y2="8.259759375" width="0" layer="20"/>
<wire x1="24.566578125" y1="8.259759375" x2="24.566578125" y2="5.292725" width="0" layer="20"/>
<wire x1="24.566578125" y1="5.292725" x2="29.859303125" y2="0" width="0" layer="20" curve="90"/>
<wire x1="29.859303125" y1="0" x2="100.945" y2="0" width="0" layer="20"/>
<wire x1="100.945" y1="0" x2="100.945" y2="25.705" width="0" layer="20"/>
<wire x1="100.945" y1="25.705" x2="30.795521875" y2="25.7048125" width="0" layer="20"/>
<wire x1="30.795521875" y1="25.7048125" x2="24.6634" y2="19.572675" width="0" layer="20" curve="92.468018"/>
<wire x1="24.6634" y1="19.572675" x2="24.6634" y2="17.7294" width="0" layer="20"/>
<wire x1="24.6634" y1="17.7294" x2="7.62" y2="17.7294" width="0" layer="20"/>
<wire x1="7.62" y1="17.7294" x2="7.622896875" y2="8.252709375" width="0" layer="20"/>
<text>RaedKit</text>
<text>2013©</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="transistor-pnp">
<description>&lt;b&gt;PNP Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun" package="AXIAL-0.4" value="100"/>
<element name="R2" library="SparkFun" package="AXIAL-0.4" value="2.2k"/>
<element name="R3" library="SparkFun" package="AXIAL-0.4" value="10k"/>
<element name="Q1" library="transistor-pnp" package="TO92" value="2N3906"/>
<element name="Q2" library="transistor-npn" package="TO92" value="2N3904"/>
<element name="LED1" library="SparkFun" package="LED5MM" value=""/>
<element name="JP1" library="pinhead" package="1X01" value=""/>
<element name="JP2" library="SparkFun" package="SCREWTERMINAL-5MM-2" value=""/>
<element name="R4" library="SparkFun" package="AXIAL-0.4" value="8.2k"/>
<element name="R5" library="SparkFun" package="AXIAL-0.4" value="2.2k"/>
<element name="R6" library="SparkFun" package="AXIAL-0.4" value="100"/>
<element name="LED2" library="SparkFun" package="LED5MM" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="P$2"/>
<contactref element="JP2" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="P$2"/>
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="P$1"/>
<contactref element="JP2" pad="1"/>
<contactref element="LED2" pad="K"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="P$1"/>
<contactref element="JP1" pad="1"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="P$1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="K"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="P$2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="Q1" pad="1"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="P$1"/>
<contactref element="LED2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
