(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6256)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.0152))
      (layer "F.Cu" (type "copper") (thickness 0.0356))
      (layer "dielectric 1" (type "core") (thickness 1.524) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.0356))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.0152))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/2.5V_B_0")
  (net 2 "/InB_0")
  (net 3 "/2.5V_A_0")
  (net 4 "/InA_0")
  (net 5 "/2.5V_B_1")
  (net 6 "/InB_1")
  (net 7 "/2.5V_A_1")
  (net 8 "/InA_1")
  (net 9 "/2.5V_B_3")
  (net 10 "/InB_3")
  (net 11 "/2.5V_A_3")
  (net 12 "/InA_3")
  (net 13 "/2.5V_B_2")
  (net 14 "/InB_2")
  (net 15 "/2.5V_A_2")
  (net 16 "/InA_2")
  (net 17 "/2.5V_B_5")
  (net 18 "/InB_5")
  (net 19 "/2.5V_A_5")
  (net 20 "/InA_5")
  (net 21 "/2.5V_B_4")
  (net 22 "/InB_4")
  (net 23 "/2.5V_A_4")
  (net 24 "/InA_4")
  (net 25 "/2.5V_B_7")
  (net 26 "/InB_7")
  (net 27 "/2.5V_A_7")
  (net 28 "/InA_7")
  (net 29 "/2.5V_B_6")
  (net 30 "/InB_6")
  (net 31 "/2.5V_A_6")
  (net 32 "/InA_6")
  (net 33 "GND")
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 39.505)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H29" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 29 "/2.5V_B_6") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 39.505)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H30" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 30 "/InB_6") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:CON40_2X20_DUK_FTSH_SAI" (layer "F.Cu")
    (at 100 80 -90)
    (tags "FTSH-120-01-L-DV-K ")
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "FTSH-120-01-L-DV-K")
    (attr smd)
    (fp_text reference "J1" (at 0.17 0.02 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "FTSH-120-01-L-DV-K" (at -0.04 -5.06 -90 unlocked) (layer "F.Fab"))
    (fp_text user "40" (at -16.2968 -1.9556 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at 13.4466 2.0576 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "39" (at -16.2968 2.1084 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "2" (at 13.472 -2.0318 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at 13.208 2.032 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.01 7.77 -90 unlocked) (layer "F.Fab"))
    (fp_text user "2" (at 13.208 -2.032 -90 unlocked) (layer "F.Fab"))
    (fp_text user "39" (at -13.208 2.032 -90 unlocked) (layer "F.Fab"))
    (fp_text user "40" (at -13.208 -2.032 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 12.065 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/2.5V_B_0") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at 12.065 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/InB_0") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at 10.795 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/2.5V_A_0") (pinfunction "3") (pintype "unspecified"))
    (pad "4" smd rect (at 10.795 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/InA_0") (pinfunction "4") (pintype "unspecified"))
    (pad "5" smd rect (at 9.525 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/2.5V_B_1") (pinfunction "5") (pintype "unspecified"))
    (pad "6" smd rect (at 9.525 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/InB_1") (pinfunction "6") (pintype "unspecified"))
    (pad "7" smd rect (at 8.255 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/2.5V_A_1") (pinfunction "7") (pintype "unspecified"))
    (pad "8" smd rect (at 8.255 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/InA_1") (pinfunction "8") (pintype "unspecified"))
    (pad "9" smd rect (at 6.985 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/2.5V_B_3") (pinfunction "9") (pintype "unspecified"))
    (pad "10" smd rect (at 6.985 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/InB_3") (pinfunction "10") (pintype "unspecified"))
    (pad "11" smd rect (at 5.715 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/2.5V_A_3") (pinfunction "11") (pintype "unspecified"))
    (pad "12" smd rect (at 5.715 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/InA_3") (pinfunction "12") (pintype "unspecified"))
    (pad "13" smd rect (at 4.445 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/2.5V_B_2") (pinfunction "13") (pintype "unspecified"))
    (pad "14" smd rect (at 4.445 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/InB_2") (pinfunction "14") (pintype "unspecified"))
    (pad "15" smd rect (at 3.175 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/2.5V_A_2") (pinfunction "15") (pintype "unspecified"))
    (pad "16" smd rect (at 3.175 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/InA_2") (pinfunction "16") (pintype "unspecified"))
    (pad "17" smd rect (at 1.905 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/2.5V_B_5") (pinfunction "17") (pintype "unspecified"))
    (pad "18" smd rect (at 1.905 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/InB_5") (pinfunction "18") (pintype "unspecified"))
    (pad "19" smd rect (at 0.635 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/2.5V_A_5") (pinfunction "19") (pintype "unspecified"))
    (pad "20" smd rect (at 0.635 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/InA_5") (pinfunction "20") (pintype "unspecified"))
    (pad "21" smd rect (at -0.635 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/2.5V_B_4") (pinfunction "21") (pintype "unspecified"))
    (pad "22" smd rect (at -0.635 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/InB_4") (pinfunction "22") (pintype "unspecified"))
    (pad "23" smd rect (at -1.905 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/2.5V_A_4") (pinfunction "23") (pintype "unspecified"))
    (pad "24" smd rect (at -1.905 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/InA_4") (pinfunction "24") (pintype "unspecified"))
    (pad "25" smd rect (at -3.175 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/2.5V_B_7") (pinfunction "25") (pintype "unspecified"))
    (pad "26" smd rect (at -3.175 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/InB_7") (pinfunction "26") (pintype "unspecified"))
    (pad "27" smd rect (at -4.445 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/2.5V_A_7") (pinfunction "27") (pintype "unspecified"))
    (pad "28" smd rect (at -4.445 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/InA_7") (pinfunction "28") (pintype "unspecified"))
    (pad "29" smd rect (at -5.715 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/2.5V_B_6") (pinfunction "29") (pintype "unspecified"))
    (pad "30" smd rect (at -5.715 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/InB_6") (pinfunction "30") (pintype "unspecified"))
    (pad "31" smd rect (at -6.985 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/2.5V_A_6") (pinfunction "31") (pintype "unspecified"))
    (pad "32" smd rect (at -6.985 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/InA_6") (pinfunction "32") (pintype "unspecified"))
    (pad "33" smd rect (at -8.255 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "GND") (pinfunction "33") (pintype "unspecified"))
    (pad "34" smd rect (at -8.255 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "GND") (pinfunction "34") (pintype "unspecified"))
    (pad "35" smd rect (at -9.525 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "GND") (pinfunction "35") (pintype "unspecified"))
    (pad "36" smd rect (at -9.525 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "GND") (pinfunction "36") (pintype "unspecified"))
    (pad "37" smd rect (at -10.795 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "GND") (pinfunction "37") (pintype "unspecified"))
    (pad "38" smd rect (at -10.795 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "GND") (pinfunction "38") (pintype "unspecified"))
    (pad "39" smd rect (at -12.065 2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "GND") (pinfunction "39") (pintype "unspecified"))
    (pad "40" smd rect (at -12.065 -2.032 270) (size 0.762 2.794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "GND") (pinfunction "40") (pintype "unspecified"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 120.495)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H3" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 3 "/2.5V_A_0") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 70.655)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H19" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 19 "/2.5V_A_5") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 108.035)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H8" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 8 "/InA_1") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 126.725)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H2" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 2 "/InB_0") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 114.265)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H6" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 6 "/InB_1") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 58.195)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H23" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 23 "/2.5V_A_4") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 51.965)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H25" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 25 "/2.5V_B_7") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 83.115)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H15" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 15 "/2.5V_A_2") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 64.425)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H21" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 21 "/2.5V_B_4") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 89.345)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H13" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 13 "/2.5V_B_2") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 76.885)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H18" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 18 "/InB_5") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 45.735)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H28" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 28 "/InA_7") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 101.805)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H9" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 9 "/2.5V_B_3") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 95.575)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H11" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 11 "/2.5V_A_3") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 120.495)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H4" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 4 "/InA_0") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 70.655)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H20" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 20 "/InA_5") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 101.805)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H10" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 10 "/InB_3") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 51.965)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H26" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 26 "/InB_7") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 83.115)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H16" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 16 "/InA_2") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 33.275)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H31" (at -5.396 0.0498 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 31 "/2.5V_A_6") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 45.735)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H27" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 27 "/2.5V_A_7") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 114.265)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H5" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 5 "/2.5V_B_1") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 95.575)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H12" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 12 "/InA_3") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 89.345)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H14" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 14 "/InB_2") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 108.035)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H7" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 7 "/2.5V_A_1") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 64.425)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H22" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 22 "/InB_4") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 58.195)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H24" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 24 "/InA_4") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 148.35 33.275)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H32" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 32 "/InA_6") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 76.885)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H17" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 17 "/2.5V_B_5") (pinfunction "1") (pintype "input"))
  )
  (footprint "DownloadedParts:MillMax_OmniBall" (layer "F.Cu")
    (at 51.65 126.725)
    (property "Sheetfile" "Tile resistance jig contact board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H1" (at -3.73 -0.01 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0.01 2.77 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.19) (layers "*.Cu" "*.Mask")
      (net 1 "/2.5V_B_0") (pinfunction "1") (pintype "input"))
  )
  (gr_rect (start 48.4498 30) (end 151.3708 130)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "SLAC tile contact board v2\n" (at 89.1286 126.7714) (layer "F.SilkS"))
  (zone (net 33) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 94.6658 63.627)
        (xy 105.1814 63.627)
        (xy 105.3338 72.136)
        (xy 94.8182 72.136)
      )
    )
  )
  (zone (net 33) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 48.5522 30.1778)
        (xy 151.3716 30)
        (xy 151.3716 130)
        (xy 48.5522 130.1778)
      )
    )
  )
)
