<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0.13" y1="0.06" x2="160.24" y2="0.07" width="0" layer="20"/>
<wire x1="160.24" y1="0.07" x2="160.24" y2="63.59" width="0" layer="20"/>
<wire x1="160.24" y1="63.59" x2="133.82" y2="63.59" width="0" layer="20"/>
<wire x1="133.82" y1="63.59" x2="133.82" y2="70.72" width="0" layer="20"/>
<wire x1="133.82" y1="70.72" x2="132.82" y2="71.72" width="0" layer="20"/>
<wire x1="132.82" y1="71.72" x2="108.71" y2="71.72" width="0" layer="20"/>
<wire x1="108.71" y1="71.72" x2="107.71" y2="70.72" width="0" layer="20"/>
<wire x1="107.71" y1="70.72" x2="107.71" y2="63.59" width="0" layer="20"/>
<wire x1="107.71" y1="63.59" x2="104.53" y2="63.59" width="0" layer="20"/>
<wire x1="104.53" y1="63.59" x2="104.53" y2="70.72" width="0" layer="20"/>
<wire x1="104.53" y1="70.72" x2="103.53" y2="71.72" width="0" layer="20"/>
<wire x1="20.02" y1="71.72" x2="19.02" y2="70.72" width="0" layer="20"/>
<wire x1="19.02" y1="70.72" x2="19.02" y2="63.59" width="0" layer="20"/>
<wire x1="19.02" y1="63.59" x2="18.98" y2="63.59" width="0" layer="20"/>
<wire x1="18.98" y1="63.59" x2="-0.034" y2="63.584" width="0" layer="20"/>
<wire x1="-0.034" y1="63.584" x2="-0.02" y2="0.06" width="0" layer="20"/>
<hole x="4.03" y="2.63" drill="3.2"/>
<hole x="156.64" y="3.01" drill="3.2"/>
<hole x="5.3" y="58.51" drill="3.2"/>
<text>benic76</text>
<hole x="156.43" y="58.51" drill="3.2"/>
<text>mono</text>
<text>stereo</text>
<text>jamma4pc</text>
<text>version1.0      </text>
<text>22/10/2013</text>
<wire x1="103.53" y1="71.72" x2="20.02" y2="71.72" width="0" layer="20"/>
<text>volume</text>
<text>in audio</text>
<text>usb</text>
<text>protezione 15khz</text>
<text>on</text>
<text>off</text>
<text>video in rgb</text>
</plain>
<libraries>
<library name="atmel">
<packages>
<package name="TQFP44">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="con-amp">
<packages>
<package name="10X06MTA">
<description>&lt;b&gt;AMP MTA connector&lt;/b&gt;&lt;p&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_640456_W.pdf</description>
</package>
</packages>
</library>
<library name="v-reg">
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO214AC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="con-cypressindustries">
<packages>
<package name="32005-201">
<description>&lt;b&gt;MINI USB-B R/A SMT W/ REAR&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-201.pdf</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA03-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lumberg">
<description>&lt;b&gt;Lumberg Connectors&lt;/b&gt;&lt;p&gt;
include con-mfs.lbr - 2001.03.22&lt;br&gt;
Jack connectors - 2005.11.23&lt;p&gt;
http://www.lumberg.de&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="KLBR4">
<description>&lt;b&gt;Jack connectors according to JISC 6560, 3.5 mm&lt;/b&gt;&lt;p&gt;
Klinkensteckverbinder nach JISC 6560, 3,5 mm&lt;br&gt;
Source: &lt;a href="http://www.lumberg.com/Produkte/PDFs/KLBR4.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="alps_japan_potentiometers">
<description>ALPS Potentiometers, Series RK097, RK27
Single and Dual Elements, Rotary and Push Lock Switch
ALPS Japan

By Omar Masri
Audiosquare.com
http://stores.ebay.com/Audio-Grade?_rdc=1</description>
<packages>
<package name="RK097-DUAL-ELEMENT">
<description>ALPS RK097 Dual Element D-Shaft</description>
</package>
</packages>
</library>
<library name="Panasonic-EEE-EEV-EEF-ECQ">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cad_tools/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="CAPAE1350X1400N">
</package>
</packages>
</library>
<library name="con-subd">
<description>&lt;b&gt;SUB-D Connectors&lt;/b&gt;&lt;p&gt;
Harting&lt;br&gt;
NorComp&lt;br&gt;
&lt;p&gt;
PREFIX :&lt;br&gt;
H = High density&lt;br&gt;
F = Female&lt;br&gt;
M = Male&lt;p&gt;
NUMBER: Number of pins&lt;p&gt;
SUFFIX :&lt;br&gt;
H = Horizontal&lt;br&gt;
V = Vertical &lt;br&gt;
P = Shield pin on housing&lt;br&gt;
B = No mounting holes&lt;br&gt;
S = Pins individually placeable (Single)&lt;br&gt;
D = Direct mounting &lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HDF15H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="LM4952">
<packages>
<package name="TO97P1435X475-10N">
</package>
</packages>
</library>
<library name="JAMMA NUOVO">
<packages>
<package name="JAMMA">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="TQFP44" value="ATMEGA32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="M1206" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="crystal" package="HC49UP" value="12.MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-amp" package="10X06MTA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="v-reg" package="SOT223" value="LD117AS33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="resistor" package="PANASONIC_C" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="resistor" package="PANASONIC_C" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO214AC" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="M1206" value="68">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="M1206" value="68">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor" package="M1206" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="resistor" package="M1206" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-cypressindustries" package="32005-201" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-lstb" package="MA03-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="linear" package="SO14" value="LMV324M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="resistor" package="M1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="resistor" package="M1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="resistor" package="M1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="resistor" package="PANASONIC_D" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="resistor" package="M1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="resistor" package="PANASONIC_C" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="resistor" package="PANASONIC_C" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="resistor" package="M1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="resistor" package="M1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="jumper" package="JP2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-lumberg" package="KLBR4" value="KLBR4">
<attribute name="OC_NEWARK" value="97K2709"/>
<attribute name="MPN" value="KLBR 4"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1217016"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="alps_japan_potentiometers" package="RK097-DUAL-ELEMENT" value="RK097-DUAL-ELEMENT"/>
<element name="C10" library="Panasonic-EEE-EEV-EEF-ECQ" package="CAPAE1350X1400N" value="470UF">
<attribute name="OC_NEWARK" value="53W3911 "/>
<attribute name="TOLERANCE" value="±20 %"/>
<attribute name="MPN" value="EEVFK1V471Q"/>
<attribute name="SUPPLIER" value="PANASONIC"/>
<attribute name="VOLTAGERATING" value="35V"/>
<attribute name="OC_FARNELL" value="2282105 "/>
<attribute name="VALUE" value="470UF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="Panasonic-EEE-EEV-EEF-ECQ" package="CAPAE1350X1400N" value="470UF">
<attribute name="OC_NEWARK" value="53W3911 "/>
<attribute name="TOLERANCE" value="±20 %"/>
<attribute name="MPN" value="EEVFK1V471Q"/>
<attribute name="SUPPLIER" value="PANASONIC"/>
<attribute name="VOLTAGERATING" value="35V"/>
<attribute name="OC_FARNELL" value="2282105 "/>
<attribute name="VALUE" value="470UF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="con-subd" package="HDF15H" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="40xx" package="SO14" value="4066D">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IC5" library="74xx-eu" package="SO14" value="74HC86D">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C17" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="resistor" package="PANASONIC_D" value="22uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="resistor" package="PANASONIC_D" value="22uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="resistor" package="M1206" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="resistor" package="M1206" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="resistor" package="M1206" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jumper" package="JP2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="74xx-eu" package="SO16" value="74LS123D">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="transistor-npn" package="SOT23-BEC" value="BCX20">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2/2" library="rcl" package="C0805" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1/1" library="rcl" package="C0805" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2/2" library="resistor" package="M1206" value="18">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1/1" library="resistor" package="M1206" value="12k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3/3" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="con-amp" package="10X06MTA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="LM4952" package="TO97P1435X475-10N" value="LM4952TS">
<attribute name="PACKAGE" value="TO-263-9"/>
<attribute name="OC_NEWARK" value="41K5994"/>
<attribute name="MPN" value="LM4952TS"/>
<attribute name="SUPPLIER" value="National Semiconductors"/>
<attribute name="OC_FARNELL" value="1008028"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="Panasonic-EEE-EEV-EEF-ECQ" package="CAPAE1350X1400N" value="470UF">
<attribute name="OC_NEWARK" value="53W3911 "/>
<attribute name="TOLERANCE" value="±20 %"/>
<attribute name="MPN" value="EEVFK1V471Q"/>
<attribute name="SUPPLIER" value="PANASONIC"/>
<attribute name="VOLTAGERATING" value="35V"/>
<attribute name="OC_FARNELL" value="2282105 "/>
<attribute name="VALUE" value="470UF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="Panasonic-EEE-EEV-EEF-ECQ" package="CAPAE1350X1400N" value="470UF">
<attribute name="OC_NEWARK" value="53W3911 "/>
<attribute name="TOLERANCE" value="±20 %"/>
<attribute name="MPN" value="EEVFK1V471Q"/>
<attribute name="SUPPLIER" value="PANASONIC"/>
<attribute name="VOLTAGERATING" value="35V"/>
<attribute name="OC_FARNELL" value="2282105 "/>
<attribute name="VALUE" value="470UF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="resistor" package="PANASONIC_D" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="resistor" package="PANASONIC_C" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="resistor" package="M1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0805" value="390nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0805" value="390nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="resistor" package="PANASONIC_D" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$1" library="JAMMA NUOVO" package="JAMMA" value=""/>
</elements>
<signals>
<signal name="AGND">
<contactref element="IC1" pad="28"/>
</signal>
<signal name="GND1">
<contactref element="IC1" pad="18"/>
</signal>
<signal name="GND2">
<contactref element="IC1" pad="39"/>
</signal>
<signal name="VCC1">
<contactref element="IC1" pad="17"/>
</signal>
<signal name="VCC2">
<contactref element="IC1" pad="38"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="7"/>
<contactref element="Q1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="27"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="4"/>
<contactref element="C5" pad="+"/>
<contactref element="D1" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="R4" pad="2"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="-"/>
<contactref element="LED1" pad="C"/>
<contactref element="IC2" pad="1"/>
<contactref element="C4" pad="-"/>
<contactref element="R5" pad="2"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="5"/>
<contactref element="J1" pad="5"/>
<contactref element="IC1" pad="6"/>
<contactref element="SV1" pad="6"/>
<contactref element="IC3" pad="11"/>
<contactref element="C7" pad="2"/>
<contactref element="IC3" pad="10"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="-"/>
<contactref element="R8" pad="1"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC5" pad="7"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="-"/>
<contactref element="C19" pad="-"/>
<contactref element="X4" pad="10"/>
<contactref element="X4" pad="5"/>
<contactref element="X4" pad="6"/>
<contactref element="X4" pad="7"/>
<contactref element="X4" pad="8"/>
<contactref element="IC4" pad="7"/>
<contactref element="C20" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="IC6" pad="9"/>
<contactref element="IC6" pad="8"/>
<contactref element="C3/3" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="J3" pad="6"/>
<contactref element="C24" pad="-"/>
<contactref element="C25" pad="-"/>
<contactref element="U1" pad="10"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="C26" pad="-"/>
<contactref element="U1" pad="5"/>
<contactref element="X2" pad="S"/>
</signal>
<signal name="#RES">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="AREF">
<contactref element="IC1" pad="29"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="3"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="2"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="1"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="44"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="43"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="42"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="40"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="26"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="25"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="24"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="21"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="20"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="37"/>
</signal>
<signal name="N$42">
<contactref element="IC1" pad="36"/>
</signal>
<signal name="N$43">
<contactref element="IC1" pad="35"/>
</signal>
<signal name="N$44">
<contactref element="IC1" pad="34"/>
</signal>
<signal name="N$45">
<contactref element="IC1" pad="33"/>
</signal>
<signal name="N$46">
<contactref element="IC1" pad="32"/>
</signal>
<signal name="N$47">
<contactref element="IC1" pad="31"/>
</signal>
<signal name="N$48">
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$49">
<contactref element="IC1" pad="16"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="N$50">
<contactref element="IC1" pad="15"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$51">
<contactref element="IC1" pad="14"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$53">
<contactref element="IC1" pad="12"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="IC1" pad="10"/>
</signal>
<signal name="S$8">
<contactref element="C26" pad="+"/>
<contactref element="X1" pad="1"/>
<contactref element="C4" pad="+"/>
<contactref element="IC2" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="+5V">
<contactref element="C10" pad="1"/>
<contactref element="IC5" pad="14"/>
<contactref element="C17" pad="1"/>
<contactref element="IC5" pad="13"/>
<contactref element="JP2" pad="3"/>
<contactref element="IC4" pad="14"/>
<contactref element="C20" pad="2"/>
<contactref element="IC6" pad="11"/>
<contactref element="IC6" pad="16"/>
<contactref element="C3/3" pad="1"/>
<contactref element="IC6" pad="2"/>
<contactref element="IC6" pad="3"/>
<contactref element="Q2" pad="C"/>
<contactref element="R2/2" pad="2"/>
<contactref element="R1/1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$22">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="USB_P">
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="USB_N">
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$35">
</signal>
<signal name="N$39">
</signal>
<signal name="S$1">
</signal>
<signal name="N$38">
</signal>
<signal name="S$4">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="N$25">
</signal>
<signal name="N$37">
</signal>
<signal name="N$12">
<contactref element="IC1" pad="41"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="IC3" pad="9"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="+12V">
<contactref element="C7" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="R9" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="C24" pad="+"/>
<contactref element="R14" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="IC3" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="S$9">
<contactref element="C13" pad="+"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R6" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="IC3" pad="6"/>
<contactref element="R7" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R7" pad="2"/>
<contactref element="IC3" pad="7"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="IC3" pad="14"/>
<contactref element="C8" pad="2"/>
<contactref element="IC3" pad="13"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="N$31">
<contactref element="IC3" pad="12"/>
<contactref element="C9" pad="+"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="C14" pad="+"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R11" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="X2" pad="T"/>
<contactref element="C14" pad="-"/>
</signal>
<signal name="N$55">
<contactref element="X2" pad="R"/>
<contactref element="C13" pad="-"/>
</signal>
<signal name="N$63">
<contactref element="IC5" pad="11"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$64">
<contactref element="C18" pad="+"/>
<contactref element="IC5" pad="1"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="C19" pad="+"/>
<contactref element="IC5" pad="4"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="X4" pad="14"/>
<contactref element="R16" pad="2"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC6" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="X4" pad="13"/>
<contactref element="R17" pad="2"/>
<contactref element="IC5" pad="5"/>
</signal>
<signal name="N$68">
<contactref element="IC5" pad="6"/>
<contactref element="IC5" pad="9"/>
</signal>
<signal name="N$69">
<contactref element="IC5" pad="10"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="N$70">
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="12"/>
</signal>
<signal name="N$71">
<contactref element="IC4" pad="12"/>
<contactref element="IC4" pad="13"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC4" pad="6"/>
<contactref element="JP2" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$73">
<contactref element="X4" pad="3"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$74">
<contactref element="X4" pad="2"/>
<contactref element="IC4" pad="10"/>
</signal>
<signal name="N$75">
<contactref element="X4" pad="1"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="N$62">
</signal>
<signal name="N$78">
<contactref element="C23" pad="2"/>
</signal>
<signal name="N$79">
<contactref element="C22" pad="2"/>
</signal>
<signal name="N$80">
<contactref element="IC4" pad="9"/>
</signal>
<signal name="N$81">
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$99">
<contactref element="IC4" pad="11"/>
</signal>
<signal name="N$100">
<contactref element="IC4" pad="1"/>
</signal>
<signal name="N$76">
<contactref element="C1/1" pad="1"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="N$77">
<contactref element="C2/2" pad="1"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="N$82">
<contactref element="IC6" pad="15"/>
<contactref element="C1/1" pad="2"/>
<contactref element="R1/1" pad="1"/>
</signal>
<signal name="N$84">
<contactref element="IC6" pad="7"/>
<contactref element="C2/2" pad="2"/>
<contactref element="R2/2" pad="1"/>
</signal>
<signal name="N$86">
<contactref element="Q2" pad="E"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$88">
<contactref element="IC6" pad="5"/>
<contactref element="Q2" pad="B"/>
</signal>
<signal name="N$90">
<contactref element="IC6" pad="13"/>
<contactref element="IC6" pad="10"/>
</signal>
<signal name="N$72">
<contactref element="LED2" pad="C"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$87">
<contactref element="J3" pad="2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$52">
</signal>
<signal name="N$83">
<contactref element="U1" pad="4"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="N$85">
<contactref element="U1" pad="7"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="N$93">
<contactref element="C25" pad="+"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$59">
<contactref element="U1" pad="1"/>
<contactref element="U$1" pad="P$5"/>
</signal>
<signal name="N$56">
<contactref element="C16" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="C15" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$23">
</signal>
<signal name="S$2">
</signal>
<signal name="N$89">
</signal>
<signal name="S$3">
</signal>
<signal name="N$91">
</signal>
<signal name="N$92">
</signal>
<signal name="N$94">
</signal>
<signal name="N$95">
</signal>
<signal name="S$5">
<contactref element="R14" pad="1"/>
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="S$6">
</signal>
<signal name="S$7">
</signal>
</signals>
</board>
</drawing>
</eagle>
