(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 84)
    (tracks 279)
    (zones 0)
    (modules 25)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.1 2.1)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module segac2:Generic_0.96in-128x64-OLED-Display-IIC (layer F.Cu) (tedit 607C47E3)
    (at 67.6656 63.5)
    (descr http://www.ebay.com/itm/0-96-I2C-IIC-SPI-Serial-128X64-White-OLED-LCD-LED-Display-Module-for-Arduino-BU/361916106520)
    (fp_text reference "OLED PANEL (128x64)" (at -0.1524 1.524) (layer F.SilkS))
    (fp_text value Display_OLED_LCD_IIC (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 10.35 11.6) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -10.35 11.6) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -10.35 -11.6) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.81 -11.95) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 1.27 -11.95) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1.27 -11.95) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -3.81 -11.95) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.35 -11.6) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x04_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A422)
    (at 63.7032 44.6024 90)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (fp_text reference "To Multi Dip Switch" (at -1.27 3.2512 90) (layer B.SilkS))
    (fp_text value PinSocket_2x04_P2.54mm_Vertical (at -1.27 -10.39 90) (layer B.Fab))
    (fp_text user %R (at -1.27 -3.81 180) (layer B.Fab))
    (pad 8 thru_hole oval (at -2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 123.6345 64.3255 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference 0.1uf (at 2.6035 1.905) (layer F.SilkS))
    (fp_text value C_Disc_D4.3mm_W1.9mm_P5.00mm (at 2.5 2.2) (layer F.Fab))
    (fp_text user C6 (at 2.5 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 121.2215 25.273 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference 0.1uf (at 2.413 1.905 90) (layer F.SilkS))
    (fp_text value C_Disc_D4.3mm_W1.9mm_P5.00mm (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user C1 (at 2.5 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 91.7575 49.403 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference 0.1uf (at 2.413 1.905) (layer F.SilkS))
    (fp_text value C_Disc_D4.3mm_W1.9mm_P5.00mm (at 2.5 2.2) (layer F.Fab))
    (fp_text user C3 (at 2.413 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 94.1705 33.909 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference 0.1uf (at 2.413 2.159) (layer F.SilkS))
    (fp_text value C_Disc_D4.3mm_W1.9mm_P5.00mm (at 2.5 2.2) (layer F.Fab))
    (fp_text user C2 (at 2.5 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 110.617 46.99 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 1K (at 5.2705 -2.286 90) (layer F.SilkS))
    (fp_text value R2 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 113.0935 49.911 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 2K (at 5.0165 -2.54 90) (layer F.SilkS))
    (fp_text value R3 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sega16:arrow (layer F.Cu) (tedit 0)
    (at 51.6636 37.7444 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module sega16:arrow (layer F.Cu) (tedit 0)
    (at 51.689 54.9148 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 110.0455 56.7055 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference 22pf (at 2.159 -2.0955) (layer F.SilkS))
    (fp_text value C_Disc_D4.3mm_W1.9mm_P5.00mm (at 2.5 2.2) (layer F.Fab))
    (fp_text user C5 (at 2.5 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 110.0455 52.832 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference 22pf (at 2.413 2.159) (layer F.SilkS))
    (fp_text value C_Disc_D4.3mm_W1.9mm_P5.00mm (at 2.5 2.2) (layer F.Fab))
    (fp_text user C4 (at 2.5 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 73.914 45.6565 90)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference "ATMEGA 328P" (at 3.8735 -2.9845 270) (layer F.SilkS))
    (fp_text value DIP-28_W7.62mm_Socket (at 3.81 35.35 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 16.51 90) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 127.0635 48.641)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference "To RPi GPIO" (at 5.7785 3.3655 180) (layer B.SilkS))
    (fp_text value PinHeader_2x06_P2.54mm_Horizontal (at 5.655 -14.97) (layer B.Fab))
    (fp_text user %R (at 5.31 -6.35 -90) (layer B.Fab))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 112.522 67.945)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference RESET (at 3.3655 7.874) (layer F.SilkS))
    (fp_text value SW_PUSH_6mm (at 3.75 6.7) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5A1AD3B8)
    (at 116.9035 44.704 90)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference "XTAL (16 MHZ)" (at 2.4765 -3.7465 90) (layer F.SilkS))
    (fp_text value Crystal_HC49-U_Vertical (at 2.44 3.525 90) (layer F.Fab))
    (fp_text user X1 (at 2.44 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 4.88 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:USB_A_Female_UE27AC54100 (layer B.Cu) (tedit 5D25FE01)
    (at 129.413 65.4685 270)
    (fp_text reference "RPi USB POWER" (at 10.16 -3.429 180) (layer B.SilkS))
    (fp_text value USB_A_Female_UE27AC54100 (at 0 -12 270) (layer B.Fab) hide)
    (fp_text user %R (at -0.025 -0.975 270) (layer B.Fab) hide)
    (pad 4 thru_hole circle (at 3.5 2.71 270) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 1 2.71 270) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 2.71 270) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.5 2.71 270) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at 6.57 0 270) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at -6.57 0 270) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 129.6035 26.3525)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference "To Sega16B pcb" (at 4.3815 3.3655) (layer B.SilkS))
    (fp_text value PinHeader_1x03_P2.54mm_Horizontal (at 4.385 -7.35 180) (layer B.Fab) hide)
    (fp_text user %R (at 2.77 -2.54 90) (layer B.Fab) hide)
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 106.1085 75.184 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 220Ω (at 4.953 2.54 90) (layer F.SilkS))
    (fp_text value R4 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 84.1248 70.5104)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SELECT (at 12.1412 2.1844) (layer F.SilkS))
    (fp_text value SW_PUSH_6mm (at 3.75 6.7) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 84.1248 61.6712)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference DOWN (at 11.2776 2.2352) (layer F.SilkS))
    (fp_text value SW_PUSH_6mm (at 3.75 6.7) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 84.1248 52.8828)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference UP (at 10.0076 2.3876) (layer F.SilkS))
    (fp_text value SW_PUSH_6mm (at 3.75 6.7) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sega16:Rpi (layer F.Cu) (tedit 0)
    (at 55.6895 22.479)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module sega16:sega16 (layer F.Cu) (tedit 0)
    (at 76.8985 22.606)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 73.9775 33.147)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 10K (at 5.207 -2.4765) (layer F.SilkS))
    (fp_text value R1 (at 5.334 -0.0635) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "(3.3V)" (at 66.5988 55.118) (layer F.SilkS))
  (gr_text SDA (at 71.7296 53.8988) (layer F.SilkS))
  (gr_text SCL (at 69.1896 53.8988) (layer F.SilkS))
  (gr_text VCC (at 66.5988 53.8988) (layer F.SilkS))
  (gr_text "(GPIO 3)" (at 133.096 49.276) (layer F.SilkS))
  (gr_text "(GPIO 3)" (at 133.096 46.6725) (layer F.SilkS))
  (gr_text "(GPIO 15)" (at 123.698 49.403) (layer B.SilkS))
  (gr_text "(GPIO 14)" (at 123.698 46.9265) (layer B.SilkS))
  (gr_text "(GPIO 15)" (at 123.698 49.403) (layer F.SilkS))
  (gr_text "(GPIO 14)" (at 123.698 46.9265) (layer F.SilkS))
  (gr_text "(GPIO 17)" (at 133.0325 41.656) (layer F.SilkS))
  (gr_text "(GPIO 27)" (at 133.0325 39.1795) (layer F.SilkS))
  (gr_text "(GPIO 22)" (at 133.0325 36.449) (layer F.SilkS))
  (gr_text "(GPIO 12)" (at 123.698 44.45) (layer B.SilkS))
  (gr_text "(GPIO 23)" (at 123.698 41.8465) (layer B.SilkS))
  (gr_text "(GPIO 24)" (at 123.6345 36.6395) (layer F.SilkS))
  (gr_text "(GPIO 24)" (at 123.6345 36.6395) (layer B.SilkS))
  (gr_text "(GPIO 12)" (at 123.698 44.45) (layer F.SilkS))
  (gr_text "(GPIO 23)" (at 123.698 41.8465) (layer F.SilkS))
  (gr_text "(GPIO 18)" (at 123.6345 39.3065) (layer F.SilkS))
  (gr_text "(GPIO 18)" (at 123.6345 39.3065) (layer B.SilkS))
  (gr_text SDA (at 135.4455 49.784) (layer B.SilkS))
  (gr_text 15 (at 134.9375 35.8775) (layer B.SilkS))
  (gr_text 11 (at 134.9375 40.9575) (layer B.SilkS))
  (gr_text 13 (at 134.9375 38.4175) (layer B.SilkS))
  (gr_text SCL (at 135.4455 46.0375) (layer B.SilkS))
  (gr_text 3.3v (at 135.4455 43.4975) (layer B.SilkS))
  (gr_text "10 (RxD)" (at 123.6345 48.3235) (layer B.SilkS))
  (gr_text 12 (at 123.6345 38.354) (layer B.SilkS))
  (gr_text 32 (at 123.6345 43.3705) (layer B.SilkS))
  (gr_text "8 (TxD)" (at 123.6345 45.847) (layer B.SilkS))
  (gr_text 18 (at 123.571 35.6235) (layer B.SilkS))
  (gr_text 16 (at 123.698 40.8305) (layer B.SilkS))
  (gr_text 5v (at 126.1745 21.844) (layer B.SilkS))
  (gr_text VCC (at 126.111 20.6375) (layer B.SilkS))
  (gr_text GND (at 126.3015 24.003) (layer B.SilkS))
  (gr_text RESET (at 125.7935 26.6065) (layer B.SilkS))
  (gr_text "RPi USB POWER" (at 132.715 65.278 90) (layer F.SilkS))
  (gr_text "Faces Edge Connector" (at 51.816 46.2788 90) (layer F.SilkS))
  (gr_text 5v (at 126.1745 21.844) (layer F.SilkS))
  (gr_text "3 (SDA)" (at 132.969 48.0695) (layer F.SilkS))
  (gr_text 13 (at 132.842 38.1635) (layer F.SilkS))
  (gr_text 3.3v (at 132.7785 43.4975) (layer F.SilkS))
  (gr_text "5 (SCL)" (at 132.969 45.5295) (layer F.SilkS))
  (gr_text 15 (at 132.842 35.3695) (layer F.SilkS))
  (gr_text 11 (at 132.7785 40.64) (layer F.SilkS))
  (gr_text "10 (RxD)" (at 123.6345 48.3235) (layer F.SilkS))
  (gr_text "8 (TxD)" (at 123.6345 45.847) (layer F.SilkS))
  (gr_text 32 (at 123.6345 43.3705) (layer F.SilkS))
  (gr_text 16 (at 123.698 40.8305) (layer F.SilkS))
  (gr_text 12 (at 123.6345 38.354) (layer F.SilkS))
  (gr_text 18 (at 123.571 35.6235) (layer F.SilkS))
  (gr_text RESET (at 125.7935 26.6065) (layer F.SilkS))
  (gr_text GND (at 126.3015 24.003) (layer F.SilkS))
  (gr_text VCC (at 126.111 20.6375) (layer F.SilkS))
  (gr_text GND (at 129.4765 68.961) (layer F.SilkS))
  (gr_text 5v (at 129.6035 62.6745) (layer F.SilkS))
  (gr_text VCC (at 129.4765 61.4045) (layer F.SilkS))
  (gr_text 5v (at 124.1425 62.6745) (layer B.SilkS))
  (gr_text VCC (at 124.0155 61.4045) (layer B.SilkS))
  (gr_text GND (at 124.1425 68.961) (layer B.SilkS))
  (gr_text GND (at 63.8556 53.8988) (layer F.SilkS))
  (gr_text "To Sega16B pcb" (at 132.715 23.876 90) (layer F.SilkS))
  (gr_text "To Multi Dip Switch" (at 67.056 46.0248 90) (layer F.SilkS))
  (gr_text 4 (at 56.0832 41.7068) (layer F.SilkS))
  (gr_text 3 (at 58.5724 41.656) (layer F.SilkS))
  (gr_text 2 (at 61.1632 41.7068) (layer F.SilkS))
  (gr_text 1 (at 63.6524 41.656) (layer F.SilkS))
  (gr_arc (start 138.43 75.311) (end 138.43 77.851) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 52.07 75.311) (end 49.53 75.311) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 52.07 19.05) (end 52.07 16.51) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 138.43 19.05) (end 140.97 19.05) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "BladeZX  rev1.0" (at 131.191 75.819) (layer F.SilkS))
  (gr_text "SEGA C2-Pi\nMulti Selector" (at 96.3295 20.828) (layer F.SilkS))
  (gr_line (start 49.53 75.311) (end 49.53 19.05) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 138.43 77.851) (end 52.07 77.851) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.97 19.05) (end 140.97 75.311) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 52.07 16.51) (end 138.43 16.51) (layer Edge.Cuts) (width 0.05))
)
